|  | E |
SECTION E — FIXED CONSTRUCTIONS

BUILDING

|  | E05 |
LOCKS; KEYS; WINDOW AND DOOR FITTINGS; SAFES

|  | E05 |
Note(s) In this class, the following terms are used with the meanings stated: "Wing" is a general term for doors or openable windows, and other movable members to which similar fastening devices may be applied, e.g. drawers, lids of chests, car boots, car bonnets. A wing may swing, slide, or move in any other manner. "Frame" means any member to which a wing may be held by a fastening device. It does not include a framework forming part of the wing, but it may be another wing. "Lock" means primarily a device for releasing or securing any member, which requires a key or a permutation mechanism for release. "Bolt" means a sliding, pivoted, or otherwise movable member such as is normally carried by a door to hold it shut by engagement with a keeper on the frame. It may be operated by hand directly or through mechanism or by a key; it may be a latch (see (5) below.) "Latch" means a bolt arranged to be moved to the releasing position against the force of a spring, or some other returning force, when a wing meets the frame on closing, so that it does not have to be operated by hand to secure the wing, but only to open it. "Hasp" means a member hinged to the frame or wing so that it can be moved towards the face of the wing or frame and secured thereto, e.g. by a turn-button, by a padlock and staple.

|  | E05D |
HINGES AND OTHER SUSPENSION DEVICES FOR DOORS, WINDOWS, OR WINGS (pivotal connections in general Fulltext... Hierarchy... Expanded...F16C 11/00)

|  | E05D 1/00 |
Pinless hinges; Substitutes for hinges

|  | E05D 1/02 |
· | made of one piece

|  | E05D 1/04 |
· | with guide members shaped as circular arcs

|  | E05D 1/06 |
· | consisting of two easily-separable parts

|  | E05D 3/00 |
Hinges with pins

|  | E05D 3/02 |
· | with one pin

|  | E05D 3/04 |
· · | engaging three or more parts, e.g. sleeves, movable relatively to one another for connecting two or more wings to another member

|  | E05D 3/06 |
· | with two or more pins

|  | E05D 3/08 |
· · | for swing-doors, i.e. openable by pushing from either side

|  | E05D 3/10 |
· · | with non-parallel pins

|  | E05D 5/00 |
Construction of single parts, e.g. the parts for attachment

|  | E05D 5/02 |
· | Parts for attachment, e.g. flaps

|  | E05D 5/04 |
· · | Flat flaps

|  | E05D 5/06 |
· · | Bent flaps

|  | E05D 5/08 |
· · | of cylindrical shape

|  | E05D 5/10 |
· | Pins and/or sockets or sleeves; Removable pins

|  | E05D 5/12 |
· · | Securing pins in sockets, movably or not

|  | E05D 5/14 |
· · | Construction of sockets or sleeves

|  | E05D 5/16 |
· · · | to be secured without special attachment parts on the socket or sleeve

|  | E05D 7/00 |
Hinges or pivots of special construction (used for special suspension arrangements Fulltext... Hierarchy... Expanded...E05D 15/00; so as to be self-closing Fulltext... Hierarchy... Expanded...E05F 1/06, Fulltext... Hierarchy... Expanded...E05F 1/12; with means for raising wings before being turned Fulltext... Hierarchy... Expanded...E05F 7/02)

|  | E05D 7/02 |
· | for use on the right-hand as well as the left-hand side; Convertible right-hand or left-hand hinges

|  | E05D 7/04 |
· | Hinges adjustable relative to the wing or the frame

|  | E05D 7/06 |
· | to allow tilting of the members

|  | E05D 7/08 |
· | for use in suspensions comprising two spigots placed at opposite edges of the wing, especially at the top and the bottom, e.g. trunnions

|  | E05D 7/10 |
· | to allow easy separation of the parts at the hinge axis (substitutes for hinges Fulltext... Hierarchy... Expanded...E05D 1/06)

|  | E05D 7/12 |
· | to allow easy detachment of the hinge from the wing or the frame

|  | E05D 7/14 |
· | Hinges for safes

|  | E05D 9/00 |
Flaps or sleeves specially designed for making from particular material, e.g. hoop-iron, sheet metal, plastics

|  | E05D 11/00 |
Additional features or accessories of hinges

|  | E05D 11/02 |
· | Lubricating arrangements

|  | E05D 11/04 |
· | relating to the use of free balls as bearing-surfaces (Fulltext... Hierarchy... Expanded...E05D 7/06 takes precedence)

|  | E05D 11/06 |
· | Devices for limiting the opening movement of hinges

|  | E05D 11/08 |
· | Friction devices between relatively-movable hinge parts

|  | E05D 11/10 |
· | Devices for preventing movement between relatively-movable hinge parts

|  | E05D 13/00 |
Accessories for sliding wings (for lifting wings Fulltext... Hierarchy... Expanded...E05D 17/00)

|  | E05D 13/02 |
· | Suspension devices, e.g. sliding or rolling guides

|  | E05D 13/04 |
· | Fasteners specially adapted for holding sliding wings open (for holding wings closed Fulltext... Hierarchy... Expanded...E05C)

|  | E05D 13/06 |
· · | with notches

|  | E05D 13/08 |
· · | acting by friction

|  | E05D 13/10 |
· | Counterbalance devices for sliding wings

|  | E05D 13/12 |
· · | with springs

|  | E05D 13/14 |
· · | with weights

|  | E05D 15/00 |
Suspension arrangements for wings (arrangements of wings not characterised by the construction of the supporting means Fulltext... Hierarchy... Expanded...E06B 3/32)

|  | E05D 15/02 |
· | for revolving wings

|  | E05D 15/04 |
· | with arms fixed on the wing pivoting about an axis outside of the wing

|  | E05D 15/06 |
· | for wings sliding horizontally more or less in their own plane

|  | E05D 15/08 |
· · | consisting of two or more independent parts movable each in its own guides

|  | E05D 15/10 |
· · | movable out of one plane into a second parallel plane

|  | E05D 15/12 |
· · | consisting of parts connected at their edges

|  | E05D 15/14 |
· · | with movable arms situated in the plane of the wing

|  | E05D 15/16 |
· | for wings sliding vertically more or less in their own plane

|  | E05D 15/18 |
· · | consisting of two or more independent parts, movable each in its own guides

|  | E05D 15/20 |
· · | movable out of one plane into a second parallel plane

|  | E05D 15/22 |
· · | allowing an additional movement

|  | E05D 15/24 |
· · | consisting of parts connected at their edges

|  | E05D 15/26 |
· | for folding wings

|  | E05D 15/28 |
· | supported on arms movable in horizontal plane

|  | E05D 15/30 |
· · | with pivoted arms and sliding guides

|  | E05D 15/32 |
· · | with two pairs of pivoted arms

|  | E05D 15/34 |
· · · | with wings opening parallel to themselves

|  | E05D 15/36 |
· | moving along slide-ways so arranged that one guide, member of the wing moves in a direction substantially perpendicular to the movement of another guide member

|  | E05D 15/38 |
· · | for upwardly-moving wings, e.g. up-and-over doors

|  | E05D 15/40 |
· | supported on arms movable in vertical planes

|  | E05D 15/42 |
· · | with pivoted arms and horizontally-sliding guides

|  | E05D 15/44 |
· · | with pivoted arms and vertically-sliding guides

|  | E05D 15/46 |
· · | with two pairs of pivoted arms

|  | E05D 15/48 |
· | allowing alternative movements (for vertically-sliding wings Fulltext... Hierarchy... Expanded...E05D 15/22)

|  | E05D 15/50 |
· · | for opening at either of two opposite edges

|  | E05D 15/52 |
· · | for opening about a vertical as well as a horizontal axis

|  | E05D 15/54 |
· · | for opening both inwards and outwards

|  | E05D 15/56 |
· | with successive different movements

|  | E05D 15/58 |
· · | with both swinging and sliding movements

|  | E05D 17/00 |
Construction of single parts specially adapted for suspending lifting wings, e.g. pulleys, counter-weights; Safety catches