|  | E |
SECTION E — FIXED CONSTRUCTIONS

BUILDING

|  | E05 |
LOCKS; KEYS; WINDOW OR DOOR FITTINGS; SAFES

|  | E05 |
Note(s) In this class, the following terms are used with the meanings stated: "Wing" is a general term for doors, openable windows, and other movable members to which similar fastening devices may be applied, e.g. drawers, lids of chests, car boots, car bonnets. A wing may swing, slide, or move in any other manner. "Frame" means any member to which a wing may be held by a fastening device. It does not include a framework forming part of the wing, but it may be another wing. "Lock" means primarily a device for releasing or securing any member, which requires a key or a permutation mechanism for release. "Bolt" means a sliding, pivoted, or otherwise movable member such as is normally carried by a door to hold it shut by engagement with a keeper on the frame. It may be operated by hand directly or through mechanism or by a key; it may be a latch (see (5) below) "Latch" means a bolt arranged to be moved to the releasing position against the force of a spring, or some other returning force, when a wing meets the frame on closing, so that it does not have to be operated by hand to secure the wing, but only to open it. "Hasp" means a member hinged to the frame or wing so that it can be moved towards the face of the wing or frame and secured thereto, e.g. by a turn-button, by a padlock and staple.

|  | E05C |
BOLTS OR FASTENING DEVICES FOR WINGS, SPECIALLY FOR DOORS OR WINDOWS (fastening devices specially adapted for bags, trunks, etc. Fulltext... Hierarchy... Expanded...A45C 13/00, specially adapted for containers Fulltext... Hierarchy... Expanded...B65D; fastening devices for constructional or engineering elements Fulltext... Hierarchy... Expanded...E04, Fulltext... Hierarchy... Expanded...F16B; locks, devices structurally or operatively combined with locks Fulltext... Hierarchy... Expanded...E05B; handles or casings not restricted to particular types of fastening devices Fulltext... Hierarchy... Expanded...E05B; keepers or other parts for engagement by bolts or fastening devices Fulltext... Hierarchy... Expanded...E05B 15/00; non-mechanical control or operation of fastening devices Fulltext... Hierarchy... Expanded...E05B 47/00, Fulltext... Hierarchy... Expanded...E05B 51/00; vehicle door locking arrangements Fulltext... Hierarchy... Expanded...E05B 65/12; for holding sliding wings open Fulltext... Hierarchy... Expanded...E05D 13/04; means for operating or controlling wing fasteners in conjunction with mechanism for moving the wing Fulltext... Hierarchy... Expanded...E05F)

|  | E05C |
Note(s) Attention is drawn to the definitions following the class title of class Fulltext... Hierarchy... Expanded...E05. In this sub-class, only the movement essential for securing the wing is considered, e.g. a sliding bolt which is rotated on its axis to prevent its withdrawal is classified as having only a sliding movement.

|  | E05C 1/00 - E05C 5/00 |
Bolts, latches, or equivalent wing-fastening devices, characterised by special way of movement, e.g. moving rectilinearly, pivotally, or rotatively (devices released automatically by pull or pressure on the wing Fulltext... Hierarchy... Expanded...E05C 19/02; hasps Fulltext... Hierarchy... Expanded...E05C 19/08; hook fastenings Fulltext... Hierarchy... Expanded...E05C 19/10)

|  | E05C 1/00 |
Fastening devices with bolts moving rectilinearly

|  | E05C 1/02 |
· | without latching action

|  | E05C 1/04 |
· · | with operating handle or equivalent member rigid with the bolt

|  | E05C 1/06 |
· · | with operating handle or equivalent member moving otherwise than rigidly with the bolt

|  | E05C 1/08 |
· | with latching action

|  | E05C 1/10 |
· · | with operating handle or equivalent member rigid with the latch

|  | E05C 1/12 |
· · | with operating handle or equivalent member moving otherwise than rigidly with the latch

|  | E05C 1/14 |
· · · | the handle or member moving essentially towards, or away from, the plane of the wing or frame

|  | E05C 1/16 |
· · · | the handle or member moving essentially in a plane substantially parallel to the wing

|  | E05C 3/00 |
Fastening devices with bolts moving pivotally or rotatively

|  | E05C 3/02 |
· | without latching action

|  | E05C 3/04 |
· · | with operating handle or equivalent member rigid with the bolt

|  | E05C 3/06 |
· · | with operating handle or equivalent member moving otherwise than rigidly with the bolt

|  | E05C 3/08 |
· · · | the handle or member moving essentially towards, or away from, the plane of the wing or frame

|  | E05C 3/10 |
· · · | the handle or member moving essentially in a plane substantially parallel to the wing

|  | E05C 3/12 |
· | with latching action (devices in which the securing part is formed or merely carried by a spring and moves only by distortion of the spring, e.g. snaps, Fulltext... Hierarchy... Expanded...E05C 19/06)

|  | E05C 3/14 |
· · | with operating handle or equivalent member rigid with the latch

|  | E05C 3/16 |
· · | with operating handle or equivalent member moving otherwise than rigidly with the latch

|  | E05C 3/22 |
· · · | the bolt being spring-controlled

|  | E05C 3/24 |
· · · · | in the form of a bifurcated member

|  | E05C 3/26 |
· · · · · | engaging a stud-like keeper

|  | E05C 3/28 |
· · · · · · | with simultaneously-operating double bolts

|  | E05C 3/30 |
· · · · | in the form of a hook

|  | E05C 3/32 |
· · · · · | engaging a hooked keeper (Fulltext... Hierarchy... Expanded...E05C 3/34 takes precedence)

|  | E05C 3/34 |
· · · · · | with simultaneously-operating double bolts

|  | E05C 3/36 |
· · · · | in the form of a rotary gear

|  | E05C 3/38 |
· · · · | with bolts engaging a hooked keeper (Fulltext... Hierarchy... Expanded...E05C 3/24, Fulltext... Hierarchy... Expanded...E05C 3/30, Fulltext... Hierarchy... Expanded...E05C 3/36 take precedence)

|  | E05C 3/40 |
· · · · | with bolts engaging a stud-like keeper (Fulltext... Hierarchy... Expanded...E05C 3/24, Fulltext... Hierarchy... Expanded...E05C 3/30, Fulltext... Hierarchy... Expanded...E05C 3/36 take precedence)

|  | E05C 5/00 |
Fastening devices with bolts moving otherwise than only rectilinearly and only pivotally or rotatively

|  | E05C 5/02 |
· | both moving axially and turning about their axes to secure the wing

|  | E05C 5/04 |
· · | performing both movements simultaneously, e.g. screwing into a keeper

|  | E05C 7/00 |
Fastening devices specially adapted for two wings

|  | E05C 7/00 |
Note(s) If a fastening device merely secures one wing to another wing which is already closed it is not regarded as specially adapted for two wings.

|  | E05C 7/02 |
· | for wings which lie one behind the other when closed

|  | E05C 7/04 |
· | for wings which abut when closed

|  | E05C 7/06 |
· · | a fastening device for one wing being actuated or controlled by closing another wing

|  | E05C 9/00 |
Arrangements of simultaneously-actuated bolts or other securing devices at well-separated positions on the same wing (essentially involving locking means Fulltext... Hierarchy... Expanded...E05B 63/14; similar constructions for engineering closures Fulltext... Hierarchy... Expanded...F16J 13/08)

|  | E05C 9/02 |
· | with one sliding bar for fastening when moved in one direction and unfastening when moved in opposite direction

|  | E05C 9/04 |
· | with two sliding bars moved in opposite directions when fastening or unfastening

|  | E05C 9/06 |
· | with three or more sliding bars

|  | E05C 9/08 |
· | with a rotary bar for actuating the fastening means

|  | E05C 9/10 |
· | Actuating mechanisms for bars

|  | E05C 9/12 |
· · | with gears and racks

|  | E05C 9/14 |
· · | with pins engaging slots

|  | E05C 9/16 |
· · | with crank pins and connecting rods

|  | E05C 9/18 |
· | Details of fastening means or of fixed retaining means for the ends of bars

|  | E05C 11/00 |
Fastenings in which the members which engage one another, mounted respectively on the wing and the frame, are both movable, e.g. for release by moving either of them (hasp fastenings Fulltext... Hierarchy... Expanded...E05C 19/08)

|  | E05C 13/00 |
Additional equipment, adjuncts, or details of wing fastenings; Fastenings characterised thereby (locks, accessories in connection with locks or lock handles Fulltext... Hierarchy... Expanded...E05B; buffers per se Fulltext... Hierarchy... Expanded...E05F 5/00; means per se for preventing rattling of wings Fulltext... Hierarchy... Expanded...E05F 7/04; means per se for taking the weight of the wing Fulltext... Hierarchy... Expanded...E05F 7/06)

|  | E05C 13/02 |
· | Means for securing the bolt in the fastening position or the released position; Arrangements for preventing unauthorised opening, e.g. by sealing (seals Fulltext... Hierarchy... Expanded...G09F 3/00)

|  | E05C 13/04 |
· | Means for controlling or operating wing-fastening members by mechanical remote control (Fulltext... Hierarchy... Expanded...E05C 9/00 takes precedence; means for operating or controlling wing fasteners in conjunction with mechanism for moving the wing Fulltext... Hierarchy... Expanded...E05F)

|  | E05C 13/06 |
· · | for one wing

|  | E05C 13/08 |
· · | for two or more wings

|  | E05C 13/10 |
· | Means for operating or controlling devices other than fastenings, e.g. switches, indicators

|  | E05C 15/00 |
Wing-fastening devices for special use

|  | E05C 15/02 |
· | for ready releasing in case of emergency or panic

|  | E05C 15/04 |
· | for a plurality of drawers; for securing one or more drawers by closing another one (controlled by a key Fulltext... Hierarchy... Expanded...E05B 65/46)

|  | E05C 17/00 |
Devices specially designed for holding wings in one or more opened positions or for limiting opening or preventing closing (combined with hinges Fulltext... Hierarchy... Expanded...E05D 11/00; holding sliding wings Fulltext... Hierarchy... Expanded...E05D 13/04; combined with operating apparatus for wings Fulltext... Hierarchy... Expanded...E05F; devices affecting the motion of the wing during a substantial part of its movement Fulltext... Hierarchy... Expanded...E05F 5/00; stops, buffers, with or without holding means, Fulltext... Hierarchy... Expanded...E05F 5/00)

|  | E05C 17/02 |
· | by mechanical means

|  | E05C 17/04 |
· · | with a movable bar or equivalent member extending between frame and wing

|  | E05C 17/06 |
· · · | releasable to allow further opening only when the wing is nearly closed

|  | E05C 17/08 |
· · · | with special means for release, e.g. automatic release by further opening

|  | E05C 17/10 |
· · · | incorporating a special device for securing the wing in the closed position

|  | E05C 17/12 |
· · · | consisting of a single rod

|  | E05C 17/14 |
· · · · | Hook and eye, or equivalent

|  | E05C 17/16 |
· · · · | pivoted only at one end and having an elongated slot

|  | E05C 17/18 |
· · · · | pivoted only at one end and having a row of holes, notches, or pins

|  | E05C 17/20 |
· · · · | sliding through a guide (Fulltext... Hierarchy... Expanded...E05C 17/18 takes precedence)

|  | E05C 17/22 |
· · · · · | and clamping or securing means in the guide

|  | E05C 17/24 |
· · · · | pivoted at one end, and with the other end running along a guide member

|  | E05C 17/26 |
· · · · · | and clamping or securing means at the pivot of the rod

|  | E05C 17/28 |
· · · · · | with clamping or securing means at the connection to the guide member

|  | E05C 17/30 |
· · · | of extensible, e.g. telescopic, construction (flexible members Fulltext... Hierarchy... Expanded...E05C 17/36)

|  | E05C 17/32 |
· · · | consisting of two or more pivoted rods

|  | E05C 17/34 |
· · · · | with means for holding in more than one position

|  | E05C 17/36 |
· · · | comprising a flexible member, e.g. chains

|  | E05C 17/38 |
· · | with a curved rail rigid with the frame for engagement with means on the wing, or vice versa

|  | E05C 17/40 |
· · | Bars or like parts connecting a right wing with a left wing which move against each other when being closed

|  | E05C 17/42 |
· · | connecting exterior and interior wings

|  | E05C 17/44 |
· · | with a device carried on the wing for frictional or like engagement with a fixed flat surface, e.g. retractable feet

|  | E05C 17/46 |
· · | in which the wing or a member fixed thereon is engaged by a movable fastening member in a fixed position; in which a movable fastening member mounted on the wing engages a stationary member (specially adapted for sliding wings Fulltext... Hierarchy... Expanded...E05D 13/04)

|  | E05C 17/48 |
· · · | comprising a sliding securing member

|  | E05C 17/50 |
· · · | comprising a single pivoted securing member

|  | E05C 17/52 |
· · · | comprising a snap, catch, or the like

|  | E05C 17/54 |
· · | Portable devices, e.g. wedges

|  | E05C 17/56 |
· | by magnetic or electromagnetic attraction (operation of locks or fasteners by electric or magnetic means Fulltext... Hierarchy... Expanded...E05B 47/00)

|  | E05C 17/58 |
· | operated or controlled from a distance

|  | E05C 19/00 |
Other devices specially designed for securing wings (movable draft sealings additionally used for bolting Fulltext... Hierarchy... Expanded...E06B 7/18)

|  | E05C 19/02 |
· | Automatic catches, i.e. released by pull or pressure on the wing (Fulltext... Hierarchy... Expanded...E05C 19/06 takes precedence)

|  | E05C 19/04 |
· · | Ball or roller catches

|  | E05C 19/06 |
· | in which the securing part is formed or carried by a spring and moves only by distortion of the spring, e.g. snaps

|  | E05C 19/08 |
· | Hasps; Hasp fastenings; Spring catches therefor

|  | E05C 19/10 |
· | Hook fastenings; Fastenings in which a link engages a fixed hook-like member

|  | E05C 19/12 |
· · | pivotally mounted

|  | E05C 19/14 |
· · · | with toggle action

|  | E05C 19/16 |
· | Devices holding the wing by magnetic or electromagnetic attraction

|  | E05C 19/18 |
· | Portable devices specially adapted for securing wings (preventing operation of handles Fulltext... Hierarchy... Expanded...E05B 13/00)

|  | E05C 21/00 |
Arrangements or combinations of wing fastening, securing, or holding devices, not covered by a single preceding main group

|  | E05C 21/02 |
· | for holding a wing closed only