|  | B |
SECTION B — PERFORMING OPERATIONS

TRANSPORTING

|  | B67 |
LIQUID HANDLING

|  | B67B |
METHODS OF, OR APPARATUS OR DEVICES FOR, APPLYING CLOSURE MEMBERS TO BOTTLES, JARS, OR SIMILAR CONTAINERS; HAND- OR POWER-OPERATED APPARATUS OR DEVICES OPENING CLOSED CONTAINERS (attached to, or incorporated in containers or container closures Fulltext... Hierarchy... Expanded...B65D)

|  | B67B 1/00 |
Closing bottles or jars by applying stoppers

|  | B67B 1/02 |
· | Preparatory cleaning, steaming, or heating of the stoppers (mechanical working of cork Fulltext... Hierarchy... Expanded...B27J 5/00)

|  | B67B 1/04 |
· | by inserting threadless stoppers, e.g. corks

|  | B67B 1/06 |
· | by inserting and rotating screw stoppers

|  | B67B 1/08 |
· | Securing stoppers, e.g. swing stoppers, which are held in position by associated pressure-applying means coacting with the bottle neck

|  | B67B 3/00 |
Closing bottles or jars by applying caps

|  | B67B 3/02 |
· | by applying flanged caps, e.g. crown caps, and securing by deformation of flanges

|  | B67B 3/04 |
· · | Cutting caps from strip material in capping machines (devices for registering moving strip material Fulltext... Hierarchy... Expanded...B65H 23/00)

|  | B67B 3/06 |
· · | Feeding caps to dies

|  | B67B 3/062 |
· · · | from a magazine

|  | B67B 3/064 |
· · · | from a hopper

|  | B67B 3/08 |
· · | Mechanisms for causing relative movement between bottle or jar and cap-applying die

|  | B67B 3/10 |
· · | Dies for securing caps

|  | B67B 3/12 |
· · · | movable axially relative to cap to deform flanges thereof

|  | B67B 3/14 |
· · · | with movable elements, e.g. hinged fingers, for applying radial pressure to the flange of the cap (elastic dies Fulltext... Hierarchy... Expanded...B67B 3/16)

|  | B67B 3/16 |
· · · | elastic

|  | B67B 3/18 |
· · · | Rotary dies, e.g. for forming screw threads in situ

|  | B67B 3/20 |
· | by applying and rotating preformed threaded caps (elastic dies for forming threads on flanged caps in situ Fulltext... Hierarchy... Expanded...B67B 3/16)

|  | B67B 3/22 |
· | by applying snap-on caps

|  | B67B 3/24 |
· | Special measures for applying and securing caps under vacuum

|  | B67B 3/26 |
· | Applications of control, warning, or safety devices in capping machinery

|  | B67B 5/00 |
Closing bottles or jars by applying and securing or by forming other types of closures; Applying protective or decorative covers to closures; Devices for securing bottle closures with wire (infant-feeding teats with means for fastening to bottles Fulltext... Hierarchy... Expanded...A61J 11/04)

|  | B67B 5/02 |
· | by inserting disc-closures

|  | B67B 5/04 |
· | Forming closures, or protective or decorative covers therefor, in situ by applying liquids, w. g. by dipping

|  | B67B 5/06 |
· | Devices for securing bottle closures with wire

|  | B67B 7/00 |
Hand- or power-operated devices for opening closed containers (nail pullers or extractors Fulltext... Hierarchy... Expanded...B25C 11/00; attached to, or incorporated in containers or in container closures Fulltext... Hierarchy... Expanded...B65D)

|  | B67B 7/02 |
· | for removing stoppers

|  | B67B 7/04 |
· · | Cork-screws

|  | B67B 7/06 |
· · | Other cork removers

|  | B67B 7/08 |
· · · | using air or gas pressure

|  | B67B 7/10 |
· · | with means for retrieving stoppers from the interior of the container

|  | B67B 7/12 |
· | for removing disc-closures

|  | B67B 7/14 |
· | for removing tightly-fitting lids or covers, e.g. of shoe-polish tins, by gripping and rotating

|  | B67B 7/16 |
· | for removing flanged caps, e.g. crown caps

|  | B67B 7/18 |
· | for removing threaded caps (wrenches Fulltext... Hierarchy... Expanded...B25B 13/00) [2]

|  | B67B 7/20 |
· | for breaking vacuum seals between lids or covers and bodies of preserving jars, e.g. by wedge action

|  | B67B 7/22 |
· · | incorporating loops, e.g. of wire, which are tightened around seal

|  | B67B 7/24 |
· | Hole-piercing devices

|  | B67B 7/26 |
· · | combined with spouts

|  | B67B 7/28 |
· · · | and associated with receptacle holders

|  | B67B 7/30 |
· | Hand-operated cutting devices

|  | B67B 7/32 |
· · | propelled by rotary gears or wheels around periphery of container

|  | B67B 7/34 |
· · | with rotatable cutters

|  | B67B 7/36 |
· · | adapted to be mounted on walls

|  | B67B 7/38 |
· | Power-operated cutting devices (machines for domestic use with a plurality of interchangeable units Fulltext... Hierarchy... Expanded...A47J 43/06, Fulltext... Hierarchy... Expanded...A47J 44/00)

|  | B67B 7/40 |
· | Devices for engaging tags, strips, or tongues for opening by tearing, e.g. slotted keys for opening sardine tins

|  | B67B 7/42 |
· | Devices for removing barrel bungs

|  | B67B 7/44 |
· | Combination tools, e.g. comprising cork-screws, can piercers, crown-cap removers (combinations of opening devices with cutting tools Fulltext... Hierarchy... Expanded...B26, with devices serving other purposes, see appropriate sub-classes, e.g. Fulltext... Hierarchy... Expanded...B25F, Fulltext... Hierarchy... Expanded...B43K 29/00)