|  | F |
SECTION F — MECHANICAL ENGINEERING; LIGHTING; HEATING; WEAPONS; BLASTING

LIGHTING AND HEATING

|  | F22 |
STEAM GENERATION (chemical or physical apparatus for generating gases Fulltext... Hierarchy... Expanded...B01J; chemical generation of gas, e.g. under pressure, Section C; generating combustion products of high pressure or high velocity Fulltext... Hierarchy... Expanded...F23R)

|  | F22 |
Note(s) In this class, the term "steam" also covers other condensable vapours, g. mercury, diphenyl, diphenyl oxide.

|  | F22G |
SUPERHEATING OF STEAM (steam-separating arrangements in boilers Fulltext... Hierarchy... Expanded...F22B 37/26)

|  | F22G 1/00 |
Steam superheating characterised by heating method (exothermal chemical reactions not involving a supply of free oxygen gas, apparatus or devices for using the heat therefrom Fulltext... Hierarchy... Expanded...F24J)

|  | F22G 1/02 |
· | with heat supply by hot flue gases from the furnace of the steam boiler

|  | F22G 1/04 |
· · | by diverting flow or hot flue gases to separate superheaters operating in reheating cycle, e.g. for reheating steam between a high-pressure turbine stage and an intermediate turbine stage

|  | F22G 1/06 |
· | with heat supply predominantly by radiation

|  | F22G 1/08 |
· · | from heated brickwork or the like

|  | F22G 1/10 |
· | with provision for superheating by throttling

|  | F22G 1/12 |
· | by mixing steam with furnace gases or other combustion products

|  | F22G 1/14 |
· | using heat generated by chemical reactions

|  | F22G 1/16 |
· | by using a separate heat source independent from heat supply of the steam boiler, e.g. by electricity, by auxiliary combustion of fuel oil

|  | F22G 3/00 |
Steam superheaters characterised by constructional features; Details of component parts thereof (general aspects of enclosed heat-exchangers Fulltext... Hierarchy... Expanded...F28D)

|  | F22G 5/00 |
Controlling superheat temperature (control systems for steam boilers Fulltext... Hierarchy... Expanded...F22B; regulating or controlling in general Fulltext... Hierarchy... Expanded...G05)

|  | F22G 5/02 |
· | Applications of combustion-control devices, e.g. tangential-firing burners, tilting burners

|  | F22G 5/04 |
· | by regulating flue gas flow, e.g. by proportioning or diverting

|  | F22G 5/06 |
· | by recirculating flue gases

|  | F22G 5/08 |
· · | preventing furnace gas backflow through recirculating fan

|  | F22G 5/10 |
· | by displacing superheater sections

|  | F22G 5/12 |
· | by attemperating the superheated steam, e.g. by injected water sprays (spray mixers Fulltext... Hierarchy... Expanded...B01F 5/18)

|  | F22G 5/14 |
· · | by live steam

|  | F22G 5/16 |
· | by indirectly cooling or heating the superheated steam in auxiliary enclosed heat-exchanger

|  | F22G 5/18 |
· | by by-passing steam around superheater sections

|  | F22G 5/20 |
· | by combined controlling procedures

|  | F22G 7/00 |
Steam superheaters characterised by location, arrangement, or disposition

|  | F22G 7/02 |
· | in fire tubes

|  | F22G 7/04 |
· | in jackets around fire tubes

|  | F22G 7/06 |
· | in furnace tubes

|  | F22G 7/08 |
· | in fire-boxes

|  | F22G 7/10 |
· | in smoke-boxes

|  | F22G 7/12 |
· | in flues

|  | F22G 7/14 |
· | in water-tube boilers, e.g. between banks of water tubes