|  | E |
SECTION E — FIXED CONSTRUCTIONS

BUILDING

|  | E05 |
LOCKS; KEYS; WINDOW OR DOOR FITTINGS; SAFES

|  | E05 |
Note(s) In this class, the following terms are used with the meanings stated: "Wing" is a general term for doors, openable windows, and other movable members to which similar fastening devices may be applied, e.g. drawers, lids of chests, car boots, car bonnets. A wing may swing, slide, or move in any other manner. "Frame" means any member to which a wing may be held by a fastening device. It does not include a framework forming part of the wing, but it may be another wing. "Lock" means primarily a device for releasing or securing any member, which requires a key or a permutation mechanism for release. "Bolt" means a sliding, pivoted, or otherwise movable member such as is normally carried by a door to hold it shut by engagement with a keeper on the frame. It may be operated by hand directly or through mechanism or by a key; it may be a latch (see (5) below) "Latch" means a bolt arranged to be moved to the releasing position against the force of a spring, or some other returning force, when a wing meets the frame on closing, so that it does not have to be operated by hand to secure the wing, but only to open it. "Hasp" means a member hinged to the frame or wing so that it can be moved towards the face of the wing or frame and secured thereto, e.g. by a turn-button, by a padlock and staple.

|  | E05B |
LOCKS OR ACCESSORIES; KEYLESS LOCKS; CONTROL OR OPERATION OF LOCKS; NON-MECHANICAL CONTROL OR OPERATION OF OTHER WING-FASTENING DEVICES (wing-fastening devices per se, other than locks, Fulltext... Hierarchy... Expanded...E05C); LOCKING DEVICES FOR OBJECTS; HANDCUFFS

|  | E05B 1/00 - E05B 17/00 |
Parts of locks or the like mountable on or in wings

|  | E05B 1/00 |
Knobs or handles for wings (for furniture Fulltext... Hierarchy... Expanded...A47B 95/02); Knobs, handles, or press buttons for locks or latches on wings (Fulltext... Hierarchy... Expanded...A47B 5/00, Fulltext... Hierarchy... Expanded...A47B 7/00 take precedence)

|  | E05B 1/02 |
· | of solid material

|  | E05B 1/04 |
· | with inner rigid member and outer cover or covers

|  | E05B 1/06 |
· | of sheet material

|  | E05B 3/00 |
Fastening handles to lock or latch parts

|  | E05B 3/02 |
· | Fastening handles to the spindle by pinning or riveting

|  | E05B 3/04 |
· | Fastening the handle shank to the spindle by screws, springs, or snap bolts

|  | E05B 3/06 |
· | by means arranged in or on the rose

|  | E05B 3/08 |
· | Fastening the spindle to the follower

|  | E05B 3/10 |
· | by a bipartite or cleft spindle in the follower or in the handle shank

|  | E05B 5/00 |
Handles completely let into the surface of the wing

|  | E05B 5/02 |
· | able to be turned outwards before operation

|  | E05B 5/04 |
· | able to be shifted parallel to the wing after being pulled out

|  | E05B 7/00 |
Handles pivoted about an axis parallel to the wing (Fulltext... Hierarchy... Expanded...E05B 5/00 takes precedence)

|  | E05B 9/00 |
Lock or latch-mechanism casings (padlock casings Fulltext... Hierarchy... Expanded...E05B 67/02)

|  | E05B 9/02 |
· | of latch-bolt locks

|  | E05B 9/04 |
· | of cylinder locks

|  | E05B 9/06 |
· | Fastening together the parts of casings

|  | E05B 9/08 |
· | Fastening the casings of latch-bolt locks or cylinder locks to the wing

|  | E05B 9/10 |
· | Coupling devices for the two halves of double cylinder locks

|  | E05B 11/00 |
Devices preventing keys from being removed from the lock

|  | E05B 11/02 |
· | before the wing is locked

|  | E05B 11/04 |
· | before the wing is closed

|  | E05B 11/06 |
· | for catching skeleton or incorrect keys

|  | E05B 13/00 |
Devices preventing the key or the handle or both from being used

|  | E05B 13/02 |
· | shaped as sectors of escutcheons, arranged in the keyhole

|  | E05B 13/04 |
· | shaped as fork-like implements grasping and fixing the key

|  | E05B 13/06 |
· | shaped as bolt detents arranged in the path of motion of the key bit

|  | E05B 13/08 |
· | formed by longitudinal bolt or cross-bar connecting the handle with a stationary lock part or fitting

|  | E05B 13/10 |
· | formed by a lock arranged in the handle

|  | E05B 15/00 |
Other details of locks; Parts for engagement by bolts of fastening devices (specially adapted for particular kinds of fastening devices, see the relevant groups for the kinds of devices in Fulltext... Hierarchy... Expanded...E05C)

|  | E05B 15/02 |
· | Striking-plates; Keepers; Bolt staples; Escutcheons

|  | E05B 15/04 |
· | Spring arrangements in locks

|  | E05B 15/06 |
· | Lock wards

|  | E05B 15/08 |
· | Key guides; Key pins

|  | E05B 15/10 |
· | Bolts of locks or night latches

|  | E05B 15/12 |
· | Pins or detents for locking bolts

|  | E05B 15/14 |
· | Tumblers

|  | E05B 15/16 |
· | Use of special materials for parts of locks (for handles Fulltext... Hierarchy... Expanded...E05B 1/00)

|  | E05B 17/00 |
Accessories in connection with locks or latch handles

|  | E05B 17/02 |
· | Coupling devices for double doors, i.e. two doors one behind the other and hinged on the same side

|  | E05B 17/04 |
· | Devices for coupling the turning cylinder of a single or double cylinder lock with the bolt-operating member

|  | E05B 17/06 |
· | Templates for marking the position of apertures in fittings of wings

|  | E05B 17/08 |
· | Lubricating devices

|  | E05B 17/10 |
· | Illuminating devices on, or for, locks or keys

|  | E05B 17/12 |
· | Devices for removing keys stuck in the lock

|  | E05B 17/14 |
· | Closures or guards for keyholes

|  | E05B 17/16 |
· · | shaped as pins or key bits

|  | E05B 17/18 |
· · | shaped as lids or slides

|  | E05B 19/00 |
Keys; Accessories therefor

|  | E05B 19/02 |
· | Construction of the shank of the key

|  | E05B 19/04 |
· | Construction of the bow of the key; Construction of flat keys

|  | E05B 19/06 |
· | Key bits; Flat key bits

|  | E05B 19/08 |
· · | Special forms of key bits, e.g. double key bits, folding key bits

|  | E05B 19/10 |
· | Fastening the key bit and bow on the shank of the key

|  | E05B 19/12 |
· | Keys with several bits moving relatively to each other when in use

|  | E05B 19/14 |
· | Double keys

|  | E05B 19/16 |
· | Extremely thin keys acting without rotation

|  | E05B 19/18 |
· | Keys adjustable before use

|  | E05B 19/20 |
· | Skeleton keys; Devices for picking locks; Other devices for similar purposes

|  | E05B 19/22 |
· | Keys with devices for indicating whether the last operation was locking or unlocking

|  | E05B 19/24 |
· | Key-distinguishing marks

|  | E05B 19/26 |
· | Use of special materials for keys

|  | E05B 21/00 - E05B 25/00 |
Locks with rotary keys moving lamelliform tumblers perpendicular to the key

|  | E05B 21/00 |
Locks with tumblers not following the movement of the bolt

|  | E05B 21/02 |
· | with identical tumblers

|  | E05B 21/04 |
· | with stop pins on the tumbler (Fulltext... Hierarchy... Expanded...E05B 21/02 takes precedence)

|  | E05B 21/06 |
· | Cylinder locks, e.g. protector locks

|  | E05B 23/00 |
Locks with tumblers following the movement of the bolt

|  | E05B 25/00 |
Locks with special tumblers

|  | E05B 25/02 |
· | with tumblers in the cut-out of which the key bit is moved

|  | E05B 25/04 |
· | with tumblers in which the stop pin is guided from one locked position to the other in an inclined direction

|  | E05B 25/06 |
· | with tumblers in which the stop pin is guided from one locked position to the other along a curved path

|  | E05B 25/08 |
· | with tumblers with movable pawls engaging the key

|  | E05B 25/10 |
· | with tumblers formed to engage one another to determine their unlocked position

|  | E05B 27/00 - E05B 33/00 |
Locks of which the tumblers are set by pushing the key in

|  | E05B 27/00 |
Cylinder locks with tumbler pins or balls

|  | E05B 27/02 |
· | operated by the edge of the key

|  | E05B 27/04 |
· · | arranged radially in one row

|  | E05B 27/06 |
· · | arranged radially in more than one row

|  | E05B 27/08 |
· · | arranged axially

|  | E05B 27/10 |
· | operated by other surfaces of the key, e.g. openings receiving projections on the tumblers

|  | E05B 29/00 |
Cylinder locks with plate tumblers

|  | E05B 29/02 |
· | operated by the edge of the key

|  | E05B 29/04 |
· · | arranged singly

|  | E05B 29/06 |
· · | arranged in pairs

|  | E05B 29/08 |
· | operated by other surfaces of the key

|  | E05B 29/10 |
· · | operated by a curved groove or slot

|  | E05B 29/12 |
· · | operated by a curved rib

|  | E05B 29/14 |
· | with both axially and radially arranged plate tumblers

|  | E05B 31/00 |
Cylinder locks with both tumbler pins or balls and plate tumblers

|  | E05B 33/00 |
Cylinder locks in which the bolt is moved by means other than the key

|  | E05B 35/00 |
Locks for use with special keys or a plurality of keys

|  | E05B 35/02 |
· | which can be shifted laterally

|  | E05B 35/04 |
· | for pull keys

|  | E05B 35/06 |
· | for screw keys

|  | E05B 35/08 |
· | operable by a plurality of keys

|  | E05B 35/10 |
· · | with master and pass keys

|  | E05B 35/12 |
· · | requiring the use of two keys, e.g. safe-deposit locks

|  | E05B 35/14 |
· | with keys of which different parts operate separate mechanisms

|  | E05B 37/00 |
Permutation locks (electric permutation locks Fulltext... Hierarchy... Expanded...E05B 49/00; for bicycles Fulltext... Hierarchy... Expanded...E05B 71/02); Puzzle locks

|  | E05B 37/02 |
· | with tumbler discs or rings arranged on a single axis, each disc being adjustable independently of the others

|  | E05B 37/04 |
· | with tumbler discs on a single axis, all the discs being adjustable by rotating a shiftable knob

|  | E05B 37/06 |
· · | in padlocks

|  | E05B 37/08 |
· | with tumbler discs on a single axis, all the discs being adjustable by a rotary knob which is not shifted

|  | E05B 37/10 |
· · | in padlocks

|  | E05B 37/12 |
· | with tumbler discs on several axes

|  | E05B 37/14 |
· · | in padlocks

|  | E05B 37/16 |
· | with two or more push or pull knobs, slides, or the like

|  | E05B 37/18 |
· · | in padlocks

|  | E05B 37/20 |
· | Puzzle locks

|  | E05B 37/22 |
· · | in padlocks

|  | E05B 39/00 - E05B 45/00 |
Locks with indicating or timing devices

|  | E05B 39/00 |
Locks giving indication of unauthorised unlocking

|  | E05B 39/02 |
· | with destructible seal closures or paper closures

|  | E05B 39/04 |
· | with counting or registering devices

|  | E05B 41/00 |
Locks with visible indication as to whether the lock is locked or unlocked

|  | E05B 43/00 |
Time locks (clocks or clock mechanisms with attached or built-in means operating any device at preselected times or after a predetermined time interval Fulltext... Hierarchy... Expanded...G04B 23/00)

|  | E05B 45/00 |
Alarm locks (alarm devices actuated by tampering with fastenings in general Fulltext... Hierarchy... Expanded...G08B)

|  | E05B 45/02 |
· | with mechanically-operated bells

|  | E05B 45/04 |
· | with detonating alarm devices

|  | E05B 45/06 |
· | Electric alarm locks

|  | E05B 45/08 |
· · | with contact making inside the lock or in the striking plate

|  | E05B 45/10 |
· · · | by introducing the key

|  | E05B 45/12 |
· · · | by movement of the bolt

|  | E05B 45/14 |
· · | with contact making outside the lock

|  | E05B 47/00 - E05B 51/00 |
Operation or control of locks by non-mechanical means, e.g. from a distance (locking doors simultaneously in passenger vehicles Fulltext... Hierarchy... Expanded...E05B 65/36; key switches Fulltext... Hierarchy... Expanded...H01H 27/00)

|  | E05B 47/00 |
Operating or controlling locks or other fastening devices by electric or magnetic means (electric permutation locks Fulltext... Hierarchy... Expanded...E05B 49/00; holding in open position or limiting movement of wings by magnetic or electromagnetic attraction Fulltext... Hierarchy... Expanded...E05C 17/56) [2]

|  | E05B 47/02 |
· | Adaptation of locks, latches, or parts thereof, for movement of the bolt by electromagnetic means

|  | E05B 47/04 |
· · | for unlocking only

|  | E05B 47/06 |
· | Controlling mechanically-operated bolts by electromagnetically-operated detents

|  | E05B 47/08 |
· · | the bolt being withdrawn by a spring which is stressed by closing the wing

|  | E05B 49/00 |
Electric permutation locks; Circuits therefor

|  | E05B 49/02 |
· | with electrical arrangements inside the lock

|  | E05B 49/04 |
· | with electrical arrangements outside the lock

|  | E05B 51/00 |
Operating or controlling locks or other fastening devices by other non-mechanical means

|  | E05B 51/02 |
· | by pneumatic or hydraulic means

|  | E05B 53/00 |
Operation or control of locks by mechanical transmissions, e.g. from a distance (for passenger vehicles Fulltext... Hierarchy... Expanded...E05B 65/20)

|  | E05B 55/00 - E05B 61/00 |
Locks with provision for latching (for passenger vehicle doors Fulltext... Hierarchy... Expanded...E05B 65/20)

|  | E05B 55/00 |
Locks in which a sliding latch is used also as a locking bolt

|  | E05B 55/02 |
· | the bolt being secured by the tumbler

|  | E05B 55/04 |
· | the bolt being secured by the cross-bar or the turnbuckle and the handle being locked

|  | E05B 55/06 |
· | the handle being disconnected

|  | E05B 55/08 |
· · | the bolt being secured by transverse bolts

|  | E05B 55/10 |
· · | without securing the bolt

|  | E05B 55/12 |
· | the bolt being secured by the operation of a hidden parallel member

|  | E05B 55/14 |
· | the bolt being secured by the operation of a wing handle, or by means in the wing handle or knob

|  | E05B 55/16 |
· · | merely by normal use of the handle on one side of the wing

|  | E05B 57/00 |
Locks in which a pivoted latch is used also as locking means

|  | E05B 59/00 |
Locks with latches separate from the lock-bolts, or with a plurality of latches or lock-bolts

|  | E05B 59/02 |
· | with arrangements for securing the latch while shooting the lock-bolt

|  | E05B 59/04 |
· | Locks in which the latch is moved by a lock-bolt, or the lock-bolt by a latch, or one latch by another, etc.

|  | E05B 59/06 |
· | with a lock-bolt slidable in the latch

|  | E05B 61/00 |
Other locks with provision for latching

|  | E05B 63/00 - E05B 67/00 |
Locks with special structural characteristics or for special use

|  | E05B 63/00 |
Locks with special structural characteristics

|  | E05B 63/02 |
· | without springs

|  | E05B 63/04 |
· | for alternative use on the right-hand or left-hand side of wings

|  | E05B 63/06 |
· | with lengthwise-adjustable bolts

|  | E05B 63/08 |
· | Mortise locks

|  | E05B 63/10 |
· · | requiring only two cylindrical holes in the wing

|  | E05B 63/12 |
· | with means carried by the bolt for interlocking with the keeper (for passenger vehicle doors Fulltext... Hierarchy... Expanded...E05B 65/28)

|  | E05B 63/14 |
· | Arrangement of several locks or locks with several bolts, e.g. arranged one behind the other (locks for keys with several bits Fulltext... Hierarchy... Expanded...E05B 35/14; with provision for latching Fulltext... Hierarchy... Expanded...E05B 59/00, Fulltext... Hierarchy... Expanded...E05B 61/00)

|  | E05B 63/16 |
· | with the handles on opposite sides moving independently (the latch being secured by the operation of a wing handle Fulltext... Hierarchy... Expanded...E05B 55/14)

|  | E05B 63/18 |
· | with arrangements independent of the locking mechanism for retaining the bolt in the retracted position

|  | E05B 63/20 |
· · | released automatically when the wing is closed

|  | E05B 63/22 |
· | operated by a pulling or pushing action perpendicular to the front plate (Fulltext... Hierarchy... Expanded...E05B 35/04 takes precedence)

|  | E05B 65/00 |
Locks for special use

|  | E05B 65/02 |
· | for thin, hollow, or thin-metal wings

|  | E05B 65/04 |
· | for wings one behind the other hinged on the same side

|  | E05B 65/06 |
· | for swing doors

|  | E05B 65/08 |
· | for sliding wings

|  | E05B 65/10 |
· | for panic or emergency doors

|  | E05B 65/12 |
· | for vehicles (Fulltext... Hierarchy... Expanded...E05B 71/00 takes precedence)

|  | E05B 65/14 |
· · | for railway freight-cars or the like; for lorries (for front doors of road vehicles Fulltext... Hierarchy... Expanded...E05B 65/20)

|  | E05B 65/16 |
· · · | for back doors of vans

|  | E05B 65/18 |
· · · | with provision for sealing

|  | E05B 65/19 |
· · | for car-boot lids; for car bonnets

|  | E05B 65/20 |
· · | for passenger or like doors (bolt-fastenings per se Fulltext... Hierarchy... Expanded...E05C)

|  | E05B 65/22 |
· · · | with rectilinearly-moving bolt

|  | E05B 65/24 |
· · · · | locked by a special movement of the door handle

|  | E05B 65/26 |
· · · · | with the outside door handle drawn into a recess when the door is locked

|  | E05B 65/28 |
· · · · | with means carried by the bolt for interlocking with the keeper

|  | E05B 65/30 |
· · · · | with two or more bolts moved simultaneously

|  | E05B 65/32 |
· · · | with the bolt turning about an axis

|  | E05B 65/34 |
· · · · | in which the member engaging the keeper is shaped as a lockable toothed wheel or the like

|  | E05B 65/36 |
· · · | Locking several doors simultaneously

|  | E05B 65/38 |
· · · · | by pneumatic or hydraulic means

|  | E05B 65/40 |
· · · | Locking one door by shutting another (by non-mechanical means Fulltext... Hierarchy... Expanded...E05B 47/00, Fulltext... Hierarchy... Expanded...E05B 51/00; fastenings, other than locks, for double doors Fulltext... Hierarchy... Expanded...E05C 7/06; operating fastenings, other than locks, by mechanical transmission Fulltext... Hierarchy... Expanded...E05C 13/04)

|  | E05B 65/42 |
· · · | Securing the latch or bolt by movement of the vehicle

|  | E05B 65/44 |
· | for furniture or drawers

|  | E05B 65/46 |
· · | Special locks for drawers, e.g. for a plurality of drawers (mechanisms for securing one drawer by closing another Fulltext... Hierarchy... Expanded...E05C 15/04)

|  | E05B 65/48 |
· | Hasp locks

|  | E05B 65/50 |
· · | for briefcases

|  | E05B 65/52 |
· | Other locks for chests, boxes, trunks, baskets, travelling bags, etc. (closures for bags or trunks Fulltext... Hierarchy... Expanded...A45C 13/06, Fulltext... Hierarchy... Expanded...A45C 13/10, Fulltext... Hierarchy... Expanded...A45C 13/16)

|  | E05B 67/00 |
Padlocks (permutation locks Fulltext... Hierarchy... Expanded...E05B 37/00); Details thereof

|  | E05B 67/02 |
· | Cases

|  | E05B 67/04 |
· · | Armoured cases

|  | E05B 67/06 |
· | Shackles; Arrangement of the shackle

|  | E05B 67/08 |
· · | Padlocks with shackles hinged on the case

|  | E05B 67/10 |
· · · | with devices for securing the free end of the shackle

|  | E05B 67/12 |
· · · · | with built-in cylinder locks

|  | E05B 67/14 |
· · · | with devices for securing the hinged end of the shackle

|  | E05B 67/16 |
· · · · | with built-in cylinder locks

|  | E05B 67/18 |
· · · | with devices for securing both ends of the shackle

|  | E05B 67/20 |
· · · · | with built-in cylinder locks

|  | E05B 67/22 |
· · | Padlocks with sliding shackles, with or without rotary or pivotal movement

|  | E05B 67/24 |
· · · | with built-in cylinder locks

|  | E05B 67/26 |
· · · | with screw action, with or without the shackle being moved by turning the key

|  | E05B 67/28 |
· · | Padlocks with shackles forming a circle

|  | E05B 67/30 |
· · · | with built-in cylinder locks

|  | E05B 67/32 |
· · | Padlocks with pincer-like shackles

|  | E05B 67/34 |
· · · | with built-in cylinder locks

|  | E05B 67/36 |
· | Padlocks with closing means other than shackles

|  | E05B 67/38 |
· | Auxiliary or protective devices

|  | E05B 69/00 - E05B 73/00 |
Locking devices for clothing, sticks, umbrellas, or cycles

|  | E05B 69/00 |
Devices for locking clothing; Lockable clothing holders or hangers (clothing holders without locking devices Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...A47G 25/00-A47G 25/10)

|  | E05B 69/02 |
· | Lockable clothing hooks (coin-controlled locking hooks Fulltext... Hierarchy... Expanded...G07F)

|  | E05B 71/00 |
Locks specially adapted for bicycles, other than padlocks (locks integral with cycles Fulltext... Hierarchy... Expanded...B62H 5/00)

|  | E05B 71/02 |
· | with permutation locking devices

|  | E05B 73/00 |
Devices for locking portable objects against unauthorised removal; Miscellaneous locking devices

|  | E05B 73/02 |
· | for walking-sticks or umbrellas (stick or umbrella holders in general Fulltext... Hierarchy... Expanded...A47G 25/12)

|  | E05B 75/00 |
Handcuffs