|  | E |
SECTION E — FIXED CONSTRUCTIONS

BUILDING

|  | E05 |
LOCKS; KEYS; WINDOW OR DOOR FITTINGS; SAFES

|  | E05 |
Note(s) In this class, the following terms are used with the meanings indicated: "Wing" is a general term for swingable, slidable, or otherwise movable doors or windows. The term also encompasses other movable structures such as drawers, lids of chests, car boots, or car bonnets, to which the operating, mounting, latching, or locking means of this class may be applied. "Frame" means any member to which a wing may be held by a fastening device. It does not include a framework forming part of the wing, but it may be another wing. "Lock" means primarily a device for releasing or securing any member, which requires a key or a permutation mechanism for release. "Bolt" means a sliding, pivoted, or otherwise movable member such as is normally carried by a door to hold it shut by engagement with a keeper on the frame. It may be operated by hand directly or through mechanism or by a key; it may be a latch (see (e) below.) "Latch" means a bolt arranged to be moved to the releasing position against the force of a spring, or some other returning force, when a wing meets the frame on closing, so that it does not have to be operated by hand to secure the wing, but only to open it. "Hasp" means a member hinged to the frame or wing so that it can be moved towards the face of the wing or frame and secured thereto, e.g. by a turn-button, by a padlock and staple.

|  | E05B |
LOCKS OR ACCESSORIES; KEYLESS LOCKS; CONTROL OR OPERATION OF LOCKS; NON-MECHANICAL CON- TROL OR OPERATION OF OTHER WING-FASTENING DEVICES (wing-fastening devices per se, other than locks, Fulltext... Hierarchy... Expanded...E05C); LOCKING DEVICES FOR OBJECTS; HANDCUFFS

|  | E05B 1/00 - E05B 17/00 |
Parts of locks or the like mountable on or in wings

|  | E05B 1/00 |
Knobs or handles for wings (for furniture Fulltext... Hierarchy... Expanded...A47B 95/02); Knobs, handles, or press buttons for locks or latches on wings (Fulltext... Hierarchy... Expanded...A47B 5/00, Fulltext... Hierarchy... Expanded...A47B 7/00 take precedence)

|  | E05B 1/02 |
· | of solid material

|  | E05B 1/04 |
· | with inner rigid member and outer cover or covers

|  | E05B 1/06 |
· | of sheet material

|  | E05B 3/00 |
Fastening handles to lock or latch parts

|  | E05B 3/02 |
· | Fastening handles to the spindle by pinning or riveting

|  | E05B 3/04 |
· | Fastening the handle shank to the spindle by screws, springs, or snap bolts

|  | E05B 3/06 |
· | by means arranged in or on the rose

|  | E05B 3/08 |
· | Fastening the spindle to the follower

|  | E05B 3/10 |
· | by a bipartite or cleft spindle in the follower or in the handle shank

|  | E05B 5/00 |
Handles completely let into the surface of the wing

|  | E05B 5/02 |
· | able to be turned outwards before operation

|  | E05B 5/04 |
· | able to be shifted parallel to the wing after being pulled out

|  | E05B 7/00 |
Handles pivoted about an axis parallel to the wing (Fulltext... Hierarchy... Expanded...E05B 5/00 takes precedence)

|  | E05B 9/00 |
Lock or latch-mechanism casings (padlock casings Fulltext... Hierarchy... Expanded...E05B 67/02)

|  | E05B 9/02 |
· | of latch-bolt locks

|  | E05B 9/04 |
· | of cylinder locks

|  | E05B 9/06 |
· | Fastening together the parts of casings

|  | E05B 9/08 |
· | Fastening the casings of latch-bolt locks or cylinder locks to the wing

|  | E05B 9/10 |
· | Coupling devices for the two halves of double cylinder locks

|  | E05B 11/00 |
Devices preventing keys from being removed from the lock

|  | E05B 11/02 |
· | before the wing is locked

|  | E05B 11/04 |
· | before the wing is closed

|  | E05B 11/06 |
· | for catching skeleton or incorrect keys

|  | E05B 13/00 |
Devices preventing the key or the handle or both from being used

|  | E05B 13/02 |
· | shaped as sectors of escutcheons, arranged in the keyhole

|  | E05B 13/04 |
· | shaped as fork-like implements grasping and fixing the key

|  | E05B 13/06 |
· | shaped as bolt detents arranged in the path of motion of the key bit

|  | E05B 13/08 |
· | formed by longitudinal bolt or cross-bar connecting the handle with a stationary lock part or fitting

|  | E05B 13/10 |
· | formed by a lock arranged in the handle

|  | E05B 15/00 |
Other details of locks; Parts for engagement by bolts of fastening devices (specially adapted for particular kinds of fastening devices, see the relevant groups for the kinds of devices in Fulltext... Hierarchy... Expanded...E05C)

|  | E05B 15/02 |
· | Striking-plates; Keepers; Bolt staples; Escutcheons

|  | E05B 15/04 |
· | Spring arrangements in locks

|  | E05B 15/06 |
· | Lock wards

|  | E05B 15/08 |
· | Key guides; Key pins

|  | E05B 15/10 |
· | Bolts of locks or night latches

|  | E05B 15/12 |
· | Pins or detents for locking bolts

|  | E05B 15/14 |
· | Tumblers

|  | E05B 15/16 |
· | Use of special materials for parts of locks (for handles Fulltext... Hierarchy... Expanded...E05B 1/00)

|  | E05B 17/00 |
Accessories in connection with locks or latch handles

|  | E05B 17/02 |
· | Coupling devices for double doors, i.e. two doors one behind the other and hinged on the same side

|  | E05B 17/04 |
· | Devices for coupling the turning cylinder of a single or double cylinder lock with the bolt-operating member

|  | E05B 17/06 |
· | Templates for marking the position of apertures in fittings of wings

|  | E05B 17/08 |
· | Lubricating devices

|  | E05B 17/10 |
· | Illuminating devices on, or for, locks or keys

|  | E05B 17/12 |
· | Devices for removing keys stuck in the lock

|  | E05B 17/14 |
· | Closures or guards for keyholes

|  | E05B 17/16 |
· · | shaped as pins or key bits

|  | E05B 17/18 |
· · | shaped as lids or slides

|  | E05B 19/00 |
Keys; Accessories therefor

|  | E05B 19/02 |
· | Construction of the shank of the key

|  | E05B 19/04 |
· | Construction of the bow of the key; Construction of flat keys

|  | E05B 19/06 |
· | Key bits; Flat key bits

|  | E05B 19/08 |
· · | Special forms of key bits, e.g. double key bits, folding key bits

|  | E05B 19/10 |
· | Fastening the key bit and bow on the shank of the key

|  | E05B 19/12 |
· | Keys with several bits moving relatively to each other when in use

|  | E05B 19/14 |
· | Double keys

|  | E05B 19/16 |
· | Extremely thin keys acting without rotation

|  | E05B 19/18 |
· | Keys adjustable before use

|  | E05B 19/20 |
· | Skeleton keys; Devices for picking locks; Other devices for similar purposes

|  | E05B 19/22 |
· | Keys with devices for indicating whether the last operation was locking or unlocking

|  | E05B 19/24 |
· | Key-distinguishing marks

|  | E05B 19/26 |
· | Use of special materials for keys

|  | E05B 21/00 - E05B 25/00 |
Locks with rotary keys moving lamelliform tumblers perpendicular to the key

|  | E05B 21/00 |
Locks with tumblers not following the movement of the bolt

|  | E05B 21/02 |
· | with identical tumblers

|  | E05B 21/04 |
· | with stop pins on the tumbler (Fulltext... Hierarchy... Expanded...E05B 21/02 takes precedence)

|  | E05B 21/06 |
· | Cylinder locks, e.g. protector locks

|  | E05B 23/00 |
Locks with tumblers following the movement of the bolt

|  | E05B 25/00 |
Locks with special tumblers

|  | E05B 25/02 |
· | with tumblers in the cut-out of which the key bit is moved

|  | E05B 25/04 |
· | with tumblers in which the stop pin is guided from one locked position to the other in an inclined direction

|  | E05B 25/06 |
· | with tumblers in which the stop pin is guided from one locked position to the other along a curved path

|  | E05B 25/08 |
· | with tumblers with movable pawls engaging the key

|  | E05B 25/10 |
· | with tumblers formed to engage one another to determine their unlocked position

|  | E05B 27/00 - E05B 33/00 |
Locks of which the tumblers are set by pushing the key in

|  | E05B 27/00 |
Cylinder locks with tumbler pins or balls

|  | E05B 27/02 |
· | operated by the edge of the key

|  | E05B 27/04 |
· · | arranged radially in one row

|  | E05B 27/06 |
· · | arranged radially in more than one row

|  | E05B 27/08 |
· · | arranged axially

|  | E05B 27/10 |
· | operated by other surfaces of the key, e.g. openings receiving projections on the tumblers

|  | E05B 29/00 |
Cylinder locks with plate tumblers

|  | E05B 29/02 |
· | operated by the edge of the key

|  | E05B 29/04 |
· · | arranged singly

|  | E05B 29/06 |
· · | arranged in pairs

|  | E05B 29/08 |
· | operated by other surfaces of the key

|  | E05B 29/10 |
· · | operated by a curved groove or slot

|  | E05B 29/12 |
· · | operated by a curved rib

|  | E05B 29/14 |
· | with both axially and radially arranged plate tumblers

|  | E05B 31/00 |
Cylinder locks with both tumbler pins or balls and plate tumblers

|  | E05B 33/00 |
Cylinder locks in which the bolt is moved by means other than the key

|  | E05B 35/00 |
Locks for use with special keys or a plurality of keys

|  | E05B 35/02 |
· | which can be shifted laterally

|  | E05B 35/04 |
· | for pull keys

|  | E05B 35/06 |
· | for screw keys

|  | E05B 35/08 |
· | operable by a plurality of keys

|  | E05B 35/10 |
· · | with master and pass keys

|  | E05B 35/12 |
· · | requiring the use of two keys, e.g. safe-deposit locks

|  | E05B 35/14 |
· | with keys of which different parts operate separate mechanisms

|  | E05B 37/00 |
Permutation locks (electric permutation locks Fulltext... Hierarchy... Expanded...E05B 49/00; for bicycles Fulltext... Hierarchy... Expanded...E05B 71/02); Puzzle locks

|  | E05B 37/02 |
· | with tumbler discs or rings arranged on a single axis, each disc being adjustable independently of the others

|  | E05B 37/04 |
· | with tumbler discs on a single axis, all the discs being adjustable by rotating a shiftable knob

|  | E05B 37/06 |
· · | in padlocks

|  | E05B 37/08 |
· | with tumbler discs on a single axis, all the discs being adjustable by a rotary knob which is not shifted

|  | E05B 37/10 |
· · | in padlocks

|  | E05B 37/12 |
· | with tumbler discs on several axes

|  | E05B 37/14 |
· · | in padlocks

|  | E05B 37/16 |
· | with two or more push or pull knobs, slides, or the like

|  | E05B 37/18 |
· · | in padlocks

|  | E05B 37/20 |
· | Puzzle locks

|  | E05B 37/22 |
· · | in padlocks

|  | E05B 39/00 - E05B 45/00 |
Locks with indicating or timing devices

|  | E05B 39/00 |
Locks giving indication of unauthorised unlocking

|  | E05B 39/02 |
· | with destructible seal closures or paper closures

|  | E05B 39/04 |
· | with counting or registering devices

|  | E05B 41/00 |
Locks with visible indication as to whether the lock is locked or unlocked

|  | E05B 43/00 |
Time locks (clocks or clock mechanisms with attached or built-in means operating any device at preselected times or after a predetermined time interval Fulltext... Hierarchy... Expanded...G04C 23/00)

|  | E05B 45/00 |
Alarm locks (alarm devices actuated by tampering with fastenings in general Fulltext... Hierarchy... Expanded...G08B)

|  | E05B 45/02 |
· | with mechanically-operated bells

|  | E05B 45/04 |
· | with detonating alarm devices

|  | E05B 45/06 |
· | Electric alarm locks

|  | E05B 45/08 |
· · | with contact making inside the lock or in the striking plate

|  | E05B 45/10 |
· · · | by introducing the key

|  | E05B 45/12 |
· · · | by movement of the bolt

|  | E05B 45/14 |
· · | with contact making outside the lock

|  | E05B 47/00 - E05B 51/00 |
Operation or control of locks by non-mechanical means, e.g. from a distance (locking doors simultaneously in passenger vehicles Fulltext... Hierarchy... Expanded...E05B 65/36; key switches Fulltext... Hierarchy... Expanded...H01H 27/00)

|  | E05B 47/00 |
Operating or controlling locks or other fastening devices by electric or magnetic means (electric permutation locks Fulltext... Hierarchy... Expanded...E05B 49/00; holding in open position or limiting movement of wings by magnetic or electromagnetic attraction Fulltext... Hierarchy... Expanded...E05C 17/56) [2]

|  | E05B 47/02 |
· | Adaptation of locks, latches, or parts thereof, for movement of the bolt by electromagnetic means

|  | E05B 47/04 |
· · | for unlocking only

|  | E05B 47/06 |
· | Controlling mechanically-operated bolts by electromagnetically-operated detents

|  | E05B 47/08 |
· · | the bolt being withdrawn by a spring which is stressed by closing the wing

|  | E05B 49/00 |
Electric permutation locks; Circuits therefor

|  | E05B 49/02 |
· | with electrical arrangements inside the lock

|  | E05B 49/04 |
· | with electrical arrangements outside the lock

|  | E05B 51/00 |
Operating or controlling locks or other fastening devices by other non-mechanical means

|  | E05B 51/02 |
· | by pneumatic or hydraulic means

|  | E05B 53/00 |
Operation or control of locks by mechanical transmissions, e.g. from a distance (for passenger vehicles Fulltext... Hierarchy... Expanded...E05B 65/20)

|  | E05B 55/00 - E05B 61/00 |
Locks with provision for latching (for passenger vehicle doors Fulltext... Hierarchy... Expanded...E05B 65/20)

|  | E05B 55/00 |
Locks in which a sliding latch is used also as a locking bolt

|  | E05B 55/02 |
· | the bolt being secured by the tumbler

|  | E05B 55/04 |
· | the bolt being secured by the cross-bar or the turnbuckle and the handle being locked

|  | E05B 55/06 |
· | the handle being disconnected

|  | E05B 55/08 |
· · | the bolt being secured by transverse bolts

|  | E05B 55/10 |
· · | without securing the bolt

|  | E05B 55/12 |
· | the bolt being secured by the operation of a hidden parallel member

|  | E05B 55/14 |
· | the bolt being secured by the operation of a wing handle, or by means in the wing handle or knob

|  | E05B 55/16 |
· · | merely by normal use of the handle on one side of the wing

|  | E05B 57/00 |
Locks in which a pivoted latch is used also as locking means

|  | E05B 59/00 |
Locks with latches separate from the lock-bolts, or with a plurality of latches or lock-bolts

|  | E05B 59/02 |
· | with arrangements for securing the latch while shooting the lock-bolt

|  | E05B 59/04 |
· | Locks in which the latch is moved by a lock-bolt, or the lock-bolt by a latch, or one latch by another, etc.

|  | E05B 59/06 |
· | with a lock-bolt slidable in the latch

|  | E05B 61/00 |
Other locks with provision for latching

|  | E05B 63/00 - E05B 67/00 |
Locks with special structural characteristics or for special use

|  | E05B 63/00 |
Locks with special structural characteristics

|  | E05B 63/02 |
· | without springs

|  | E05B 63/04 |
· | for alternative use on the right-hand or left-hand side of wings

|  | E05B 63/06 |
· | with lengthwise-adjustable bolts

|  | E05B 63/08 |
· | Mortise locks

|  | E05B 63/10 |
· · | requiring only two cylindrical holes in the wing

|  | E05B 63/12 |
· | with means carried by the bolt for interlocking with the keeper (for passenger vehicle doors Fulltext... Hierarchy... Expanded...E05B 65/28)

|  | E05B 63/14 |
· | Arrangement of several locks or locks with several bolts, e.g. arranged one behind the other (locks for keys with several bits Fulltext... Hierarchy... Expanded...E05B 35/14; with provision for latching Fulltext... Hierarchy... Expanded...E05B 59/00, Fulltext... Hierarchy... Expanded...E05B 61/00)

|  | E05B 63/16 |
· | with the handles on opposite sides moving independently (the latch being secured by the operation of a wing handle Fulltext... Hierarchy... Expanded...E05B 55/14)

|  | E05B 63/18 |
· | with arrangements independent of the locking mechanism for retaining the bolt in the retracted position

|  | E05B 63/20 |
· · | released automatically when the wing is closed

|  | E05B 63/22 |
· | operated by a pulling or pushing action perpendicular to the front plate (Fulltext... Hierarchy... Expanded...E05B 35/04 takes precedence)

|  | E05B 65/00 |
Locks for special use

|  | E05B 65/02 |
· | for thin, hollow, or thin-metal wings

|  | E05B 65/04 |
· | for wings one behind the other hinged on the same side

|  | E05B 65/06 |
· | for swing doors

|  | E05B 65/08 |
· | for sliding wings

|  | E05B 65/10 |
· | for panic or emergency doors

|  | E05B 65/12 |
· | for vehicles (Fulltext... Hierarchy... Expanded...E05B 71/00 takes precedence) [2]

|  | E05B 65/14 |
· · | for railway freight-cars or the like; for lorries (for front doors of road vehicles Fulltext... Hierarchy... Expanded...E05B 65/20)

|  | E05B 65/16 |
· · · | for back doors of vans

|  | E05B 65/18 |
· · · | with provision for sealing

|  | E05B 65/19 |
· · | for car-boot lids; for car bonnets

|  | E05B 65/20 |
· · | for passenger or like doors (bolt-fastenings per se Fulltext... Hierarchy... Expanded...E05C)

|  | E05B 65/22 |
· · · | with rectilinearly-moving bolt

|  | E05B 65/24 |
· · · · | locked by a special movement of the door handle

|  | E05B 65/26 |
· · · · | with the outside door handle drawn into a recess when the door is locked

|  | E05B 65/28 |
· · · · | with means carried by the bolt for interlocking with the keeper

|  | E05B 65/30 |
· · · · | with two or more bolts moved simultaneously

|  | E05B 65/32 |
· · · | with the bolt turning about an axis

|  | E05B 65/34 |
· · · · | in which the member engaging the keeper is shaped as a lockable toothed wheel or the like

|  | E05B 65/36 |
· · · | Locking several doors simultaneously

|  | E05B 65/38 |
· · · · | by pneumatic or hydraulic means

|  | E05B 65/40 |
· · · | Locking one door by shutting another (by non-mechanical means Fulltext... Hierarchy... Expanded...E05B 47/00, Fulltext... Hierarchy... Expanded...E05B 51/00; fastenings, other than locks, for double doors Fulltext... Hierarchy... Expanded...E05C 7/06; operating fastenings, other than locks, by mechanical transmission Fulltext... Hierarchy... Expanded...E05C 13/04)

|  | E05B 65/42 |
· · · | Securing the latch or bolt by movement of the vehicle

|  | E05B 65/44 |
· | for furniture or drawers

|  | E05B 65/46 |
· · | Special locks for drawers, e.g. for a plurality of drawers (mechanisms for securing one drawer by closing another Fulltext... Hierarchy... Expanded...E05C 15/04)

|  | E05B 65/48 |
· | Hasp locks

|  | E05B 65/50 |
· · | for briefcases

|  | E05B 65/52 |
· | Other locks for chests, boxes, trunks, baskets, travelling bags, etc. (closures for bags or trunks Fulltext... Hierarchy... Expanded...A45C 13/06, Fulltext... Hierarchy... Expanded...A45C 13/10, Fulltext... Hierarchy... Expanded...A45C 13/16)

|  | E05B 67/00 |
Padlocks (permutation locks Fulltext... Hierarchy... Expanded...E05B 37/00); Details thereof

|  | E05B 67/02 |
· | Cases

|  | E05B 67/04 |
· · | Armoured cases

|  | E05B 67/06 |
· | Shackles; Arrangement of the shackle

|  | E05B 67/08 |
· · | Padlocks with shackles hinged on the case

|  | E05B 67/10 |
· · · | with devices for securing the free end of the shackle

|  | E05B 67/12 |
· · · · | with built-in cylinder locks

|  | E05B 67/14 |
· · · | with devices for securing the hinged end of the shackle

|  | E05B 67/16 |
· · · · | with built-in cylinder locks

|  | E05B 67/18 |
· · · | with devices for securing both ends of the shackle

|  | E05B 67/20 |
· · · · | with built-in cylinder locks

|  | E05B 67/22 |
· · | Padlocks with sliding shackles, with or without rotary or pivotal movement

|  | E05B 67/24 |
· · · | with built-in cylinder locks

|  | E05B 67/26 |
· · · | with screw action, with or without the shackle being moved by turning the key

|  | E05B 67/28 |
· · | Padlocks with shackles forming a circle

|  | E05B 67/30 |
· · · | with built-in cylinder locks

|  | E05B 67/32 |
· · | Padlocks with pincer-like shackles

|  | E05B 67/34 |
· · · | with built-in cylinder locks

|  | E05B 67/36 |
· | Padlocks with closing means other than shackles

|  | E05B 67/38 |
· | Auxiliary or protective devices

|  | E05B 69/00 - E05B 73/00 |
Locking devices for clothing, sticks, umbrellas, or cycles

|  | E05B 69/00 |
Devices for locking clothing; Lockable clothing holders or hangers (clothing holders without locking devices Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...A47G 25/00-A47G 25/10)

|  | E05B 69/02 |
· | Lockable clothing hooks (coin-controlled locking hooks Fulltext... Hierarchy... Expanded...G07F)

|  | E05B 71/00 |
Locks specially adapted for bicycles, other than padlocks (locks integral with cycles Fulltext... Hierarchy... Expanded...B62H 5/00)

|  | E05B 71/02 |
· | with permutation locking devices

|  | E05B 73/00 |
Devices for locking portable objects against unauthorised removal; Miscellaneous locking devices

|  | E05B 73/02 |
· | for walking-sticks or umbrellas (stick or umbrella holders in general Fulltext... Hierarchy... Expanded...A47G 25/12)

|  | E05B 75/00 |
Handcuffs