|  | F |
SECTION F — MECHANICAL ENGINEERING; LIGHTING; HEATING; WEAPONS; BLASTING

LIGHTING AND HEATING

|  | F23 |
COMBUSTION APPARATUS; COMBUSTION PROCESSES

|  | F23 |
Note(s) In this class, the following terms are used with the meanings indicated: "Combustion" means the direct combination of oxygen gas, e.g. in air, and a burnable substance. Any other heat-producing combination of chemical substances, e.g. hydrogen peroxide and methane, iron oxide and aluminium, is provided for in Section C or in sub-class Fulltext... Hierarchy... Expanded...F24J. "Combustion chamber" means a chamber in which fuel is burned to establish a self-supporting fire or flame and which surrounds that fire or flame. "Burner" means a device by which fluent fuel is passed to a combustion space where it burns to produce a self-supporting flame. "Air" means a mixture of gases containing free oxygen and able to promote or support combustion.

|  | F23L |
AIR SUPPLY; DRAUGHT-INDUCING; SUPPLYING NON-COMBUSTIBLE LIQUID OR GAS (air-supply arrangements for fluent fuels Fulltext... Hierarchy... Expanded...F23C; dampers and throat restrictors for open fire-places Fulltext... Hierarchy... Expanded...F24; air inlet valves for open fire fronts Fulltext... Hierarchy... Expanded...F24)

|  | F23L 1/00 |
Passages or apertures for delivering primary air for combustion

|  | F23L 1/02 |
· | by discharging the air below the fire

|  | F23L 3/00 |
Arrangements of valves or dampers before the fire

|  | F23L 5/00 |
Blast-producing apparatus before the fire

|  | F23L 5/02 |
· | Arrangements of fans or blowers (fans or blowers per se Fulltext... Hierarchy... Expanded...F04)

|  | F23L 5/04 |
· | by induction of air for combustion, e.g. using steam jet

|  | F23L 7/00 |
Supplying non-combustible liquids or gases, other than air, to the fire, e.g. oxygen, steam

|  | F23L 9/00 |
Passages or apertures for delivering secondary air for completing combustion of fuel

|  | F23L 9/02 |
· | by discharging the air above the fire

|  | F23L 9/04 |
· | by discharging the air beyond the fire, i.e. nearer the smoke outlet

|  | F23L 9/06 |
· | by discharging the air into the fire bed

|  | F23L 11/00 |
Arrangements of valves or dampers after the fire

|  | F23L 11/02 |
· | for reducing draught by admission of air to flues

|  | F23L 13/00 |
Construction of valves or dampers for controlling air supply or draught (in general Fulltext... Hierarchy... Expanded...F16K)

|  | F23L 13/02 |
· | pivoted about a single axis but having no other movement (formed as linked slats each pivoted about an axis Fulltext... Hierarchy... Expanded...F23L 13/08)

|  | F23L 13/04 |
· · | with axis perpendicular to face

|  | F23L 13/06 |
· | slidable only

|  | F23L 13/08 |
· | operating as a roller blind; operating as a venetian blind

|  | F23L 13/10 |
· | having a compound movement involving both sliding and pivoting

|  | F23L 15/00 |
Heating of air supplied for combustion

|  | F23L 15/02 |
· | Arrangements of regenerators

|  | F23L 15/04 |
· | Arrangements of recuperators

|  | F23L 17/00 |
Inducing draught

|  | F23L 17/02 |
· | Tops for chimneys or ventilating shafts; Terminals for flues

|  | F23L 17/04 |
· · | Balanced-flue arrangements, i.e. devices which combine air inlet to combustion unit with smoke outlet

|  | F23L 17/06 |
· · | branched; T-headed

|  | F23L 17/08 |
· · | with coaxial cones or louvres

|  | F23L 17/10 |
· · | wherein the top moves as a whole

|  | F23L 17/12 |
· · | Devices for fastening the top or terminal to chimney, shaft, or flue

|  | F23L 17/14 |
· · | Draining devices

|  | F23L 17/16 |
· | Induction apparatus, e.g. steam jet, acting on combustion products beyond the fire