|  | E |
SECTION E — FIXED CONSTRUCTIONS

BUILDING

|  | E05 |
LOCKS; KEYS; WINDOW OR DOOR FITTINGS; SAFES

|  | E05 |
Note(s) In this class, the following terms are used with the meanings indicated: "Wing" is a general term for swingable, slidable, or otherwise movable doors or windows. The term also encompasses other movable structures such as drawers, lids of chests, car boots, or car bonnets, to which the operating, mounting, latching, or locking means of this class may be applied. "Frame" means any member to which a wing may be held by a fastening device. It does not include a framework forming part of the wing, but it may be another wing. "Lock" means primarily a device for releasing or securing any member, which requires a key or a permutation mechanism for release. "Bolt" means a sliding, pivoted, or otherwise movable member such as is normally carried by a door to hold it shut by engagement with a keeper on the frame. It may be operated by hand directly or through mechanism or by a key; it may be a latch (see (e) below.) "Latch" means a bolt arranged to be moved to the releasing position against the force of a spring, or some other returning force, when a wing meets the frame on closing, so that it does not have to be operated by hand to secure the wing, but only to open it. "Hasp" means a member hinged to the frame or wing so that it can be moved towards the face of the wing or frame and secured thereto, e.g. by a turn-button, by a padlock and staple.

|  | E05F |
DEVICES FOR MOVING WINGS INTO OPEN OR CLOSED POSITION; CHECKS FOR WINGS; WING FITTINGS NOT OTHERWISE PROVIDED FOR, CONCERNED WITH THE FUNCTIONING OF THE WING

|  | E05F 1/00 |
Closers or openers for wings, not otherwise provided for in this sub-class

|  | E05F 1/02 |
· | gravity-actuated

|  | E05F 1/04 |
· · | for wings which lift during movement

|  | E05F 1/06 |
· · · | Mechanisms in the shape of hinges or pivots, operated by the weight of the wing

|  | E05F 1/08 |
· | spring-actuated

|  | E05F 1/10 |
· · | for swinging wings

|  | E05F 1/12 |
· · · | Mechanisms in the shape of hinges or pivots, operated by springs

|  | E05F 1/14 |
· · · | with double-acting springs, e.g. for closing and opening or checking and closing

|  | E05F 3/00 |
Closers or openers with braking devices, e.g. checks; Construction of pneumatic or liquid braking devices (construction of non-pneumatic or non-liquid braking devices Fulltext... Hierarchy... Expanded...E05F 5/00; friction devices in hinges Fulltext... Hierarchy... Expanded...E05D 11/08)

|  | E05F 3/02 |
· | with pneumatic piston brakes (rotary type Fulltext... Hierarchy... Expanded...E05F 3/14)

|  | E05F 3/04 |
· | with liquid piston brakes (rotary type Fulltext... Hierarchy... Expanded...E05F 3/14)

|  | E05F 3/06 |
· · | in which a torsion spring rotates a member around an axis perpendicular to the axis of the piston

|  | E05F 3/08 |
· · | in which a torsion spring rotates a member around an axis arranged in the direction of the axis of the piston

|  | E05F 3/10 |
· · | with a spring, other than a torsion spring, and a piston, the axes of which are the same or lie in the same direction

|  | E05F 3/12 |
· · | Special devices controlling the circulation of the liquid, e.g. valve arrangement (valves per se Fulltext... Hierarchy... Expanded...F16K)

|  | E05F 3/14 |
· | with fluid brakes of the rotary type

|  | E05F 3/16 |
· | with friction brakes

|  | E05F 3/18 |
· | with counteracting springs (double-acting springs Fulltext... Hierarchy... Expanded...E05F 1/14)

|  | E05F 3/20 |
· | in hinges

|  | E05F 3/22 |
· | Additional arrangements for closers, e.g. for holding the wing in opened or other position

|  | E05F 5/00 |
Braking devices, e.g. checks; Spring-actuated devices having only a small effect on the motion of the wing, e.g. assisting operation by hand; Stops; Buffers (construction of pneumatic or liquid braking devices Fulltext... Hierarchy... Expanded...E05F 3/00; devices for limiting opening by a movable member extending between the fixed frame and the wing Fulltext... Hierarchy... Expanded...E05C 17/04)

|  | E05F 5/02 |
· | specially for preventing the slamming of wings

|  | E05F 5/04 |
· · | hand-operated; operated by centrifugal action

|  | E05F 5/06 |
· | Buffers (Fulltext... Hierarchy... Expanded...E05F 5/02 takes precedence)

|  | E05F 5/08 |
· · | with springs

|  | E05F 5/10 |
· · | with piston brakes

|  | E05F 5/12 |
· | specially for preventing the closing of a wing before another wing has been closed

|  | E05F 5/14 |
· | with provision for holding the wing in one ore more opened positions, with or without arrangements for limiting the opening movement of the wing, e.g. for vehicle doors

|  | E05F 7/00 |
Miscellaneous accessories for wings (specially adapted for furniture Fulltext... Hierarchy... Expanded...A47B 95/00; door-lifters Fulltext... Hierarchy... Expanded...A47H 33/02; knobs or handles Fulltext... Hierarchy... Expanded...E05B) [2]

|  | E05F 7/02 |
· | for raising wings before being turned

|  | E05F 7/04 |
· | Arrangements affording protection against rattling (with buffering action Fulltext... Hierarchy... Expanded...E05F 5/00)

|  | E05F 7/06 |
· | Devices for taking the weight of the wing, arranged away from the hinge axis

|  | E05F 7/08 |
· | Special means for transmitting movements between vertical and horizontal sliding bars, rods, or cables (in general Fulltext... Hierarchy... Expanded...F16)

|  | E05F 9/00 - E05F 17/00 |
Operating mechanisms for wings (for safeguarding bank teller windows Fulltext... Hierarchy... Expanded...E05G 5/00; for interconnected louvres Fulltext... Hierarchy... Expanded...E06B 7/086; for blinds or roll-type closures Fulltext... Hierarchy... Expanded...E06B 9/00)

|  | E05F 9/00 |
Means for operating wings by hand rods not guided in or on the frame, including those which also operate the fastening (fastening devices not specially modified for operation by detachable rods Fulltext... Hierarchy... Expanded...E05C)

|  | E05F 11/00 |
Man-operated mechanisms for operating wings, including those which also operate the fastening (connecting mechanisms for a plurality of wings Fulltext... Hierarchy... Expanded...E05F 17/00)

|  | E05F 11/02 |
· | for wings in general, e.g. fanlights (Fulltext... Hierarchy... Expanded...E05F 11/36 takes precedence; for windows to be lowered vertically Fulltext... Hierarchy... Expanded...E05F 11/38; for doors Fulltext... Hierarchy... Expanded...E05F 11/54)

|  | E05F 11/04 |
· · | with cords, chains, or cables

|  | E05F 11/06 |
· · · | in guide-channels

|  | E05F 11/08 |
· · | with longitudinally-moving bars guided, e.g. by pivoted links, in or on the frame

|  | E05F 11/10 |
· · · | Mechanisms by which a handle moves the bar

|  | E05F 11/12 |
· · · | Mechanisms by which the bar shifts the wing

|  | E05F 11/14 |
· · · · | directly, i.e. without links, shifting the wing, e.g. by rack-and-gear or pin-and-slot

|  | E05F 11/16 |
· · · · | shifting the wing by pivotally-connected members in a plane perpendicular to the pivot axis of the wing

|  | E05F 11/18 |
· · · · · | consisting of a lever, e.g. an angle lever, only

|  | E05F 11/20 |
· · · · · | consisting of a lever, e.g. an angle lever, and only one additional link

|  | E05F 11/22 |
· · · · · | consisting of a lever, e.g. an angle lever, and two or more additional links in series

|  | E05F 11/24 |
· · · · | shifting the wing by pivotally-connected members in a plane parallel to the pivot axis of the wing

|  | E05F 11/26 |
· · · · · | consisting of a lever, e.g. an angle lever, only

|  | E05F 11/28 |
· · · · · | consisting of a lever, e.g. an angle lever, and one or more additional links

|  | E05F 11/30 |
· · · · · | consisting of links in rhomb form

|  | E05F 11/32 |
· · | with rotary bars guided in the frame (Fulltext... Hierarchy... Expanded...E05F 11/34 takes precedence)

|  | E05F 11/34 |
· · | with screw mechanisms

|  | E05F 11/36 |
· | specially designed for passing through a wall

|  | E05F 11/38 |
· | for sliding windows, e.g. vehicle windows, to be opened or closed by vertical movement

|  | E05F 11/40 |
· · | operated by screw mechanism

|  | E05F 11/42 |
· · | operated by rack bars and toothed wheels

|  | E05F 11/44 |
· · | operated by one or more lifting arms

|  | E05F 11/46 |
· · | operated by lazy-tongs mechanism

|  | E05F 11/48 |
· · | operated by cords or chains

|  | E05F 11/50 |
· · | Crank gear with clutches or retaining brakes, for operating window mechanisms

|  | E05F 11/52 |
· · | combined with means for producing an additional movement, e.g. a horizontal or a rotary movement

|  | E05F 11/53 |
· | for sliding windows, e.g. vehicle windows, to be opened or closed by horizontal movement [2]

|  | E05F 11/54 |
· | for doors

|  | E05F 13/00 |
Mechanisms operated by the movement or weight of a person or vehicle (through power-operated wing-operating mechanisms Fulltext... Hierarchy... Expanded...E05F 15/00)

|  | E05F 13/02 |
· | by devices, e.g. lever arms, affected by the movement of the user

|  | E05F 13/04 |
· | by platforms lowered by the weight of the user

|  | E05F 15/00 |
Power-operated mechanisms for wings

|  | E05F 15/02 |
· | with pressure medium

|  | E05F 15/04 |
· · | for swinging wings

|  | E05F 15/06 |
· · | for horizontally-sliding wings

|  | E05F 15/08 |
· · | for vertically-sliding wings

|  | E05F 15/10 |
· | with rotary electromotors

|  | E05F 15/12 |
· · | for swinging wings

|  | E05F 15/14 |
· · | for horizontally-sliding wings

|  | E05F 15/16 |
· · | for vertically-sliding wings

|  | E05F 15/18 |
· | with other electrical means, e.g. solenoids

|  | E05F 15/20 |
· | controlled by automatically-acting means, e.g. by photocells, by electric waves, by thermostats, by rain, by fire

|  | E05F 17/00 |
Special devices for shifting a plurality of wings operated simultaneously (for simultaneously moving a plurality of interconnected ventilating lamellae Fulltext... Hierarchy... Expanded...E06B 7/086) [2]