|  | F |
SECTION F — MECHANICAL ENGINEERING; LIGHTING; HEATING; WEAPONS; BLASTING

WEAPONS; BLASTING

|  | F41 |
WEAPONS

|  | F41 |
Note(s) In this class, the following terms are used with the meanings indicated: "Semi-automatic firearm" — a firearm from which one shot is fired after actuation of the trigger and which then returns to a condition for firing a subsequent shot upon renewed actuation of the trigger. "Automatic gun" — a gun which will continue firing so long as the initial firing pressure is maintained on the trigger. "Sighting" — bringing into visual coincidence a direction defined by a so-called "sighting" device with the direction of a target. "Aiming" — bringing a weapon to a direction differing from the sighting direction by corrections in order that the projectile may hit the target. "Laying" — setting a weapon in the correct position for hitting a mark. (not applicable in English). Although simulators are generally in class Fulltext... Hierarchy... Expanded...G09, provision is included in class Fulltext... Hierarchy... Expanded...F41 for means for practice and training which may have aspects of simulation, e.g. in apparatus for so-called "military games".

|  | F41J |
TARGETS; TARGET RANGES; BULLET CATCHERS

|  | F41J 1/00 |
Stationary targets (for arrows or darts Fulltext... Hierarchy... Expanded...F41J 3/00)

|  | F41J 1/02 |
· | adapted for weapons employed, e.g. for pistols

|  | F41J 1/04 |
· · | for rifles

|  | F41J 1/06 |
· · | for automatic-firing weapons

|  | F41J 1/08 |
· · | for guns; for cannons

|  | F41J 1/10 |
· | Target stands; Target holders

|  | F41J 1/12 |
· | Bullet catchers; Bullet traps

|  | F41J 1/14 |
· · | combined with targets

|  | F41J 1/16 |
· | Target-hit indicators or recorders, e.g. manual

|  | F41J 1/18 |
· | Target ranges

|  | F41J 1/20 |
· · | Safety means therefor

|  | F41J 3/00 |
Targets for arrows or darts, e.g. for sporting or amusement purposes

|  | F41J 3/02 |
· | Indicators or score boards for arrow or dart games

|  | F41J 5/00 |
Target-indicating systems

|  | F41J 5/02 |
· | Photo-electric hit-detector systems

|  | F41J 5/04 |
· | Electric hit-indicating systems

|  | F41J 5/06 |
· | Sound hit-indicating systems

|  | F41J 5/08 |
· | Infra-red hit-indicating systems

|  | F41J 5/10 |
· | Cinematographic hit-indicating systems (cinematographic targets Fulltext... Hierarchy... Expanded...F41J 9/14)

|  | F41J 5/12 |
· | for indicating the distance by which a bullet misses the target

|  | F41J 7/00 |
Movable targets which are stationary when fired at

|  | F41J 7/02 |
· | movable for checking

|  | F41J 7/04 |
· | disappearing when hit

|  | F41J 9/00 |
Moving targets, i.e. moving when fired at

|  | F41J 9/02 |
· | Land-based targets

|  | F41J 9/04 |
· | Sea-going targets

|  | F41J 9/06 |
· · | towed

|  | F41J 9/08 |
· | Airborne targets, e.g. drones, kites, balloons

|  | F41J 9/10 |
· · | towed

|  | F41J 9/12 |
· | Radar-reflector targets, e.g. foil strips; Active targets transmitting electromagnetic waves

|  | F41J 9/13 |
· · | Active targets transmitting infra-red radiation [3]

|  | F41J 9/14 |
· | Cinematographic targets, e.g. moving-picture targets

|  | F41J 9/16 |
· | Clay-pigeon targets; Clay-disc targets

|  | F41J 9/18 |
· · | Traps or throwing-apparatus therefor

|  | F41J 9/20 |
· · · | with spring-operated throwing arm [3]

|  | F41J 9/22 |
· · · · | cocked by manual action [3]

|  | F41J 9/24 |
· · · · | cocked by electromechanical means [3]

|  | F41J 9/26 |
· · · | operated by fluid means [3]

|  | F41J 9/28 |
· · · | operated by manual action [3]

|  | F41J 9/30 |
· · · | characterised by using a magazine of targets [3]

|  | F41J 9/32 |
· · · | characterised by means for obviating the anticipation of the flight path [3]