|  | E |
SECTION E — FIXED CONSTRUCTIONS

EARTH DRILLING; MINING

|  | E21 |
EARTH DRILLING; MINING

|  | E21 |
Note(s) In this class, the term "drilling" covers "boring" and vice versa.

|  | E21C |
MINING OR QUARRYING

|  | E21C |
Note(s) This sub-class covers methods or apparatus specific to mining or quarrying. [3] Even though disclosed only for mining or quarrying, drill bits, bore reamers, core taking devices, drilling pipes or rods, handling, racking or connecting arrangements for drilling pipes or rods, counterboring or enlarging drilled holes, flame drilling, or other drilling apparatus not provided for in this sub-class, are covered by sub-class Fulltext... Hierarchy... Expanded...E21B. [3]

|  | E21C 1/00 - E21C 3/00 |
Drilling machines

|  | E21C 1/00 |
Rotary-drilling machines (rotary-drilling machines in general Fulltext... Hierarchy... Expanded...B23B; rotary earth drilling Fulltext... Hierarchy... Expanded...E21B 3/00; driving of shafts, galleries or tunnels Fulltext... Hierarchy... Expanded...E21D)

|  | E21C 1/02 |
· | with a continuous rotation of the tool, with or without variable speed gearing

|  | E21C 1/04 |
· · | with slipping or elastic transmission

|  | E21C 1/06 |
· | with a to-and-fro rotation of the tool

|  | E21C 1/08 |
· | with an intermittent unidirectional rotation of the tool

|  | E21C 1/10 |
· | with a built-in feeding device (feeding devices Fulltext... Hierarchy... Expanded...E21C 5/00)

|  | E21C 1/12 |
· | with percussive action superimposed on a continuously-rotating tool always in contact with the working face

|  | E21C 1/14 |
( transferred to Fulltext... Hierarchy... Expanded...E21B, covered by Fulltext... Hierarchy... Expanded...E21C 1/00 )

|  | E21C 3/00 |
Drilling machines with reciprocating tool that is intermittently turned when out of contact with the working face (portable percussion tools in general Fulltext... Hierarchy... Expanded...B25D)

|  | E21C 3/02 |
· | Machines in which the tool is connected to an impulse member

|  | E21C 3/04 |
· | Hammer drilling machines in which the tool is hit by an impulse member

|  | E21C 3/06 |
· | Means for driving the impulse member

|  | E21C 3/08 |
· · | by a rotating mechanism

|  | E21C 3/10 |
· · · | formed as centrifugal hammers

|  | E21C 3/12 |
· · · | with spring-mounted reciprocating masses

|  | E21C 3/14 |
· · · · | with elastic joining of the drive to the push-rod by double buffer springs

|  | E21C 3/16 |
· · | by electromagnets

|  | E21C 3/18 |
· · | directly by a piston of an internal-combustion engine

|  | E21C 3/20 |
· · | directly by liquid pressure

|  | E21C 3/22 |
· · · | working with pulses

|  | E21C 3/24 |
· · | directly by air, steam, or gas pressure

|  | E21C 3/26 |
· · · | working with pulses

|  | E21C 3/28 |
· | Intermittent turning of tool obtained by rifled-bar or ratchet device

|  | E21C 3/30 |
· · | driven by separate motor

|  | E21C 3/32 |
· | with arrangements for automatic stopping when the tool is lifted from the working face or suffers excessive bore resistance (pick hammers Fulltext... Hierarchy... Expanded...E21C 37/24)

|  | E21C 3/34 |
· | Arrangements for locking the drill to the hammer or to the machine

|  | E21C 5/00 - E21C 11/00 |
Details of drilling apparatus

|  | E21C 5/00 |
Devices for feeding tool to working face (feeding devices for metal-boring machines Fulltext... Hierarchy... Expanded...B23B)

|  | E21C 5/02 |
· | Screw-and-nut feed mechanism

|  | E21C 5/04 |
· | Cam, rack, or like feed mechanism

|  | E21C 5/06 |
· | Flexible drawing means, e.g. cables

|  | E21C 5/08 |
· | Means for driving feed mechanism

|  | E21C 5/10 |
· · | Separate motor, e.g. compressed-air motor or cylinder (Fulltext... Hierarchy... Expanded...E21C 5/11 takes precedence)

|  | E21C 5/11 |
· · | combined with supporting means, e.g. feed legs

|  | E21C 5/12 |
· · | Weight or spring drive

|  | E21C 5/14 |
· · | Automatic feed by jump or recoil of the drilling machine

|  | E21C 5/16 |
· | with arrangements for automatically interrupting the feed when the tool suffers excessive bore resistance

|  | E21C 7/00 |
Dust eliminating or dust removing while drilling (equipment for preventing the formation of dust by slitting or dislodging machines Fulltext... Hierarchy... Expanded...E21C 35/22; exhausting dust from mines Fulltext... Hierarchy... Expanded...E21F 5/20)

|  | E21C 7/02 |
· | by exhausting dust-loaded air

|  | E21C 7/04 |
· | using exhaust air from the drill motor for blowing-off the dust

|  | E21C 7/06 |
· | by foam

|  | E21C 7/08 |
· | by liquids

|  | E21C 7/10 |
· · | Liquid flushing installations

|  | E21C 7/12 |
· | Preventing exhaust air from the drill motor from blowing-off towards the working face

|  | E21C 9/00 |
Supporting, guiding or centralising devices for boring rods (handling, racking, connecting Fulltext... Hierarchy... Expanded...E21B 19/00)

|  | E21C 11/00 |
Supports or guides for drilling machines; Columns to which the machine is clamped (feed legs Fulltext... Hierarchy... Expanded...E21C 5/11; slitting machines mounted on supports Fulltext... Hierarchy... Expanded...E21C 25/64; guiding, slitting, or dislodging machines Fulltext... Hierarchy... Expanded...E21C 35/08)

|  | E21C 11/02 |
· | Drill wagons (trucks for slitting or dislodging machines Fulltext... Hierarchy... Expanded...E21C 29/24)

|  | E21C 13/00 |
( transferred to Fulltext... Hierarchy... Expanded...E21B 10/00 )

|  | E21C 15/00 |
( transferred to Fulltext... Hierarchy... Expanded...E21B 17/00, Fulltext... Hierarchy... Expanded...E21B 19/00, Fulltext... Hierarchy... Expanded...E21B 21/00 )

|  | E21C 17/00 |
( transferred to Fulltext... Hierarchy... Expanded...E21B 10/00 )

|  | E21C 19/00 |
( transferred to Fulltext... Hierarchy... Expanded...E21B )

|  | E21C 21/00 |
( transferred to Fulltext... Hierarchy... Expanded...E21B 7/14 )

|  | E21C 23/00 |
( transferred to Fulltext... Hierarchy... Expanded...E21B 7/28 )

|  | E21C 25/00 - E21C 39/00 |
Cutting; Slitting; Dislodging

|  | E21C 25/00 |
Cutting machines, i.e. for making slits approximately parallel or perpendicular to the seam (dislodging machines with slitting means Fulltext... Hierarchy... Expanded...E21C 27/02, Fulltext... Hierarchy... Expanded...E21C 27/10, Fulltext... Hierarchy... Expanded...E21C 27/18)

|  | E21C 25/02 |
· | Machines slitting solely by one or more percussive tools moved through the seam

|  | E21C 25/04 |
· · | Cutting crowns or other tools (percussion drill bits Fulltext... Hierarchy... Expanded...E21B 10/36)

|  | E21C 25/06 |
· | Machines slitting solely by one or more cutting rods or cutting drums which rotate, move through the seam, and may or may not reciprocate

|  | E21C 25/08 |
· · | Mountings for the rods or drums

|  | E21C 25/10 |
· · | Rods; Drums; Picks

|  | E21C 25/12 |
· · · | Picks (general features of picks Fulltext... Hierarchy... Expanded...E21C 35/18)

|  | E21C 25/14 |
· · | with equipment for cleaning the slit (associated with cutter chain machines Fulltext... Hierarchy... Expanded...E21C 25/50)

|  | E21C 25/16 |
· | Machines slitting solely by one or more rotating saws, cutting discs, or wheels

|  | E21C 25/18 |
· · | Saws; Discs; Wheels

|  | E21C 25/20 |
· | Machines slitting solely by one or more reciprocating sawing implements or reciprocating cutter chains; Shaker conveyers with cutting means

|  | E21C 25/22 |
· | Machines slitting solely by one or more cutter chains moving unidirectionally along jibs

|  | E21C 25/24 |
· · | with flat jibs only

|  | E21C 25/26 |
· · | with curved jibs only

|  | E21C 25/28 |
· · | Chains or chain guides; Picks for same

|  | E21C 25/30 |
· · · | Chain guides

|  | E21C 25/32 |
· · · · | specially adapted for curved jibs

|  | E21C 25/34 |
· · · | Chains

|  | E21C 25/36 |
· · · · | Couplings for links

|  | E21C 25/38 |
· · · | Picks (general features of picks Fulltext... Hierarchy... Expanded...E21C 35/18)

|  | E21C 25/40 |
· · · · | integral with links of chains

|  | E21C 25/42 |
· · · · | Attachment of the picks to the links of chains

|  | E21C 25/44 |
· · · · · | by wedge or taper

|  | E21C 25/46 |
· · · · · | by resilient means

|  | E21C 25/48 |
· · · · · | by means of screws or pins

|  | E21C 25/50 |
· · | with equipment for cleaning the slit (associated with rotary-rod or rotary-drum machines Fulltext... Hierarchy... Expanded...E21C 25/14)

|  | E21C 25/52 |
· | Machines incorporating two or more of the slitting means according to groups Fulltext... Hierarchy... Expanded...E21C 25/02, Fulltext... Hierarchy... Expanded...E21C 25/06, Fulltext... Hierarchy... Expanded...E21C 25/16, Fulltext... Hierarchy... Expanded...E21C 25/20 and Fulltext... Hierarchy... Expanded...E21C 25/22

|  | E21C 25/54 |
· | Slitting by unguided cutter cables or cutter chains or by unguided tools drawn along the working face by cables or the like (dislodging by planing means Fulltext... Hierarchy... Expanded...E21C 27/32; propulsion by haulage cables Fulltext... Hierarchy... Expanded...E21C 29/14)

|  | E21C 25/56 |
· | Slitting by cutter cables or cutter chains or by tools drawn along the working face by cables or the like, in each case guided parallel to the face, e.g. by a conveyer, by a guide parallel to a conveyer (pressing the conveyer equipped with tools toward the working face Fulltext... Hierarchy... Expanded...E21C 35/14)

|  | E21C 25/58 |
· | Machines slitting by drilling hole on hole

|  | E21C 25/60 |
· | Slitting by jets of water or other liquid

|  | E21C 25/62 |
· | Machines for making slits approximately perpendicular to the seams either level with, or above or below the level of, the machine

|  | E21C 25/64 |
· | Slitting machines guided solely by hand and either carried by hand or mounted on supports (supports or guides for drilling machines Fulltext... Hierarchy... Expanded...E21C 11/00; hand-held power-operated tools Fulltext... Hierarchy... Expanded...E21C 37/22)

|  | E21C 25/66 |
· | Machines for making slits with additional arrangements for drilling

|  | E21C 25/68 |
· | Machines for making slits combined with equipment for removing, e.g. by loading, material won by other means (slitting machines combined with planing means Fulltext... Hierarchy... Expanded...E21C 27/18; removing chippings Fulltext... Hierarchy... Expanded...E21C 35/20)

|  | E21C 27/00 |
Machines which completely free the mineral from the seam

|  | E21C 27/01 |
· | specially adapted for removing overhanging coal

|  | E21C 27/02 |
· | solely by slitting (rods, drums, picks, for same Fulltext... Hierarchy... Expanded...E21C 25/10; saws, discs, wheels Fulltext... Hierarchy... Expanded...E21C 25/18; chains, chain guides, picks, for same Fulltext... Hierarchy... Expanded...E21C 25/28)

|  | E21C 27/04 |
· · | by a single chain guided on a frame with or without auxiliary slitting means

|  | E21C 27/06 |
· · · | with a slewing frame

|  | E21C 27/08 |
· · | with additional means for cutting the mineral into blocks

|  | E21C 27/10 |
· | by both slitting and breaking-down

|  | E21C 27/12 |
· · | breaking-down effected by acting on the vertical face of the mineral, e.g. by percussive tools

|  | E21C 27/14 |
· · | breaking-down effected by force or pressure applied to side of slit, e.g. by wedges (breaking-down by means inserted in boreholes Fulltext... Hierarchy... Expanded...E21C 37/00)

|  | E21C 27/16 |
· · · | with means for both slitting and breaking-down

|  | E21C 27/18 |
· | by both slitting and planing

|  | E21C 27/20 |
· | Mineral freed by means not involving slitting

|  | E21C 27/22 |
· · | by rotary drills with breaking-down means, e.g. wedge-shaped drills

|  | E21C 27/24 |
· · | by milling means acting on the full working face

|  | E21C 27/26 |
· · | by closely adjacent cutter chains acting on the full working face

|  | E21C 27/28 |
· · | by percussive drills with breaking-down means, e.g. wedge-shaped tools

|  | E21C 27/30 |
· · | by jaws, buckets, or scoops that scoop-out the mineral

|  | E21C 27/32 |
· · | by adjustable or non-adjustable planing means with or without loading arrangements (by percussed planing means Fulltext... Hierarchy... Expanded...E21C 27/46)

|  | E21C 27/34 |
· · · | Machine propelled along the working face by cable or chain

|  | E21C 27/35 |
· · · · | Ram-ploughs

|  | E21C 27/36 |
· · · | Machine self-propelled along the working face

|  | E21C 27/38 |
· · · | Machine stationary while planing in an arc

|  | E21C 27/40 |
· · · | Machine and its planing tool making alternative step-wise movements along the working face

|  | E21C 27/42 |
· · · | combined with scraper or collector box

|  | E21C 27/44 |
· · · | Planing knives

|  | E21C 27/46 |
· · | by percussed planing means

|  | E21C 29/00 |
Propulsion of machines for slitting or completely freeing the mineral from the seam

|  | E21C 29/02 |
· | by means on the machine exerting a thrust against fixed supports

|  | E21C 29/04 |
· | by cable or chains

|  | E21C 29/06 |
· · | anchored at one or both ends to the mine working face

|  | E21C 29/08 |
· · · | Anchoring arrangements (for anchoring of conveyers only Fulltext... Hierarchy... Expanded...E21F 13/00)

|  | E21C 29/10 |
· · · | Cable or chain co-operating with a winch or the like on the machine

|  | E21C 29/12 |
· · · | Machines propelled by thrust or pull against a part alternately anchored to, and released from, a cable or chain

|  | E21C 29/14 |
· · | by haulage cable or chain pulling the machine along the working face

|  | E21C 29/16 |
· · · | Winches or other means for pulling cable or chain (winches per se Fulltext... Hierarchy... Expanded...B66D)

|  | E21C 29/18 |
· · · | Coupling and uncoupling machine to cable or chain

|  | E21C 29/20 |
· · | with safety devices operating in the event of breakage of the cable or chain

|  | E21C 29/22 |
· | by wheels, endless tracks, or the like

|  | E21C 29/24 |
· · | Trucks carrying the machine while working

|  | E21C 29/26 |
· · · | with means for adjustably positioning the machine on the truck

|  | E21C 29/28 |
· · · · | adjusting the height of the whole machine

|  | E21C 31/00 |
Driving means incorporated in machines for slitting or completely freeing the mineral from the seam

|  | E21C 31/02 |
· | for cutting or breaking-down devices

|  | E21C 31/04 |
· · | imparting both a rotary and reciprocating motion

|  | E21C 31/06 |
· · | actuated by an endless cable or chain

|  | E21C 31/08 |
· | for adjusting parts of the machines

|  | E21C 31/10 |
· | for slewing parts of the machines

|  | E21C 31/12 |
· | Component parts

|  | E21C 33/00 |
Trucks or other devices for transporting machines for slitting or completely freeing the mineral from the seam

|  | E21C 33/02 |
· | with equipment for loading or unloading the machine on to, or from, the truck

|  | E21C 35/00 |
Miscellaneous items relating to machines for slitting or completely freeing the mineral from the seam

|  | E21C 35/02 |
· | Locking equipment for slewable parts

|  | E21C 35/04 |
· | Safety devices (operating in the event of breakage of a haulage cable or chain Fulltext... Hierarchy... Expanded...E21C 29/20)

|  | E21C 35/06 |
· | Equipment for positioning the whole machine in relation to its sub-structure

|  | E21C 35/08 |
· | Guiding the machine

|  | E21C 35/10 |
· · | by feelers contacting the working face

|  | E21C 35/12 |
· · | along a conveyer for the cut material

|  | E21C 35/14 |
· · · | Equipment for pressing the conveyer towards the working face

|  | E21C 35/16 |
· · | by making use of the timbering, filling, or other supports

|  | E21C 35/18 |
· | General features of picks, e.g. use of special materials (picks for slitting machines Fulltext... Hierarchy... Expanded...E21C 25/12, Fulltext... Hierarchy... Expanded...E21C 25/38)

|  | E21C 35/20 |
· | General features of equipment for removal of chippings, e.g. for loading on conveyer

|  | E21C 35/22 |
· | Equipment for preventing the formation of, or for removal of, dust (removing dust while drilling Fulltext... Hierarchy... Expanded...E21C 7/00)

|  | E21C 35/24 |
· | Remote control specially adapted for machines for slitting or completely freeing the mineral (control in general Fulltext... Hierarchy... Expanded...G05)

|  | E21C 37/00 |
Other methods or devices for dislodging with or without loading (breaking-down by means inserted in slits Fulltext... Hierarchy... Expanded...E21C 27/14)

|  | E21C 37/02 |
· | by wedges

|  | E21C 37/04 |
· | by devices with parts pressed mechanically against the wall of a borehole

|  | E21C 37/06 |
· | by making use of hydraulic or pneumatic pressure in a borehole

|  | E21C 37/08 |
· · | Devices with pistons, plungers, etc. pressed locally against the wall of the borehole

|  | E21C 37/10 |
· · | Devices with expanding elastic casings

|  | E21C 37/12 |
· · | by injecting into the borehole a liquid, either initially at high pressure or subsequently subjected to high pressure, e.g. by pulses, by explosive cartridges acting on the liquid (slitting by jets of water Fulltext... Hierarchy... Expanded...E21C 25/60; blasting by explosives Fulltext... Hierarchy... Expanded...F42D)

|  | E21C 37/14 |
· · | by compressed air; by gas blast; by gasifying liquids

|  | E21C 37/16 |
· | by fire-setting or by similar methods based on a heat effect (drilling by use of heat Fulltext... Hierarchy... Expanded...E21B 7/14)

|  | E21C 37/18 |
· | by electricity

|  | E21C 37/20 |
· | by ultrasonics

|  | E21C 37/22 |
· | Hand tools or hand-held power-operated tools specially adapted for dislodging minerals (slitting machines guided solely by hand Fulltext... Hierarchy... Expanded...E21C 25/64)

|  | E21C 37/24 |
· · | Pick hammers (drilling machines with reciprocating tool Fulltext... Hierarchy... Expanded...E21C 3/00; pneumatic hammers in general Fulltext... Hierarchy... Expanded...B25D)

|  | E21C 37/26 |
· | Chisels or other cutting tools not mentioned before

|  | E21C 39/00 |
Devices for testing in situ the hardness or other properties of minerals, e.g. for giving information as to the selection of suitable mining tools

|  | E21C 41/00 - E21C 51/00 |
Methods of mining or quarrying; Open-pit mining; Layouts therefor

|  | E21C 41/00 |
Methods of mining (Fulltext... Hierarchy... Expanded...E21C 43/00, Fulltext... Hierarchy... Expanded...E21C 45/00 take precedence); Layouts (for peat Fulltext... Hierarchy... Expanded...E21C 49/00)

|  | E21C 41/02 |
· | for brown coal

|  | E21C 41/04 |
· | for hard coal

|  | E21C 41/06 |
· | for ores

|  | E21C 41/08 |
· | for rock salt; for potash salts (obtaining by dissolving out of boreholes Fulltext... Hierarchy... Expanded...E21B 43/28)

|  | E21C 41/10 |
· | for oil-bearing deposits

|  | E21C 41/12 |
· | for stone, e.g. marble

|  | E21C 41/14 |
· | for other specified minerals, e.g. gold, mercury, other heavy metals, sulphur, slate; for clay

|  | E21C 43/00 |
Methods for preparing for the gasification of coal underground (methods for generating gas Fulltext... Hierarchy... Expanded...C10B)

|  | E21C 45/00 |
Methods of mining placers; Hydraulic monitors or other hydraulic machines for obtaining minerals out of alluvial deposits

|  | E21C 47/00 |
Machines for obtaining, or the removal of, materials in open-pit mines (obtaining peat Fulltext... Hierarchy... Expanded...E21C 49/00)

|  | E21C 47/02 |
· | for coal, brown coal, or the like (dredgers or soil-shifting machines per se Fulltext... Hierarchy... Expanded...E02F)

|  | E21C 47/04 |
· · | Conveyer bridges used in co-operation with the winning apparatus

|  | E21C 47/06 |
· · | Cableway conveyers used in co-operation with the winning apparatus (underground hauling Fulltext... Hierarchy... Expanded...E21F 13/00)

|  | E21C 47/08 |
· · | Devices for cutting-out partings, e.g. layers of sand between seams of coal

|  | E21C 47/10 |
· | for quarrying stone, sand, gravel, or clay

|  | E21C 49/00 |
Obtaining peat; Machines therefor (treating peat Fulltext... Hierarchy... Expanded...C10F)

|  | E21C 49/02 |
· | by excavating

|  | E21C 49/04 |
· | by digging in the form of peat sods

|  | E21C 51/00 |
Apparatus for, or methods of, winning materials from extraterrestrial sources (cosmonautics Fulltext... Hierarchy... Expanded...B64G) [2]