|  | B |
SECTION B — PERFORMING OPERATIONS; TRANSPORTING

SEPARATING; MIXING

|  | B01 - B09 |
Note(s) The following notes are meant to assist in the use of this part of the classification scheme; they must not be read as modifying in any way the elaborations. In this sub-section, the separation of different materials, e.g. of different matter, size, or state, is predominantly found in the following subclasses: Fulltext... Hierarchy... Expanded...B01D Fulltext... Hierarchy... Expanded...B03B, Fulltext... Hierarchy... Expanded...B03C, Fulltext... Hierarchy... Expanded...B03D Fulltext... Hierarchy... Expanded...B04B, Fulltext... Hierarchy... Expanded...B04C, Fulltext... Hierarchy... Expanded...B07B, Fulltext... Hierarchy... Expanded...B07C. The classifying characteristics of these subclasses are: the physical state of the matter to be separated; the principle of the process used; particular kinds of apparatus. The first of these characteristics involves six different aspects, assembled in three groups: liquid/liquid or liquid/gas and gas/gas; solid/liquid or solid/gas; solid/solid. These subclasses are to be used according to the following general rules: Fulltext... Hierarchy... Expanded...B01D is the most general class as far as separation other than solids from solids is concerned. Apparatus for separating solids from solids are covered by Fulltext... Hierarchy... Expanded...B03B when the process concerned is regarded as the equivalent of ''washing'' in the sense of the mining art, even if such apparatus is a pneumatic one, especially pneumatic tables or jigs. Screens per se are not covered by this subclass but are classified in Fulltext... Hierarchy... Expanded...B07B, even if they are being used in a wet process. All other apparatus for the separation of solids from solids according to dry methods are classified in Fulltext... Hierarchy... Expanded...B07B. If the separation takes place as a result of the detection or measurement of some feature of the material or articles to be sorted it is classified in Fulltext... Hierarchy... Expanded...B07C. It should also be noted that the separation of isotopes of the same chemical element is covered by Fulltext... Hierarchy... Expanded...B01D 59/00, whatever process or apparatus is employed. The following scheme illustrates the classification according to these rules.

|  | B01 |
PHYSICAL OR CHEMICAL PROCESSES OR APPARATUS IN GENERAL (furnaces, kilns, ovens, retorts, in general Fulltext... Hierarchy... Expanded...F27)

|  | B01B |
BOILING; BOILING APPARATUS

|  | B01B 1/00 |
Boiling; Boiling apparatus for physical or chemical purposes (preparation of starch Fulltext... Hierarchy... Expanded...C08B 30/00; sugar industry Fulltext... Hierarchy... Expanded...C13; steam generation Fulltext... Hierarchy... Expanded...F22; domestic boilers Fulltext... Hierarchy... Expanded...F24) [2]

|  | B01B 1/02 |
· | Preventing foaming (in general Fulltext... Hierarchy... Expanded...B01D 19/02)

|  | B01B 1/04 |
· · | by chemical means

|  | B01B 1/06 |
· | Preventing bumping

|  | B01B 1/08 |
· | Boiling apparatus provided with reflux condenser