|  | B |
SECTION B — PERFORMING OPERATIONS; TRANSPORTING

SEPARATING; MIXING

|  | B01 - B09 |
Note(s) The following notes are meant to assist in the use of this part of the classification scheme; they must not be read as modifying in any way the elaborations. In this sub-section, the separation of different materials, e.g. of different matter, size, or state, is predominantly found in the following subclasses: Fulltext... Hierarchy... Expanded...B01D Fulltext... Hierarchy... Expanded...B03B, Fulltext... Hierarchy... Expanded...B03C, Fulltext... Hierarchy... Expanded...B03D Fulltext... Hierarchy... Expanded...B04B, Fulltext... Hierarchy... Expanded...B04C, Fulltext... Hierarchy... Expanded...B07B, Fulltext... Hierarchy... Expanded...B07C. The classifying characteristics of these subclasses are: the physical state of the matter to be separated; the principle of the process used; particular kinds of apparatus. The first of these characteristics involves six different aspects, assembled in three groups: liquid/liquid or liquid/gas and gas/gas; solid/liquid or solid/gas; solid/solid. These subclasses are to be used according to the following general rules: Fulltext... Hierarchy... Expanded...B01D is the most general class as far as separation other than solids from solids is concerned. Apparatus for separating solids from solids are covered by Fulltext... Hierarchy... Expanded...B03B when the process concerned is regarded as the equivalent of ''washing'' in the sense of the mining art, even if such apparatus is a pneumatic one, especially pneumatic tables or jigs. Screens per se are not covered by this subclass but are classified in Fulltext... Hierarchy... Expanded...B07B, even if they are being used in a wet process. All other apparatus for the separation of solids from solids according to dry methods are classified in Fulltext... Hierarchy... Expanded...B07B. If the separation takes place as a result of the detection or measurement of some feature of the material or articles to be sorted it is classified in Fulltext... Hierarchy... Expanded...B07C. It should also be noted that the separation of isotopes of the same chemical element is covered by Fulltext... Hierarchy... Expanded...B01D 59/00, whatever process or apparatus is employed. The following scheme illustrates the classification according to these rules.

|  | B01 |
PHYSICAL OR CHEMICAL PROCESSES OR APPARATUS IN GENERAL (furnaces, kilns, ovens, retorts, in general Fulltext... Hierarchy... Expanded...F27)

|  | B01B |
BOILING; BOILING APPARATUS

|  | B01D |
SEPARATION (separating solids from solids by wet methods Fulltext... Hierarchy... Expanded...B03B, Fulltext... Hierarchy... Expanded...B03D; by pneumatic jigs or tables Fulltext... Hierarchy... Expanded...B03B; by other dry methods Fulltext... Hierarchy... Expanded...B07; magnetic or electrostatic separation of solid materials from solid materials or fluids, separation by high-voltage electric fields Fulltext... Hierarchy... Expanded...B03C; centrifuges, vortex apparatus Fulltext... Hierarchy... Expanded...B04; presses per se for squeezing-out liquid from liquid-containing material Fulltext... Hierarchy... Expanded...B30B 9/02; treatment of water Fulltext... Hierarchy... Expanded...C02F, e.g. softening by ion-exchange Fulltext... Hierarchy... Expanded...C02F 1/42) [5]

|  | B01D |
Note(s) This subclass covers: evaporation, distillation, crystallisation, filtration, dust precipitation, gas cleaning, absorption, adsorption; similar processes which are not concerned with, or limited to, separation (except in the case of absorption or adsorption). In this subclass, the terms or expressions are used with the meaning indicated: "filtration" and analogous terms include straining solids from fluids; "filter medium" is a porous material or porous arrangement of material used to filter solids from fluids; "filtering element" is a section of filter medium in addition to parts to which the medium is demountably or permanently fixed, including other sections of medium, end caps, peripheral frames or edge strips, but excluding housings; "filter housing" is the fluid-constraining impervious vessel, whether open or closed, which contains, or is adapted to contain, one or more filtering elements or filter media; "filter chamber" is the space within a housing, where filtering elements or filter media are located. Partitions may divide a single housing into a plurality of chambers; "filtering apparatus" consists of filtering elements combined with housings, cleaning arrangements, motor or the like parts, which are characteristic of the particular type of apparatus. Ancillary devices such as pumps or valves are considered part of a filtering apparatus when inside the apparatus. Ancillary devices performing similar or different unit operation such as comminutors, mixers or non-filtering separators, whether or not inside the apparatus, are not considered part of a filtering apparatus. The term does not extend to apparatus, e.g. washing machines, of which the filter forms only a part. For apparatus used in drying or evaporation, class Fulltext... Hierarchy... Expanded...F26 takes precedence over this subclass. Group Fulltext... Hierarchy... Expanded...B01D 59/00 takes precedence over the other groups of this subclass and over other subclasses.

|  | B01F |
MIXING, e.g. DISSOLVING, EMULSIFYING, DISPERSING

|  | B01F |
Note(s) In this subclass, the following term or expression is used with the meaning indicated: "mixing" covers stirring of a single material. [2]

|  | B01J |
CHEMICAL OR PHYSICAL PROCESSES, e.g. CATALYSIS, COLLOID CHEMISTRY; THEIR RELEVANT APPARATUS (processes or apparatus for specific applications, see the relevant places for these processes or apparatus, e.g. Fulltext... Hierarchy... Expanded...F26B 3/08) [2]

|  | B01J |
Note(s) In this subclass, the following terms or expressions are used with the meanings indicated: "solid particles" includes such particles whether catalysts, reactants or inert in solid, semi-solid or pasty state; [2] "fluidised particles" means finely divided solid particles lifted and agitated by a stream of fluid; [2] "fluidised-bed technique" means fluid-solid contacting technique in which finely divided particles are lifted and agitated by a rising stream of fluid, said stream having such a speed as to form a lower dense phase (the "bed") and an upper dilute fluidised phase of "fluidised particles"; [2] "processes conducted in the presence of solid particles" does not include processes wherein the only solid particles present are formed during the reaction. [3]

|  | B01L |
CHEMICAL OR PHYSICAL LABORATORY APPARATUS FOR GENERAL USE (apparatus for medical or pharmaceutical purposes Fulltext... Hierarchy... Expanded...A61; apparatus for industrial purposes or laboratory apparatus whose construction and performance are comparable to that of similar industrial apparatus, see the relevant classes for industrial apparatus, particularly subclasses of Fulltext... Hierarchy... Expanded...B01 and Fulltext... Hierarchy... Expanded...C12; separating or distilling apparatus Fulltext... Hierarchy... Expanded...B01D; mixing or stirring devices Fulltext... Hierarchy... Expanded...B01F; atomisers Fulltext... Hierarchy... Expanded...B05B; sieves Fulltext... Hierarchy... Expanded...B07B; corks, bungs Fulltext... Hierarchy... Expanded...B65D; handling liquids in general Fulltext... Hierarchy... Expanded...B67; vacuum pumps Fulltext... Hierarchy... Expanded...F04; siphons Fulltext... Hierarchy... Expanded...F04F 10/00; taps, stop-cocks Fulltext... Hierarchy... Expanded...F16K; tubes, tube joints Fulltext... Hierarchy... Expanded...F16L; apparatus specially adapted for investigating or analysing materials Fulltext... Hierarchy... Expanded...G01, particularly Fulltext... Hierarchy... Expanded...G01N; electrical or optical apparatus, see the relevant classes in sections G and H)

|  | B01L |
Note(s) This subclass covers only laboratory apparatus which is either applicable solely to laboratory purposes or which, by reason of its simple construction and adaptability, is such as would not be suitable for industrial use.