|  | E |
SECTION E — FIXED CONSTRUCTIONS

BUILDING

|  | E05 |
LOCKS; KEYS; WINDOW OR DOOR FITTINGS; SAFES

|  | E05 |
Note(s) In this class, the following terms are used with the meanings indicated: "wing" is a general term for swingable, slidable, or otherwise movable doors or windows. This term also includes other movable structures such as drawers, lids of chests, car boots, or car bonnets, to which the operating, mounting, latching, or locking means covered by this class may be applied; "frame" means any member to which a wing may be held by a fastening device. It does not include a framework forming part of the wing, but it may be another wing; "lock" means primarily a device for releasing or securing any member, which requires a key or a permutation mechanism for release. In groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...E05B 1/00-E05B 9/00, Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...E05B 13/00-E05B 17/00, Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...E05B 39/00-E05B 47/00, Fulltext... Hierarchy... Expanded...E05B 51/00, Fulltext... Hierarchy... Expanded...E05B 53/00, Fulltext... Hierarchy... Expanded...E05B 63/00 and Fulltext... Hierarchy... Expanded...E05B 65/00 however, the term "lock" may include other fastening devices; "bolt" means a sliding, pivoted, or otherwise movable member such as is normally carried by a door to hold it shut by engagement with a keeper on the frame. It may be operated by hand directly or through mechanism or by a key; it may be a latch (see below); "latch" means a bolt arranged to be moved to the releasing position against the force of a spring, or some other returning force, when a wing meets the frame on closing, so that it does not have to be operated by hand to secure the wing, but only to open it; "hasp" means a member hinged to the frame or wing so that it can be moved towards the face of the wing or frame and secured thereto, e.g. by a turn-button, by a padlock and staple.

|  | E05C |
BOLTS OR FASTENING DEVICES FOR WINGS, SPECIALLY FOR DOORS OR WINDOWS (latching means for sideboard or tailgate structures for vehicles Fulltext... Hierarchy... Expanded...B62D 33/037; fastening devices for constructional or engineering elements Fulltext... Hierarchy... Expanded...E04, Fulltext... Hierarchy... Expanded...F16B; locks, fastening devices structurally or operatively combined or having significant cooperation with locks Fulltext... Hierarchy... Expanded...E05B; means for operating or controlling wing fasteners in conjunction with mechanisms for moving the wing Fulltext... Hierarchy... Expanded...E05F)

|  | E05C |
Note(s) In this subclass, only the movement essential for securing the wing is considered, e.g. a sliding bolt which is rotated on its axis to prevent its withdrawal is classified as having only a sliding movement. Attention is drawn to the definitions following the title of class Fulltext... Hierarchy... Expanded...E05.

|  | E05C |
Subclass index
FASTENING DEVICES |
characterised by the way the bolt is moved | 1/00 - 5/00
specially for holding wings open | 17/00, 19/00
specially adapted for two wings | 7/00
ARRANGEMENT OF FASTENING, SECURING, OR LOCKING DEVICES | 9/00, 21/00

|  | E05C 1/00 - E05C 5/00 |
Bolts, latches, or equivalent wing-fastening devices, characterised by special way of movement, e.g. moving rectilinearly, pivotally, or rotatively (devices released automatically by pull or pressure on the wing Fulltext... Hierarchy... Expanded...E05C 19/02; hasps Fulltext... Hierarchy... Expanded...E05C 19/08; hook fastenings Fulltext... Hierarchy... Expanded...E05C 19/10)

|  | E05C 1/00 |
Fastening devices with bolts moving rectilinearly

|  | E05C 1/02 |
· | without latching action

|  | E05C 1/04 |
· · | with operating handle or equivalent member rigid with the bolt

|  | E05C 1/06 |
· · | with operating handle or equivalent member moving otherwise than rigidly with the bolt

|  | E05C 1/08 |
· | with latching action

|  | E05C 1/10 |
· · | with operating handle or equivalent member rigid with the latch

|  | E05C 1/12 |
· · | with operating handle or equivalent member moving otherwise than rigidly with the latch

|  | E05C 1/14 |
· · · | the handle or member moving essentially towards, or away from, the plane of the wing or frame

|  | E05C 1/16 |
· · · | the handle or member moving essentially in a plane substantially parallel to the wing

|  | E05C 3/00 |
Fastening devices with bolts moving pivotally or rotatively

|  | E05C 3/02 |
· | without latching action

|  | E05C 3/04 |
· · | with operating handle or equivalent member rigid with the bolt

|  | E05C 3/06 |
· · | with operating handle or equivalent member moving otherwise than rigidly with the bolt

|  | E05C 3/08 |
· · · | the handle or member moving essentially towards, or away from, the plane of the wing or frame

|  | E05C 3/10 |
· · · | the handle or member moving essentially in a plane substantially parallel to the wing

|  | E05C 3/12 |
· | with latching action (devices in which the securing part is formed or merely carried by a spring and moves only by distortion of the spring, e.g. snaps, Fulltext... Hierarchy... Expanded...E05C 19/06)

|  | E05C 3/14 |
· · | with operating handle or equivalent member rigid with the latch

|  | E05C 3/16 |
· · | with operating handle or equivalent member moving otherwise than rigidly with the latch

|  | E05C 3/22 |
· · · | the bolt being spring-controlled

|  | E05C 3/24 |
· · · · | in the form of a bifurcated member

|  | E05C 3/26 |
· · · · · | engaging a stud-like keeper

|  | E05C 3/28 |
· · · · · · | with simultaneously-operating double bolts

|  | E05C 3/30 |
· · · · | in the form of a hook

|  | E05C 3/32 |
· · · · · | engaging a hooked keeper (Fulltext... Hierarchy... Expanded...E05C 3/34 takes precedence)

|  | E05C 3/34 |
· · · · · | with simultaneously-operating double bolts

|  | E05C 3/36 |
· · · · | in the form of a rotary gear

|  | E05C 3/38 |
· · · · | with bolts engaging a hooked keeper (Fulltext... Hierarchy... Expanded...E05C 3/24, Fulltext... Hierarchy... Expanded...E05C 3/30, Fulltext... Hierarchy... Expanded...E05C 3/36 take precedence)

|  | E05C 3/40 |
· · · · | with bolts engaging a stud-like keeper (Fulltext... Hierarchy... Expanded...E05C 3/24, Fulltext... Hierarchy... Expanded...E05C 3/30, Fulltext... Hierarchy... Expanded...E05C 3/36 take precedence)

|  | E05C 5/00 |
Fastening devices with bolts moving otherwise than only rectilinearly and only pivotally or rotatively

|  | E05C 5/02 |
· | both moving axially and turning about their axes to secure the wing

|  | E05C 5/04 |
· · | performing both movements simultaneously, e.g. screwing into a keeper

|  | E05C 7/00 |
Fastening devices specially adapted for two wings

|  | E05C 7/00 |
Note(s) In this group, if a fastening device merely secures one wing to another wing which is already closed it is not regarded as specially adapted for two wings.

|  | E05C 7/02 |
· | for wings which lie one behind the other when closed

|  | E05C 7/04 |
· | for wings which abut when closed

|  | E05C 7/06 |
· · | a fastening device for one wing being actuated or controlled by closing another wing

|  | E05C 9/00 |
Arrangement of simultaneously-actuated bolts or other securing devices at well-separated positions on the same wing (essentially involving locking means Fulltext... Hierarchy... Expanded...E05B 63/14; similar constructions for engineering closures for pressure vessels, in general Fulltext... Hierarchy... Expanded...F16J 13/08)

|  | E05C 9/02 |
· | with one sliding bar for fastening when moved in one direction and unfastening when moved in opposite direction; with two sliding bars moved in the same direction when fastening or unfastening [4]

|  | E05C 9/04 |
· | with two sliding bars moved in opposite directions when fastening or unfastening

|  | E05C 9/06 |
· | with three or more sliding bars

|  | E05C 9/08 |
· | with a rotary bar for actuating the fastening means

|  | E05C 9/10 |
· | Actuating mechanisms for bars

|  | E05C 9/12 |
· · | with gears and racks

|  | E05C 9/14 |
· · | with pins engaging slots

|  | E05C 9/16 |
· · | with crank pins and connecting rods

|  | E05C 9/18 |
· | Details of fastening means or of fixed retaining means for the ends of bars

|  | E05C 9/20 |
· | Coupling means for sliding bars, rods, or cables [4]

|  | E05C 9/22 |
· | Guides for sliding bars, rods, or cables (corner guides Fulltext... Hierarchy... Expanded...E05C 9/24) [4]

|  | E05C 9/24 |
· | Means for transmitting movements between vertical and horizontal sliding bars, rods, or cables, e.g. corner guides (means for transmitting movements between vertical and horizontal sliding bars, rods, or cables, for moving wings into open or closed position Fulltext... Hierarchy... Expanded...E05F 7/08) [4]

|  | E05C 17/00 |
Devices for holding wings open; Devices for limiting opening of wings or for holding wings open by a movable member extending between frame and wing; Braking devices, stops or buffers, combined therewith (combined with hinges Fulltext... Hierarchy... Expanded...E05D 11/00; combined with operating apparatus for wings Fulltext... Hierarchy... Expanded...E05F; other braking devices, stops, buffers Fulltext... Hierarchy... Expanded...E05F 5/00) [4]

|  | E05C 17/02 |
· | by mechanical means (Fulltext... Hierarchy... Expanded...E05C 17/60 takes precedence) [4]

|  | E05C 17/04 |
· · | with a movable bar or equivalent member extending between frame and wing

|  | E05C 17/06 |
· · · | releasable to allow further opening only when the wing is nearly closed

|  | E05C 17/08 |
· · · | with special means for release, e.g. automatic release by further opening

|  | E05C 17/10 |
· · · | incorporating a special device for securing the wing in the closed position

|  | E05C 17/12 |
· · · | consisting of a single rod

|  | E05C 17/14 |
· · · · | Hook and eye, or equivalent

|  | E05C 17/16 |
· · · · | pivoted only at one end and having an elongated slot

|  | E05C 17/18 |
· · · · | pivoted only at one end and having a row of holes, notches, or pins

|  | E05C 17/20 |
· · · · | sliding through a guide (Fulltext... Hierarchy... Expanded...E05C 17/18 takes precedence)

|  | E05C 17/22 |
· · · · · | with braking, clamping or securing means in the guide [4]

|  | E05C 17/24 |
· · · · | pivoted at one end, and with the other end running along a guide member

|  | E05C 17/26 |
· · · · · | with braking, clamping or securing means at the pivot of the rod [4]

|  | E05C 17/28 |
· · · · · | with braking, clamping or securing means at the connection to the guide member [4]

|  | E05C 17/30 |
· · · | of extensible, e.g. telescopic, construction (flexible members Fulltext... Hierarchy... Expanded...E05C 17/36)

|  | E05C 17/32 |
· · · | consisting of two or more pivoted rods

|  | E05C 17/34 |
· · · · | with means for holding in more than one position

|  | E05C 17/36 |
· · · | comprising a flexible member, e.g. chains

|  | E05C 17/38 |
· · | with a curved rail rigid with the frame for engagement with means on the wing, or vice versa

|  | E05C 17/40 |
· · | Bars or like parts connecting a right wing with a left wing which move against each other when being closed

|  | E05C 17/42 |
· · | connecting exterior and interior wings

|  | E05C 17/44 |
· · | with a device carried on the wing for frictional or like engagement with a fixed flat surface, e.g. retractable feet

|  | E05C 17/46 |
· · | in which the wing or a member fixed thereon is engaged by a movable fastening member in a fixed position; in which a movable fastening member mounted on the wing engages a stationary member [4]

|  | E05C 17/48 |
· · · | comprising a sliding securing member

|  | E05C 17/50 |
· · · | comprising a single pivoted securing member

|  | E05C 17/52 |
· · · | comprising a snap, catch, or the like

|  | E05C 17/54 |
· · | Portable devices, e.g. wedges

|  | E05C 17/56 |
· | by magnetic or electromagnetic attraction (operation of locks or fasteners by electric or magnetic means Fulltext... Hierarchy... Expanded...E05B 47/00) [2]

|  | E05C 17/58 |
· | operated or controlled from a distance

|  | E05C 17/60 |
· | holding sliding wings open [4]

|  | E05C 17/62 |
· · | using notches [4]

|  | E05C 17/64 |
· · | by friction [4]

|  | E05C 19/00 |
Other devices specially designed for securing wings (movable draft sealings additionally used for bolting Fulltext... Hierarchy... Expanded...E06B 7/18) [2]

|  | E05C 19/02 |
· | Automatic catches, i.e. released by pull or pressure on the wing (Fulltext... Hierarchy... Expanded...E05C 19/06 takes precedence)

|  | E05C 19/04 |
· · | Ball or roller catches

|  | E05C 19/06 |
· | in which the securing part is formed or carried by a spring and moves only by distortion of the spring, e.g. snaps

|  | E05C 19/08 |
· | Hasps; Hasp fastenings; Spring catches therefor

|  | E05C 19/10 |
· | Hook fastenings; Fastenings in which a link engages a fixed hook-like member

|  | E05C 19/12 |
· · | pivotally mounted

|  | E05C 19/14 |
· · · | with toggle action

|  | E05C 19/16 |
· | Devices holding the wing by magnetic or electromagnetic attraction

|  | E05C 19/18 |
· | Portable devices specially adapted for securing wings (preventing operation of handles Fulltext... Hierarchy... Expanded...E05B 13/00)

|  | E05C 21/00 |
Arrangement or combinations of wing fastening, securing, or holding devices, not covered by a single preceding main group

|  | E05C 21/02 |
· | for holding a wing closed only