|  | E |
SECTION E — FIXED CONSTRUCTIONS

BUILDING

|  | E05 |
LOCKS; KEYS; WINDOW OR DOOR FITTINGS; SAFES

|  | E05 |
Note(s) In this class, the following terms are used with the meanings indicated: "wing" is a general term for swingable, slidable, or otherwise movable doors or windows. This term also includes other movable structures such as drawers, lids of chests, car boots, or car bonnets, to which the operating, mounting, latching, or locking means covered by this class may be applied; "frame" means any member to which a wing may be held by a fastening device. It does not include a framework forming part of the wing, but it may be another wing; "lock" means primarily a device for releasing or securing any member, which requires a key or a permutation mechanism for release. In groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...E05B 1/00-E05B 9/00, Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...E05B 13/00-E05B 17/00, Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...E05B 39/00-E05B 47/00, Fulltext... Hierarchy... Expanded...E05B 51/00, Fulltext... Hierarchy... Expanded...E05B 53/00, Fulltext... Hierarchy... Expanded...E05B 63/00 and Fulltext... Hierarchy... Expanded...E05B 65/00 however, the term "lock" may include other fastening devices; "bolt" means a sliding, pivoted, or otherwise movable member such as is normally carried by a door to hold it shut by engagement with a keeper on the frame. It may be operated by hand directly or through mechanism or by a key; it may be a latch (see below); "latch" means a bolt arranged to be moved to the releasing position against the force of a spring, or some other returning force, when a wing meets the frame on closing, so that it does not have to be operated by hand to secure the wing, but only to open it; "hasp" means a member hinged to the frame or wing so that it can be moved towards the face of the wing or frame and secured thereto, e.g. by a turn-button, by a padlock and staple.

|  | E05G |
SAFES OR STRONG-ROOMS FOR VALUABLES; BANK PROTECTION DEVICES; SAFETY TRANSACTION PARTITIONS (alarm arrangements per se Fulltext... Hierarchy... Expanded...G08B) [2]

|  | E05G |
Note(s) In this subclass, the following terms or expressions are used with the meanings indicated: "bank" is a building or portion of a building devoted to the safekeeping or exchange of valuables between the "bank" and its customers; [2] "bank protection device" is a mechanism in or on a bank for protecting the valuables or repelling attacks by stealth or force. [2]

|  | E05G 1/00 |
Safes or strong-rooms for valuables (savings boxes Fulltext... Hierarchy... Expanded...A45C 1/12; floatable safes Fulltext... Hierarchy... Expanded...B63C 7/30; storage containers without attack or fire repellent features Fulltext... Hierarchy... Expanded...B65D; bank buildings in general, e.g. modular construction, floor plan, Fulltext... Hierarchy... Expanded...E04H 1/06; buildings resistant to earthquake or war action Fulltext... Hierarchy... Expanded...E04H 9/00)

|  | E05G 1/02 |
· | Details (safe hinges Fulltext... Hierarchy... Expanded...E05D 7/14)

|  | E05G 1/024 |
· · | Wall or panel structure [2]

|  | E05G 1/026 |
· · | Closures (protective doors, windows, or like closures against air-raid or other war-like action Fulltext... Hierarchy... Expanded...E06B 5/10; shutters, movable grilles, other safety closures Fulltext... Hierarchy... Expanded...E06B 9/02) [2]

|  | E05G 1/04 |
· · | Closure fasteners (locks Fulltext... Hierarchy... Expanded...E05B)

|  | E05G 1/06 |
· | having provision for multiple compartments [2]

|  | E05G 1/08 |
· · | secured individually [2]

|  | E05G 1/10 |
· | with alarm, signal, or indicator (burglar, theft, or intruder alarm per se Fulltext... Hierarchy... Expanded...G08B 13/00; fire or explosion alarm per se Fulltext... Hierarchy... Expanded...G08B 17/00) [2]

|  | E05G 1/12 |
· | with fluent-material releasing, generating, or distributing means, e.g. repellent or fire extinguishing (Fulltext... Hierarchy... Expanded...E05G 1/14 takes precedence; identifying, scaring or incapacitating burglars, thieves, or intruders with smoke, gas, powder, or liquid Fulltext... Hierarchy... Expanded...G08B 15/02) [2,6]

|  | E05G 1/14 |
· | with means for marking or destroying the valuables, e.g. in case of theft [6]

|  | E05G 5/00 |
Bank protection devices (Fulltext... Hierarchy... Expanded...E05G 1/12, Fulltext... Hierarchy... Expanded...E05G 7/00 take precedence; closed-circuit television systems Fulltext... Hierarchy... Expanded...H04N 7/18) [2]

|  | E05G 5/02 |
· | Trapping or confining mechanisms (thief or burglar incapacitating means in general Fulltext... Hierarchy... Expanded...G08B 15/00) [2]

|  | E05G 7/00 |
Safety transaction partitions, e.g. movable payplates (non-safety paying counters, e.g. for supermarkets, Fulltext... Hierarchy... Expanded...A47F 9/02) [2]