|  | H |
SECTION H — ELECTRICITY

|  | H |
Note(s) These Notes cover the basic principles and general instructions for use of section H. Section H covers: basic electric elements, which cover all electric units and the general mechanical structure of apparatus and circuits, including the assembly of various basic elements into what are called printed circuits and also cover to a certain extent the manufacture of these elements (when not covered elsewhere); generation of electricity, which covers the generation, conversion and distribution of electricity together with the controlling of the corresponding gear; applied electricity, which covers: general utilisation techniques, viz. those of electric heating and electric lighting circuits; some special utilisation techniques, either electric or electronic in the strict sense, which are not covered by other sections of the Classification, including: electric light sources, including lasers; electric X-ray technique; electric plasma technique and the generation and acceleration of electrically charged particles or neutrons; basic electronic circuits and their control; radio or electric communication technique; the use of a specified material for the manufacture of the article or element described. In this connection, paragraphs 57 to 59 of the Guide should be referred to. In this section, the following general rules apply: Subject to the exceptions stated in I(c), above, any electric aspect or part peculiar to a particular operation, process, apparatus, object or article, classified in one of the sections of the Classification other than section H, is always classified in the subclass for that operation, process, apparatus, object or article. Where common characteristics concerning technical subjects of similar nature have been brought out at class level, the electric aspect or part is classified, in conjunction with the operation, process, apparatus, object or article, in a subclass which covers entirely the general electrical applications for the technical subject in question; The electrical applications referred to under (a), above, either general or particular, include: the therapeutic processes and apparatus, in class Fulltext... Hierarchy... Expanded...A61; the electric processes and apparatus used in various laboratory or industrial operations, in classes Fulltext... Hierarchy... Expanded...B01 and Fulltext... Hierarchy... Expanded...B03 and in subclass Fulltext... Hierarchy... Expanded...B23K; the electricity supply, electric propulsion and electric lighting of vehicles in general and of particular vehicles, in the subsection "Transporting" of section B; the electric ignition systems of internal-combustion engines, in subclass Fulltext... Hierarchy... Expanded...F02P, and of combustion apparatus in general, in subclass Fulltext... Hierarchy... Expanded...F23Q; the whole electrical part of section G, i.e. measuring devices including apparatus for measuring electric variables, checking, signalling and calculating. Electricity in that section is generally dealt with as a means and not as an end in itself; All electrical applications, both general and particular, presuppose that the "basic electricity" aspect appears in section H (see I(a), above) as regards the electric "basic elements" which they comprise. This rule is also valid for applied electricity, referred to in I(c), above, which appears in section H itself. In this section, the following special cases occur: Among the general applications covered by sections other than section H, it is worth noting that electric heating in general is covered by subclasses Fulltext... Hierarchy... Expanded...F24D or Fulltext... Hierarchy... Expanded...F24H or class Fulltext... Hierarchy... Expanded...F27, and that electric lighting in general is partly covered by class Fulltext... Hierarchy... Expanded...F21, since in section H (see I(c), above) there are places in Fulltext... Hierarchy... Expanded...H05B which cover the same technical subjects; In the two cases referred to under (a), above, the subclasses of section F, which deal with the respective subjects, essentially cover in the first place the whole mechanical aspect of the apparatus or devices, whereas the electrical aspect, as such, is covered by subclass Fulltext... Hierarchy... Expanded...H05B; In the case of lighting, this mechanical aspect should be taken to cover the material arrangement of the various electric elements, i.e., their geometrical or physical position in relation to one another; this aspect is covered by subclass Fulltext... Hierarchy... Expanded...F21V, the elements themselves and the primary circuits remaining in section H. The same applies to electric light sources, when combined with light sources of a different kind. These are covered by subclass Fulltext... Hierarchy... Expanded...H05B, whereas the physical arrangement which their combination constitutes is covered by the various subclasses of class Fulltext... Hierarchy... Expanded...F21; As regards heating, not only the electric elements and circuitry designs, as such, are covered by subclass Fulltext... Hierarchy... Expanded...H05B, but also the electric aspects of their arrangement, where these concern cases of general application; electric furnaces being considered as such. The physical disposition of the electric elements in furnaces is covered by section F. If a comparison is made with electric welding circuits, which are covered by subclass Fulltext... Hierarchy... Expanded...B23K in connection with welding, it can be seen that electric heating is not covered by the general rule stated in II, above.

|  | H01 |
BASIC ELECTRIC ELEMENTS

|  | H01 |
Note(s) Processes involving only a single technical art, e.g. drying, coating, for which provision exists elsewhere are classified in the relevant class for that art.

|  | H01H |
ELECTRIC SWITCHES; RELAYS; SELECTORS; EMERGENCY PROTECTIVE DEVICES (contact cables Fulltext... Hierarchy... Expanded...H01B 7/10; overvoltage protection resistors, resistive arresters Fulltext... Hierarchy... Expanded...H01C 7/12, Fulltext... Hierarchy... Expanded...H01C 8/04; electrolytic self-interrupters Fulltext... Hierarchy... Expanded...H01G 9/18; switching devices of the waveguide type Fulltext... Hierarchy... Expanded...H01P; devices for interrupted current collection Fulltext... Hierarchy... Expanded...H01R 39/00; overvoltage arresters using spark gaps Fulltext... Hierarchy... Expanded...H01T 4/00; emergency protective circuit arrangements Fulltext... Hierarchy... Expanded...H02H; switching by electronic means without contact-making Fulltext... Hierarchy... Expanded...H03K 17/00)

|  | H01H |
Note(s) This subclass covers (in groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 69/00-H01H 87/00) devices for the protection of electric lines or electric machines or apparatus in the event of undesired change from normal electric working conditions, the electrical condition serving directly as the input to the device. This subclass does not cover bases, casings, or covers accommodating two or more switching devices or for accomodating a switching device as well as another electric component, e.g. bus-bar, line connector. Those bases, casings or covers are covered by group Fulltext... Hierarchy... Expanded...H02B 1/26. In this subclass, the following terms or expressions are used with the meanings indicated: "relay" means a switching device having contacts which are operated from electric inputs which supply, directly or indirectly, all the mechanical energy necessary to cause both the closure and the opening of the contacts; "driving mechanism" refers to the means by which an operating force applied to the switch is transmitted to the moving contact or contacts; "operating" is used in a broader sense than "actuating" which is reserved for those parts not touched by hand to effect switching; "acting" or "action" means a self-induced movements of parts at one stage of the switching. These connotations apply to all parts of the verbs "to operate"; "to actuate", and "to act", and to words derived therefrom, e.g. to "actuation". In this subclass, details are classified as follows: details of an unspecified type of switching device, or disclosed as applicable to two or more kinds of switching devices designated by the terms or expressions "switches", "relays", "selector switches", and "emergency protective devices", are classified in groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 1/00-H01H 9/00; details of an unspecified type of switch, or disclosed as applicable to two or more types of switches as defined by groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 13/00-H01H 43/00 and subgroups Fulltext... Hierarchy... Expanded...H01H 35/02, Fulltext... Hierarchy... Expanded...H01H 35/06, Fulltext... Hierarchy... Expanded...H01H 35/14, Fulltext... Hierarchy... Expanded...H01H 35/18, Fulltext... Hierarchy... Expanded...H01H 35/24, and Fulltext... Hierarchy... Expanded...H01H 35/42, all hereinafter called basic types, are classified in groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 1/00-H01H 9/00; details of an unspecified type of relay, or disclosed as applicable to two or more types of relays as defined by groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 51/00-H01H 61/00, hereinafter called basic types, are classified in group Fulltext... Hierarchy... Expanded...H01H 45/00; details of an unspecified protective device, or applicable to two or more types of protective devices as defined by groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 73/00-H01H 83/00, hereinafter called basic types, are classified in group Fulltext... Hierarchy... Expanded...H01H 71/00. However, details only described with reference to, or clearly only applicable to, switching devices of a single basic type, are classified in the group appropriate to switching devices of that basic type, e.g. Fulltext... Hierarchy... Expanded...H01H 19/02, Fulltext... Hierarchy... Expanded...H01H 75/04; mechanical structural details of control members of switches or of keyboards such as keys, push-buttons, levers or other mechanisms for transferring the force to the activated elements are classified in this subclass, even when they are used for controlling electronic switches. However, mechanical details directly producing electronic effects are classified in group Fulltext... Hierarchy... Expanded...H03K 17/94. [4]

|  | H01H |
Subclass index
ELECTRIC SWITCHES |
Characterised by the principle of control |
mechanical |
rectilinearly movable: one direction; two directions | 13/00; 15/00
with angular displacement: unlimited angle; limited angle | 19/00; 21/00
by pulling; by tumbling | 17/00; 23/00
with compound movements | 25/00
by removable members | 27/00
physical |
general; electric or magnetic field; heat; explosion | 35/00; 36/00; 37/00; 39/00
Characterised by the contacts |
liquid | 29/00
Characterised by the voltage or the intensity |
without arc-extinguishing means; with such means | 31/00; 33/00
Characterised by the actuation duration |
manual; programme | 41/00; 43/00
Manufacture | 11/00
RELAYS |
Electromagnetic; dynamo-electric; magnetostrictive | 51/00; 53/00; 55/00
Electrostrictive or piezo-electric; electrostatic; electrothermal | 57/00; 59/00; 61/00
Details |
general; electromechanical; circuits | 45/00; 50/00; 47/00
Manufacture | 49/00
SELECTORS |
Types | 67/00
Details | 63/00
Manufacture | 65/00
SECTIONALISERS |
low-tension with blade-type contact | 21/54
for high tension | 31/00
combined with fuses | 85/54
PROTECTIVE DEVICES |
Circuit-breaking switches |
with resetting: manual; by motor; separate | 73/00; 75/00; 77/00
Protective switches |
by short-circuit; opening and closing; particular | 79/00; 81/00; 83/00
Fuses; evaporation devices | 85/00; 87/00
Details of protective switches and relays | 71/00
Manufacture | 69/00
GENERAL DETAILS |
Contacts | 1/00
Mechanisms |
operating contacts in general; snap-action; delay | 3/00; 5/00; 7/00
Other details | 9/00

|  | H01H 1/00 - H01H 43/00 |
Electric switches

|  | H01H 1/00 |
Contacts (liquid contacts Fulltext... Hierarchy... Expanded...H01H 29/04)

|  | H01H 1/02 |
· | characterised by the material thereof

|  | H01H 1/04 |
· · | Co-operating contacts of different material

|  | H01H 1/06 |
· | characterised by the shape or structure of the contact-making surface, e.g. grooved

|  | H01H 1/08 |
· · | wetted with mercury

|  | H01H 1/10 |
· · | Laminated contacts with divided contact surface

|  | H01H 1/12 |
· | characterised by the manner in which co-operating contacts engage

|  | H01H 1/14 |
· · | by abutting

|  | H01H 1/16 |
· · · | by rolling; by wrapping; Roller or ball contacts

|  | H01H 1/18 |
· · · | with subsequent sliding

|  | H01H 1/20 |
· · · | Bridging contacts

|  | H01H 1/22 |
· · · | with rigid pivoted member carring the moving contact

|  | H01H 1/24 |
· · · | with resilient mounting

|  | H01H 1/26 |
· · · · | with spring blade support

|  | H01H 1/28 |
· · · · · | Assembly of three or more contact-supporting spring blades

|  | H01H 1/30 |
· · · · | within supporting guides

|  | H01H 1/32 |
· · · | Self-aligning contacts

|  | H01H 1/34 |
· · · | with provision for adjusting position of contact relative to its co-operating contact

|  | H01H 1/36 |
· · | by sliding (by rolling or wrapping Fulltext... Hierarchy... Expanded...H01H 1/16)

|  | H01H 1/38 |
· · · | Plug-and-socket contacts

|  | H01H 1/40 |
· · · | Contact mounted so that its contact-making surface is flush with adjoining insulation

|  | H01H 1/42 |
· · · | Knife-and-clip contacts

|  | H01H 1/44 |
· · · | with resilient mounting

|  | H01H 1/46 |
· · · | self-aligning contacts

|  | H01H 1/48 |
· · · | with provision for adjusting position of contact relative to its co-operating contact

|  | H01H 1/50 |
· | Means for increasing contact pressure, preventing vibration of contacts, holding contacts together after engagement, or biasing contacts to the open position

|  | H01H 1/52 |
· · | Contacts adapted to act as latches

|  | H01H 1/54 |
· · | by magnetic force

|  | H01H 1/56 |
· | Contact arrangements for providing make-before-break operation, e.g. for on-load tap-changing

|  | H01H 1/58 |
· | Electric connections to or between contacts; Terminals (electric connections in general Fulltext... Hierarchy... Expanded...H01R)

|  | H01H 1/60 |
· | Auxiliary means structurally associated with the switch for cleaning or lubricating contact-making surfaces (cleaning by normal sliding of contacts Fulltext... Hierarchy... Expanded...H01H 1/18, Fulltext... Hierarchy... Expanded...H01H 1/36)

|  | H01H 1/62 |
· | Heating or cooling of contacts

|  | H01H 1/64 |
· | Protective enclosures, baffle plates, or screens for contacts (for arc-extinguishing Fulltext... Hierarchy... Expanded...H01H 9/30; for mercury contacts Fulltext... Hierarchy... Expanded...H01H 29/04)

|  | H01H 1/66 |
· · | Contacts sealed in an evacuated or gas-filled envelope, e.g. magnetic dry-reed contacts

|  | H01H 3/00 |
Mechanisms for operating contacts (snap-action arrangements Fulltext... Hierarchy... Expanded...H01H 5/00; devices for introducing a predetermined time delay Fulltext... Hierarchy... Expanded...H01H 7/00; thermal actuating or release means Fulltext... Hierarchy... Expanded...H01H 37/02)

|  | H01H 3/02 |
· | Operating parts, i.e. for operating driving mechanism by a mechanical force external to the switch

|  | H01H 3/04 |
· · | Levers (tumblers Fulltext... Hierarchy... Expanded...H01H 23/14)

|  | H01H 3/06 |
· · · | Means for securing to shaft of driving mechanism

|  | H01H 3/08 |
· · | Turn knobs

|  | H01H 3/10 |
· · · | Means for securing to shaft of driving mechanism

|  | H01H 3/12 |
· · | Push-buttons

|  | H01H 3/14 |
· · | adapted for operation by a part of the human body other than the hand, e.g. by foot

|  | H01H 3/16 |
· · | adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. for a door switch, a limit switch, a floor-levelling switch of a lift

|  | H01H 3/18 |
· · · | the movement in one direction being intentionally by hand, e.g. for setting automatically cancelled trafficators

|  | H01H 3/20 |
· · | wherein an auxiliary movement thereof, or of an attachment thereto, is necessary before the main movement is possible or effective, e.g. for unlatching, for coupling

|  | H01H 3/22 |
· | Power arrangements internal to the switch for operating the driving mechanism

|  | H01H 3/24 |
· · | using pneumatic or hydraulic actuator

|  | H01H 3/26 |
· · | using dynamo-electric motor (for storing energy in a spring motor Fulltext... Hierarchy... Expanded...H01H 3/30)

|  | H01H 3/28 |
· · | using electromagnet (for storing energy in a spring motor Fulltext... Hierarchy... Expanded...H01H 3/30; for operating relays Fulltext... Hierarchy... Expanded...H01H 45/00)

|  | H01H 3/30 |
· · | using spring motor

|  | H01H 3/32 |
· | Driving mechanisms, i.e. for transmitting driving force to the contacts (snap-action arrangements Fulltext... Hierarchy... Expanded...H01H 5/00; introducing a predetermined time delay Fulltext... Hierarchy... Expanded...H01H 7/00)

|  | H01H 3/34 |
· · | using ratchet

|  | H01H 3/36 |
· · | using belt, chain, or cord

|  | H01H 3/38 |
· · | using spring or other flexible shaft coupling

|  | H01H 3/40 |
· · | using friction, toothed, or screw-and-nut gearing

|  | H01H 3/42 |
· · | using cam or eccentric

|  | H01H 3/44 |
· · | using Geneva movement

|  | H01H 3/46 |
· · | using rod or lever linkage, e.g. toggle

|  | H01H 3/48 |
· · | using lost-motion device

|  | H01H 3/50 |
· · | with indexing or locating means, e.g. indexing by ball and spring

|  | H01H 3/52 |
· · | with means to ensure stopping at intermediate operative positions

|  | H01H 3/54 |
· | Mechanisms for coupling or uncoupling operating parts, driving mechanisms, or contacts

|  | H01H 3/56 |
· · | using electromagnetic clutch

|  | H01H 3/58 |
· · | using friction, toothed, or other mechanical clutch

|  | H01H 3/60 |
· | Mechanical arrangements for preventing or damping vibration or shock

|  | H01H 3/62 |
· | Lubricating means structurally associated with the switch (for lubricating contact-making surfaces Fulltext... Hierarchy... Expanded...H01H 1/60)

|  | H01H 5/00 |
Snap-action arrangements, i.e. in which during a single opening operation or a single closing operation energy is first stored and then released to produce or assist the contact movement

|  | H01H 5/02 |
· | Energy stored by the attraction or repulsion of magnetic parts

|  | H01H 5/04 |
· | Energy stored by deformation of elastic members (by deformation of bimetallic element in thermally-actuated switches Fulltext... Hierarchy... Expanded...H01H 37/54)

|  | H01H 5/06 |
· · | by compression or extension of coil springs

|  | H01H 5/08 |
· · · | one end of spring transmitting movement to the contact member when the other end is moved by the operating part

|  | H01H 5/10 |
· · · | one end of spring being fixedly connected to the stationary or movable part of the switch, and the other end reacting with a movable or stationary rigid member respectively through pins, cams, toothed, or other shaped surfaces

|  | H01H 5/12 |
· · · | having two or more snap-action motions in succession

|  | H01H 5/14 |
· · | by twisting of torsion members

|  | H01H 5/16 |
· · · | with auxiliary means for temporarily holding parts until torsion member is sufficiently strained

|  | H01H 5/18 |
· · | by flexing of blade springs

|  | H01H 5/20 |
· · · | single blade moved across dead-centre position

|  | H01H 5/22 |
· · · | blade spring with at least one snap-acting leg and at least one separate contact-carrying or contact-actuating leg

|  | H01H 5/24 |
· · · · | having three legs

|  | H01H 5/26 |
· · · | having two or more snap-action motions in succession

|  | H01H 5/28 |
· · · | two separate blade springs forming a toggle

|  | H01H 5/30 |
· · | by buckling of disc springs

|  | H01H 7/00 |
Devices for introducing a predetermined time delay between the initiation of the switching operation and the opening or closing of the contacts (time or time-programme switches Fulltext... Hierarchy... Expanded...H01H 43/00)

|  | H01H 7/02 |
· | with fluid timing means

|  | H01H 7/03 |
· · | with dash-pots

|  | H01H 7/04 |
· · | with flies, i.e. fan governors

|  | H01H 7/06 |
· | with thermal timing means (thermally-actuated switches Fulltext... Hierarchy... Expanded...H01H 37/00)

|  | H01H 7/08 |
· | with timing by mechanical speed-control devices

|  | H01H 7/10 |
· · | by escapement

|  | H01H 7/12 |
· · · | mechanical

|  | H01H 7/14 |
· · · | electromagnetic

|  | H01H 7/16 |
· | Devices for ensuring operation of the switch at a predetermined point in the ac cycle (circuit arrangements Fulltext... Hierarchy... Expanded...H01H 9/56)

|  | H01H 9/00 |
Details of switching devices, not covered by groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 1/00-H01H 7/00 (casings for switchgear Fulltext... Hierarchy... Expanded...H02B 1/26; casings for electrical apparatus in general Fulltext... Hierarchy... Expanded...H05K 5/00)

|  | H01H 9/02 |
· | Bases, casings, or covers (accommodating more than one switch or a switch and another electrical component Fulltext... Hierarchy... Expanded...H02B 1/26)

|  | H01H 9/04 |
· · | Dustproof, splashproof, drip-proof, waterproof, or flameproof casings

|  | H01H 9/06 |
· · | Casing of switch constituted by a handle serving a purpose other than the actuation of the switch, e.g. by the handle of a vacuum cleaner

|  | H01H 9/08 |
· | Arrangements to facilitate replacement of switch, e.g. cartridge housing

|  | H01H 9/10 |
· | Adaptation for built-in fuses (mounting switch and fuse separately on, or in, common support Fulltext... Hierarchy... Expanded...H02B)

|  | H01H 9/12 |
· | Means for earthing parts of switch not normally conductively connected to the contacts

|  | H01H 9/14 |
· | Adaptation for built-in safety spark gaps

|  | H01H 9/16 |
· | Indicators for switching condition, e.g. "on" or "off"

|  | H01H 9/18 |
· | Distinguishing marks on switches, e.g. for indicating switch location in the dark; Adaptation of switches to receive distinguishing marks

|  | H01H 9/20 |
· | Interlocking, locking, or latching mechanisms (contacts adapted to act as latches Fulltext... Hierarchy... Expanded...H01H 1/52; by an auxiliary movement of the operating part or of an attachment thereto Fulltext... Hierarchy... Expanded...H01H 3/20)

|  | H01H 9/22 |
· · | for interlocking between casing, cover, or protective shutter and mechanism for operating contacts

|  | H01H 9/24 |
· · | for interlocking two or more parts of the mechanism for operating contacts

|  | H01H 9/26 |
· · | for interlocking two or more switches (by a detachable member Fulltext... Hierarchy... Expanded...H01H 9/28)

|  | H01H 9/28 |
· · | for locking switch parts by a key or equivalent removable member (switches operated by a key Fulltext... Hierarchy... Expanded...H01H 27/00; locking by removable part of two-part coupling device Fulltext... Hierarchy... Expanded...H01R)

|  | H01H 9/30 |
· | Means for extinguishing or preventing arc between current-carrying parts

|  | H01H 9/32 |
· · | Insulating body insertable between contacts

|  | H01H 9/34 |
· · | Stationary parts for restricting or subdividing the arc, e.g. barrier plate

|  | H01H 9/36 |
· · · | Metal parts

|  | H01H 9/38 |
· · | Auxiliary contacts on to which the arc is transferred from the main contacts (using arcing-horns Fulltext... Hierarchy... Expanded...H01H 9/46)

|  | H01H 9/40 |
· · | Multiple main contacts for the purpose of dividing the current through, or potential drop along, the arc

|  | H01H 9/42 |
· · | Impedances connected with contacts

|  | H01H 9/44 |
· · | using blow-out magnet

|  | H01H 9/46 |
· · | using arcing horns (using blow-out magnet Fulltext... Hierarchy... Expanded...H01H 9/44; arcing horns per se Fulltext... Hierarchy... Expanded...H01T 4/14)

|  | H01H 9/48 |
· | Means for preventing discharge to non-current-carrying parts, e.g. using corona ring

|  | H01H 9/50 |
· | Means for detecting the presence of an arc or discharge

|  | H01H 9/52 |
· | Cooling of switch parts (cooling of contacts Fulltext... Hierarchy... Expanded...H01H 1/62)

|  | H01H 9/54 |
· | Circuit arrangements not adapted to a particular application of the switching device and for which no provision exists elsewhere

|  | H01H 9/56 |
· · | for ensuring operation of the switch at a predetermined point in the ac cycle

|  | H01H 11/00 |
Apparatus or processes specially adapted for the manufacture of electric switches

|  | H01H 11/02 |
· | for mercury switches

|  | H01H 11/04 |
· | of switch contacts

|  | H01H 11/06 |
· · | Fixing of contacts to carrier

|  | H01H 13/00 |
Switches having rectilinearly-movable operating part or parts adapted for pushing or pulling in one direction only, e.g. push-button switch (wherein the operating part is flexible Fulltext... Hierarchy... Expanded...H01H 17/00)

|  | H01H 13/02 |
· | Details

|  | H01H 13/04 |
· · | Cases; Covers

|  | H01H 13/06 |
· · · | Dustproof, splashproof, drip-proof, waterproof, or flameproof casings

|  | H01H 13/08 |
· · · | Casing of switch constituted by a handle serving a purpose other than the actuation of the switch

|  | H01H 13/10 |
· · | Bases; Stationary contacts mounted thereon

|  | H01H 13/12 |
· · | Movable parts; Contacts mounted thereon

|  | H01H 13/14 |
· · · | Operating parts, e.g. push-button

|  | H01H 13/16 |
· · · · | adapted for operation by a part of the human body other than the hand, e.g. by foot

|  | H01H 13/18 |
· · · · | adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift

|  | H01H 13/20 |
· · · | Driving mechanisms

|  | H01H 13/22 |
· · · · | acting with snap action (depending upon deformation of elastic members Fulltext... Hierarchy... Expanded...H01H 13/26)

|  | H01H 13/24 |
· · · · | with means for introducing a predetermined time delay

|  | H01H 13/26 |
· · | Snap-action arrangements depending upon deformation of elastic members

|  | H01H 13/28 |
· · · | using compression or extension of coil springs

|  | H01H 13/30 |
· · · · | one end of spring transmitting movement to the contact member when the other end is moved by the operating part

|  | H01H 13/32 |
· · · · | one end of spring being fixedly connected to the stationary or movable part of the switch and the other end reacting with a movable or stationary rigid member respectively through pins, cams, toothed, or other shaped surfaces

|  | H01H 13/34 |
· · · · | having two or more snap-action motions in succession

|  | H01H 13/36 |
· · · | using flexing of blade springs

|  | H01H 13/38 |
· · · · | Single blade moved across dead-centre position

|  | H01H 13/40 |
· · · · | Blade spring with at least one snap-acting leg and at least one separate contactcarrying or contact-actuating leg

|  | H01H 13/42 |
· · · · · | having three legs

|  | H01H 13/44 |
· · · · | having two or more snap-action motions in succession

|  | H01H 13/46 |
· · · · | two separate blade springs forming a toggle

|  | H01H 13/48 |
· · · | using buckling of disc springs

|  | H01H 13/50 |
· | having a single operating member

|  | H01H 13/52 |
· · | the contact returning to its original state immediately upon removal of operating force, e.g. bell push switch

|  | H01H 13/54 |
· · | the contact returning to its original state a predetermined time interval after removal of operating force, e.g. for staircase lighting

|  | H01H 13/56 |
· · | the contact returning to its original state upon the next application of operating force

|  | H01H 13/58 |
· · · | with contact-driving member rotated step-wise in one direction

|  | H01H 13/60 |
· · · | with contact-driving member moved alternately in opposite directions

|  | H01H 13/62 |
· · | the contact returning to its original state upon manual release of a latch (latch released by second push-button Fulltext... Hierarchy... Expanded...H01H 13/68)

|  | H01H 13/64 |
· · | wherein the switch has more than two electrically distinguishable positions, e.g. multi-position push-button switches

|  | H01H 13/66 |
· · · | the operating member having only two positions

|  | H01H 13/68 |
· | having two operating members, one for opening and one for closing the same set of contacts (single operating member protruding from different sides of switch casing for alternate pushing upon opposite ends Fulltext... Hierarchy... Expanded...H01H 15/22)

|  | H01H 13/70 |
· | having a plurality of operating members associated with different sets of contacts, e.g. keyboard (keyboards for special applications, see the relevant subclasses or groups, e.g. Fulltext... Hierarchy... Expanded...B41J, Fulltext... Hierarchy... Expanded...G06F 3/023, Fulltext... Hierarchy... Expanded...H04L 15/00, Fulltext... Hierarchy... Expanded...H04L 17/00, Fulltext... Hierarchy... Expanded...H04M 1/00; mounting together a plurality of independent switches Fulltext... Hierarchy... Expanded...H02B)

|  | H01H 13/72 |
· · | wherein the switch has means for limiting the number of operating members that can concurrently be in the actuated position

|  | H01H 13/74 |
· · · | each contact set returning to its original state only upon actuation of another of the operating members

|  | H01H 13/76 |
· · | wherein some or all of the operating members actuate different combinations of the contact sets, e.g. ten operating members actuating different combinations of four contact sets

|  | H01H 15/00 |
Switches having rectilinearly-movable operating part or parts adapted for actuation in opposite directions, e.g. slide switch

|  | H01H 15/02 |
· | Details

|  | H01H 15/04 |
· · | Stationary parts; Contacts mounted thereon

|  | H01H 15/06 |
· · | Movable parts; Contacts mounted thereon

|  | H01H 15/08 |
· · · | Contact arrangements for providing make-before-break operation, e.g. for on-load tap-changing

|  | H01H 15/10 |
· · · | Operating parts

|  | H01H 15/12 |
· · · · | adapted for operation by a part of the human body other than the hand, e.g. by foot

|  | H01H 15/14 |
· · · · | adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift

|  | H01H 15/16 |
· · · | Driving mechanisms

|  | H01H 15/18 |
· · · · | acting with snap action

|  | H01H 15/20 |
· · · · | with means for introducing a predetermined time delay

|  | H01H 15/22 |
· | having a single operating part protruding from different sides of switch casing for alternate actuation from opposite ends

|  | H01H 15/24 |
· | having a single operating part only protruding from one side of the switch casing for alternate pushing and pulling

|  | H01H 17/00 |
Switches having flexible operating part adapted only for pulling, e.g. cord, chain

|  | H01H 17/02 |
· | Details

|  | H01H 17/04 |
· · | Stationary parts (guides Fulltext... Hierarchy... Expanded...H01H 17/14)

|  | H01H 17/06 |
· · | Movable parts (guides Fulltext... Hierarchy... Expanded...H01H 17/14)

|  | H01H 17/08 |
· · · | Operating part, e.g. cord

|  | H01H 17/10 |
· · · · | adapted for operation by a part of the human body other than the hand, e.g. by foot

|  | H01H 17/12 |
· · · · | adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift

|  | H01H 17/14 |
· · | Guiding means for flexible operating part

|  | H01H 17/16 |
· | having a single flexible operating part adapted for pulling at one end only

|  | H01H 17/18 |
· · | secured to a part of the switch driving mechanism that has only angular movement

|  | H01H 17/20 |
· · · | the contact returning to its original state immediately upon removal of operating force

|  | H01H 17/22 |
· · · | the contact returning to its original state upon the next application of operating force

|  | H01H 17/24 |
· · | secured to a part of the switch driving mechanism that has both angular and rectilinear motion

|  | H01H 17/26 |
· | having two flexible operating parts; having a single operating part adapted for pulling at both ends

|  | H01H 17/28 |
· · | secured to a part or parts of the switch driving mechanism having only rectilinear motion

|  | H01H 17/30 |
· · | secured to a part or parts of the switch driving mechanism having only angular motion

|  | H01H 19/00 |
Switches operated by angular displacement of the operating part thereof acted upon directly by a solid body external to the switch, e.g. by a hand, wherein this part may be turned through an unlimited or unspecified angle (rotary current collectors, distributors, or interrupters Fulltext... Hierarchy... Expanded...H01R 39/00)

|  | H01H 19/02 |
· | Details

|  | H01H 19/04 |
· · | Cases; Covers

|  | H01H 19/06 |
· · · | Dustproof, splashproof, drip-proof, waterproof, or flameproof casings

|  | H01H 19/08 |
· · | Bases; Stationary contacts mounted thereon

|  | H01H 19/10 |
· · | Movable parts; Contacts mounted thereon

|  | H01H 19/12 |
· · · | Contact arrangements for providing make-before-break operation, e.g. for on-load tap-changing

|  | H01H 19/14 |
· · · | Operating parts, e.g. turn knob

|  | H01H 19/16 |
· · · · | adapted for operation by a part of the human body other than the hand, e.g. by foot

|  | H01H 19/18 |
· · · · | adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift

|  | H01H 19/20 |
· · · | Driving mechanisms allowing angular displacement of the operating part to be effective in either direction

|  | H01H 19/22 |
· · · · | incorporating lost motion

|  | H01H 19/24 |
· · · · | acting with snap action

|  | H01H 19/26 |
· · · · | with means for introducing a predetermined time delay

|  | H01H 19/28 |
· · · | Driving mechanisms allowing angular displacement of the operating part to be effective or possible in only one direction

|  | H01H 19/30 |
· · · · | incorporating lost motion

|  | H01H 19/32 |
· · · · | acting with snap action

|  | H01H 19/34 |
· · · · | with means for introducing a predetermined time delay

|  | H01H 19/36 |
· | the operating part having only two operative positions, e.g. relatively displaced by 180°

|  | H01H 19/38 |
· · | Change-over switches

|  | H01H 19/40 |
· · · | having only axial contact pressure

|  | H01H 19/42 |
· · | providing more than two electrically-different conditions, e.g. for closing either or both of two circuits

|  | H01H 19/44 |
· · · | having only axial contact pressure

|  | H01H 19/46 |
· | the operating part having three operative positions, e.g. off/star/delta

|  | H01H 19/48 |
· · | having only axial contact pressure

|  | H01H 19/50 |
· | the operating part having four operative positions, e.g. off/two-in-series/one-only/two-in-parallel

|  | H01H 19/52 |
· · | having only axial contact pressure

|  | H01H 19/54 |
· | the operating part having at least five or an unspecified number of operative positions

|  | H01H 19/56 |
· · | Angularly-movable actuating part carrying contacts, e.g. drum switch

|  | H01H 19/58 |
· · · | having only axial contact pressure, e.g. disc switch, wafer switch

|  | H01H 19/60 |
· · | Angularly-movable actuating part carrying no contacts

|  | H01H 19/62 |
· · · | Contacts actuated by radial cams

|  | H01H 19/63 |
· · · | Contacts actuated by axial cams [2]

|  | H01H 19/64 |
· | Encased switches adapted for ganged operation when assembled in a line with identical switches, e.g. stacked switches

|  | H01H 21/00 |
Switches operated by angular displacement of the operating part thereof acted upon directly by a solid body, e.g. by a hand, wherein this part may be turned through a restricted angle only (tumbler switches Fulltext... Hierarchy... Expanded...H01H 23/00)

|  | H01H 21/02 |
· | Details

|  | H01H 21/04 |
· · | Cases; Covers

|  | H01H 21/06 |
· · · | interlocked with operating mechanism

|  | H01H 21/08 |
· · · | Dustproof, splashproof, drip-proof, waterproof, or flameproof casings

|  | H01H 21/10 |
· · · | Casing of switch constituted by a handle serving a purpose other than the actuation of the switch

|  | H01H 21/12 |
· · | Bases; Stationary contacts mounted thereon

|  | H01H 21/14 |
· · | Means for increasing contact pressure

|  | H01H 21/16 |
· · | Adaptation for built-in fuse

|  | H01H 21/18 |
· · | Movable parts; Contacts mounted thereon

|  | H01H 21/20 |
· · · | Contact arrangements for providing make-before-break operation, e.g. for on-load tap-changing

|  | H01H 21/22 |
· · · | Operating parts, e.g. handle

|  | H01H 21/24 |
· · · · | biased to return to original position upon removal of operating force

|  | H01H 21/26 |
· · · · · | adapted for operation by a part of the human body other than the hand, e.g. by foot

|  | H01H 21/28 |
· · · · · | adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift

|  | H01H 21/30 |
· · · · | not biased to return to original position upon removal of operating force

|  | H01H 21/32 |
· · · · · | adapted for operation by a part of the human body other than the hand, e.g. by foot

|  | H01H 21/34 |
· · · · · | adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift

|  | H01H 21/36 |
· · · | Driving mechanisms

|  | H01H 21/38 |
· · · · | incorporating lost motion

|  | H01H 21/40 |
· · · · | having snap action

|  | H01H 21/42 |
· · · · · | produced by compression or extension of coil spring

|  | H01H 21/44 |
· · · · · | produced by flexing blade springs

|  | H01H 21/46 |
· · · · · | with two or more snap-action motions in succession

|  | H01H 21/48 |
· · · · | incorporating a ratchet mechanism

|  | H01H 21/50 |
· · · · | with indexing or latching means, e.g. indexing by ball and spring; with means to ensure stopping at intermediate operative positions

|  | H01H 21/52 |
· · · · | with means for introducing a predetermined time delay

|  | H01H 21/54 |
· | Lever switches with blade-type contact co-operating with one or two spring-clip contacts, e.g. knife switch, sectionalisers

|  | H01H 21/56 |
· · | making contact in one position only

|  | H01H 21/58 |
· · | Change-over switches without stable intermediate position

|  | H01H 21/60 |
· · | Change-over switches with stable intermediate position

|  | H01H 21/62 |
· | Switches with moving contact sliding over stud contacts

|  | H01H 21/64 |
· · | with two operative positions, e.g. on/off

|  | H01H 21/66 |
· · · | having only axial contact pressure

|  | H01H 21/68 |
· · | with three operative positions, e.g. change-over switch with stable intermediate position

|  | H01H 21/70 |
· · · | having only axial contact pressure

|  | H01H 21/72 |
· · | with four operative positions

|  | H01H 21/74 |
· · · | having only axial contact pressure

|  | H01H 21/76 |
· · | with at least five or an unspecified number of operative positions, e.g. drum switch

|  | H01H 21/78 |
· · · | having only axial contact pressure, e.g. face-plate switch

|  | H01H 21/80 |
· | Switches with angularly-movable actuating part carrying no contacts

|  | H01H 21/82 |
· · | Contacts actuated by radial cams

|  | H01H 21/84 |
· · | Contacts actuated by rectilinearly-movable member linked to operating part, e.g. by pin and slot

|  | H01H 21/86 |
· | Switches with abutting contact carried by operating part, e.g. telegraph tapping key

|  | H01H 21/88 |
· · | with intermediate position of rest

|  | H01H 23/00 |
Tumbler switches, i.e. actuated by digitally rocking a part of the switch in one plane only

|  | H01H 23/02 |
· | Details

|  | H01H 23/04 |
· · | Cases; Covers

|  | H01H 23/06 |
· · · | Dustproof, splashproof, drip-proof, waterproof, or flameproof casings

|  | H01H 23/08 |
· · | Bases; Stationary contacts mounted thereon

|  | H01H 23/10 |
· · | Adaptation for built-in fuse

|  | H01H 23/12 |
· · | Movable parts; Contacts mounted thereon

|  | H01H 23/14 |
· · · | Tumblers

|  | H01H 23/16 |
· · · | Driving mechanisms

|  | H01H 23/18 |
· · · · | incorporating lost motion

|  | H01H 23/20 |
· · · · | having snap action

|  | H01H 23/22 |
· · · · | with means for introducing a predetermined time delay

|  | H01H 23/24 |
· | with two operating positions

|  | H01H 23/26 |
· · | one of which positions is unstable

|  | H01H 23/28 |
· | with three operating positions

|  | H01H 23/30 |
· · | with stable centre position and one or both end positions unstable

|  | H01H 25/00 |
Switches with compound movement of handle or other operating part

|  | H01H 25/04 |
· | Operating part movable angularly in more than one plane, e.g. joystick

|  | H01H 25/06 |
· | Operating part movable both angularly and rectilinearly, the rectilinear movement being along the axis of angular movement

|  | H01H 27/00 |
Switches operated by a removable member, e.g. key, plug, plate; Switches operated by setting members according to a single predetermined combination out of several possible settings (locking switch parts to prevent operation Fulltext... Hierarchy... Expanded...H01H 9/28; combined with plug-and-socket connectors Fulltext... Hierarchy... Expanded...H01R; with current-carrying plug Fulltext... Hierarchy... Expanded...H01R 31/08)

|  | H01H 27/04 |
· | Insulating plug or plate inserted between normally-closed contacts

|  | H01H 27/06 |
· | Key inserted and then turned to effect operation of the switch

|  | H01H 27/08 |
· · | wherein the key cannot be removed until the switch is returned to its original position

|  | H01H 27/10 |
· | Switch operated by setting members according to a single predetermined combination out of several possible settings

|  | H01H 29/00 |
Switches having at least one liquid contact (solid contacts wetted or soaked with mercury Fulltext... Hierarchy... Expanded...H01H 1/08)

|  | H01H 29/02 |
· | Details

|  | H01H 29/04 |
· · | Contacts; Containers for liquid contacts

|  | H01H 29/06 |
· · · | Liquid contacts characterised by the material thereof

|  | H01H 29/08 |
· · | Means for introducing a predetermined time delay

|  | H01H 29/10 |
· · · | by constricting the flow of the contact liquid

|  | H01H 29/12 |
· · | Operating mechanisms adapted for operation by a part of the human body other than the hand, e.g. by foot

|  | H01H 29/14 |
· · | Operating mechanisms adapted for actuation at a limit or other predetermined position in the path of a body, the relative movement of switch and body being primarily for a purpose other than the actuation of the switch, e.g. door switch, limit switch, floor-levelling switch of a lift

|  | H01H 29/16 |
· | operated by dipping solid contact into stationary contact liquid

|  | H01H 29/18 |
· | with level of surface of contact liquid displaced by non-electrical contact-making plunger

|  | H01H 29/20 |
· | operated by tilting contact-liquid container (centrifugal mercury switches Fulltext... Hierarchy... Expanded...H01H 29/26)

|  | H01H 29/22 |
· · | wherein contact is made and broken between liquid and solid

|  | H01H 29/24 |
· · | wherein contact is made and broken between liquid and liquid

|  | H01H 29/26 |
· | with level of surface of contact liquid displaced by centrifugal action

|  | H01H 29/28 |
· | with level of surface of contact liquid displaced by fluid pressure

|  | H01H 29/30 |
· | with level of surface of contact liquid displaced by expansion or evaporation thereof

|  | H01H 29/32 |
· | with contact made by a liquid jet, e.g. earthing switch with contact made by jet of water (operated by direct electrodynamic action Fulltext... Hierarchy... Expanded...H01H 53/00)

|  | H01H 31/00 |
Air-break switches for high tension without arc-extinguishing or arc-preventing means (in combination with high tension or heavy-current switches with arc-extinguishing or arc-preventing means Fulltext... Hierarchy... Expanded...H01H 33/00; switching arrangements for the supply or distribution of electric power Fulltext... Hierarchy... Expanded...H02B) [3]

|  | H01H 31/02 |
· | Details

|  | H01H 31/04 |
· · | Interlocking mechanisms (for interlocking with high-tension or heavy-current switches having arc-extinguishing or arc-preventing means Fulltext... Hierarchy... Expanded...H01H 33/52)

|  | H01H 31/06 |
· · · | for interlocking between casing, cover, or protective shutter and mechanism for operating contacts

|  | H01H 31/08 |
· · · | for interlocking two or more parts of the mechanism for operating contacts

|  | H01H 31/10 |
· · · | for interlocking two or more switches (for interlocking with high-tension or heavy-current switches having arc-extinguishing or arc-preventing means Fulltext... Hierarchy... Expanded...H01H 33/52)

|  | H01H 31/12 |
· · | Adaptation for built-in fuse

|  | H01H 31/14 |
· | with bridging contact that is not electrically connected to either line contact in open position of switch

|  | H01H 31/16 |
· · | with angularly-movable bridging contact or contact-carrying member

|  | H01H 31/18 |
· · · | actuated through the movement of one or more insulators

|  | H01H 31/20 |
· · · · | at least one insulator being rotatable about its own geometrical axis

|  | H01H 31/22 |
· · · | wherein the contact or contacts are rectilinearly movable with respect to the carrying member

|  | H01H 31/24 |
· · | with rectilinearly-movable bridging contact

|  | H01H 31/26 |
· | with movable contact that remains electrically connected to one line in open position of switch

|  | H01H 31/28 |
· · | with angularly-movable contact

|  | H01H 31/30 |
· · · | actuated-through the movement of one or more insulators

|  | H01H 31/32 |
· · | with rectilinearly-movable contact

|  | H01H 31/34 |
· | with movable contact adapted to engage an overhead transmission line, e.g. for branching

|  | H01H 31/36 |
· · | Contact moved by pantograph

|  | H01H 33/00 |
High-tension or heavy-current switches with arc-extinguishing or arc-preventing means

|  | H01H 33/02 |
· | Details

|  | H01H 33/04 |
· · | Means for extinguishing or preventing arc between current-carrying parts (for switches in general Fulltext... Hierarchy... Expanded...H01H 9/30)

|  | H01H 33/06 |
· · · | Insulating body insertable between contacts

|  | H01H 33/08 |
· · · | Stationary parts for restricting or subdividing the arc, e.g. barrier plate

|  | H01H 33/10 |
· · · · | Metal parts

|  | H01H 33/12 |
· · · | Auxiliary contacts on to which the arc is transferred from the main contacts (using arcing horns Fulltext... Hierarchy... Expanded...H01H 33/20)

|  | H01H 33/14 |
· · · | Multiple main contacts for the purpose of dividing the current through, or potential drop along, the arc

|  | H01H 33/16 |
· · · | Impedances connected with contacts

|  | H01H 33/18 |
· · · | using blow-out magnet

|  | H01H 33/20 |
· · · | using arcing horns (using blow-out magnet Fulltext... Hierarchy... Expanded...H01H 33/18; arcing horns per se Fulltext... Hierarchy... Expanded...H01T 4/14)

|  | H01H 33/22 |
· · · | Selection of fluids for arc-extinguishing

|  | H01H 33/24 |
· · | Means for preventing discharge to non-current-carrying parts, e.g. using corona ring

|  | H01H 33/26 |
· · | Means for detecting the presence of an arc or other discharge

|  | H01H 33/28 |
· · | Power arrangements internal to the switch for operating the driving mechanism

|  | H01H 33/30 |
· · · | using fluid actuator

|  | H01H 33/32 |
· · · · | pneumatic

|  | H01H 33/34 |
· · · · | hydraulic

|  | H01H 33/36 |
· · · | using dynamo-electric motor (for storing energy in a spring motor Fulltext... Hierarchy... Expanded...H01H 33/40)

|  | H01H 33/38 |
· · · | using electromagnet (for storing energy in a spring motor Fulltext... Hierarchy... Expanded...H01H 33/40)

|  | H01H 33/40 |
· · · | using spring motor

|  | H01H 33/42 |
· · | Driving mechanisms

|  | H01H 33/44 |
· · | Devices for ensuring operation of the switch at a predetermined point in the ac cycle (circuit arrangements Fulltext... Hierarchy... Expanded...H01H 33/59)

|  | H01H 33/46 |
· · | Interlocking mechanisms

|  | H01H 33/48 |
· · · | for interlocking between casing or cover and mechanism for operating contacts

|  | H01H 33/50 |
· · · | for interlocking two or more parts of the mechanism for operating contacts

|  | H01H 33/52 |
· · · | for interlocking two or more switches

|  | H01H 33/53 |
· · | Cases (for switchgear Fulltext... Hierarchy... Expanded...H02B 1/26); Reservoirs, tanks, piping or valves, for arc-extinguishing fluid; Accessories therefor, e.g. safety arrangements, pressure relief devices [3]

|  | H01H 33/55 |
· · · | Oil reservoirs or tanks; Lowering means therefor (associated with withdrawal mechanism for isolation of switch Fulltext... Hierarchy... Expanded...H02B 11/08)

|  | H01H 33/56 |
· · · | Gas reservoirs

|  | H01H 33/57 |
· · · | Recuperation of liquid or gas

|  | H01H 33/575 |
· · · | Pressure relief devices for normal or emergency use [3]

|  | H01H 33/58 |
· · · | Silencers for suppressing noise of switch operation [3]

|  | H01H 33/59 |
· · | Circuit arrangements not adapted to a particular application of the switch and not otherwise provided for, e.g. for ensuring operation of the switch at a predetermined point in the ac cycle

|  | H01H 33/60 |
· | Switches wherein the means for extinguishing or preventing the arc do not include separate means for obtaining or increasing flow of arc-extinguishing fluid

|  | H01H 33/62 |
· · | wherein the break is in air at atmospheric pressure, e.g. in open air

|  | H01H 33/64 |
· · | wherein the brake is in gas (in air at atmospheric pressure Fulltext... Hierarchy... Expanded...H01H 33/62; vacuum switches Fulltext... Hierarchy... Expanded...H01H 33/66)

|  | H01H 33/66 |
· · | Vacuum switches

|  | H01H 33/68 |
· · | Liquid-break switches, e.g. oil-break

|  | H01H 33/70 |
· | Switches with separate means for directing, obtaining, or increasing flow of arc-extinguishing fluid

|  | H01H 33/72 |
· · | having stationary parts for directing the flow of arc-extinguishing fluid, e.g. arc-extinguishing chamber

|  | H01H 33/73 |
· · · | wherein the break is in air at atmospheric pressure, e.g. in open air

|  | H01H 33/74 |
· · · | wherein the break is in gas (in air at atmospheric pressure Fulltext... Hierarchy... Expanded...H01H 33/73)

|  | H01H 33/75 |
· · · | Liquid-break switches, e.g. oil-break

|  | H01H 33/76 |
· · | wherein arc-extinguishing gas is evolved from stationary parts; Selection of material therefor

|  | H01H 33/77 |
· · · | wherein the break is in air at atmospheric pressure

|  | H01H 33/78 |
· · · | wherein the break is in gas (in air at atmospheric pressure Fulltext... Hierarchy... Expanded...H01H 33/77)

|  | H01H 33/80 |
· · | flow of arc-extinguishing fluid from a pressure source being controlled by a valve

|  | H01H 33/82 |
· · · | the fluid being air or gas

|  | H01H 33/825 |
· · · · | with closed circuit of air or gas (Fulltext... Hierarchy... Expanded...H01H 33/835 takes precedence) [3]

|  | H01H 33/83 |
· · · · | wherein the contacts are opened by the flow of air or gas

|  | H01H 33/835 |
· · · · · | with closed circuit of air or gas [3]

|  | H01H 33/84 |
· · · | the fluid being liquid, e.g. oil

|  | H01H 33/85 |
· · · · | wherein the contacts are opened by the flow of liquid

|  | H01H 33/86 |
· · | the flow of arc-extinguishing fluid under pressure from the contact space being controlled by a valve

|  | H01H 33/867 |
· · · | the fluid being air or gas [3]

|  | H01H 33/873 |
· · · · | with closed circuit of air or gas [3]

|  | H01H 33/88 |
· · | the flow of arc-extinguishing fluid being produced or increased by movement of pistons or other pressure-producing parts

|  | H01H 33/90 |
· · · | this movement being effected by, or in conjunction with, the contact-operating mechanism

|  | H01H 33/91 |
· · · · | the arc-extinguishing fluid being air or gas

|  | H01H 33/915 |
· · · · · | with closed circuit of air or gas [3]

|  | H01H 33/92 |
· · · · | the arc-extinguishing fluid being liquid, e.g. oil

|  | H01H 33/94 |
· · · | this movement being effected solely due to the pressure caused by the arc itself or by an auxiliary arc

|  | H01H 33/95 |
· · · · | the arc-extinguishing fluid being air or gas

|  | H01H 33/96 |
· · · · | the arc-extinguishing fluid being liquid, e.g. oil

|  | H01H 33/98 |
· · | the flow of arc-extinguishing fluid being initiated by an auxiliary arc or a section of the arc, without any moving parts for producing or increasing the flow

|  | H01H 33/985 |
· · · | the fluid being air or gas [3]

|  | H01H 33/99 |
· · · | the fluid being liquid [3]

|  | H01H 35/00 |
Switches operated by change of a physical condition (operated by change of magnetic or electric field Fulltext... Hierarchy... Expanded...H01H 36/00; thermally-actuated switches Fulltext... Hierarchy... Expanded...H01H 37/00; time switches Fulltext... Hierarchy... Expanded...H01H 43/00; relays Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 45/00-H01H 61/00; sensing elements for providing continuous conversion of a variable into mechanical displacement Fulltext... Hierarchy... Expanded...G01)

|  | H01H 35/00 |
Note(s) A switching device is classified according to that physical condition which when changed acts as input to the device, e.g. external explosion causing pressure wave to act upon switch is classified in group Fulltext... Hierarchy... Expanded...H01H 35/24, an explosion produced within the switch in group Fulltext... Hierarchy... Expanded...H01H 37/00 if initiated by heat, in group Fulltext... Hierarchy... Expanded...H01H 39/00 if initiated electrically, and in group Fulltext... Hierarchy... Expanded...H01H 35/14 if initiated by an external blow.

|  | H01H 35/02 |
· | Switches operated by change of position, inclination, or orientation of the switch itself in relation to gravitational field (tilting mercury container Fulltext... Hierarchy... Expanded...H01H 29/20; change of position due to change of liquid level Fulltext... Hierarchy... Expanded...H01H 35/18)

|  | H01H 35/06 |
· | Switches operated by change of speed (operated by change of fluid flow Fulltext... Hierarchy... Expanded...H01H 35/24)

|  | H01H 35/10 |
· · | Centrifugal switches (level of mercury displaced by centrifugal action Fulltext... Hierarchy... Expanded...H01H 29/26)

|  | H01H 35/12 |
· · | operated by reversal of direction of movement

|  | H01H 35/14 |
· | Switches operated by change of acceleration, e.g. by shock or vibration, inertia switch

|  | H01H 35/18 |
· | Switches operated by change of liquid level or of liquid density, e.g. float switch (wherein the liquid constitutes a contact of the switch Fulltext... Hierarchy... Expanded...H01H 29/00; by magnet carried on a float Fulltext... Hierarchy... Expanded...H01H 36/02)

|  | H01H 35/24 |
· | Switches operated by change of fluid pressure, by fluid pressure waves, or by change of fluid flow (wherein the change of pressure is caused by change of temperature Fulltext... Hierarchy... Expanded...H01H 37/36)

|  | H01H 35/26 |
· · | Details

|  | H01H 35/28 |
· · · | Compensation for variation of ambient pressure or temperature

|  | H01H 35/30 |
· · · | Means for transmitting pressure to pressure-responsive operating part, e.g. by capsule and capillary tube

|  | H01H 35/32 |
· · | actuated by bellows

|  | H01H 35/34 |
· · | actuated by diaphragm

|  | H01H 35/36 |
· · | actuated by curled flexible tube, e.g. Bourdon tube

|  | H01H 35/38 |
· · | actuated by piston and cylinder

|  | H01H 35/40 |
· · | actuated by devices allowing continual flow of fluid, e.g. vane

|  | H01H 35/42 |
· | Switches operated by change of humidity

|  | H01H 36/00 |
Switches actuated by change of magnetic field or of electric field, e.g. by change of relative position of magnet and switch, by shielding

|  | H01H 36/02 |
· | actuated by movement of a float carrying a magnet

|  | H01H 37/00 |
Thermally-actuated switches (electrothermal relays operated by electrical input Fulltext... Hierarchy... Expanded...H01H 61/00; protective switches with electrothermal release or actuation Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 73/00-H01H 83/00)

|  | H01H 37/02 |
· | Details

|  | H01H 37/04 |
· · | Bases; Housings; Mountings

|  | H01H 37/06 |
· · · | to facilitate replacement, e.g. cartridge housing

|  | H01H 37/08 |
· · | Indicators; Distinguishing marks

|  | H01H 37/10 |
· · | Compensation for variation of ambient temperature or pressure

|  | H01H 37/12 |
· · | Means for adjustment of "on" or "off" operating temperature

|  | H01H 37/14 |
· · · | by anticipatory electric heater

|  | H01H 37/16 |
· · · | by varying the proportion of input heat received by the thermal element, e.g. by displacement of a shield

|  | H01H 37/18 |
· · · | by varying bias on the thermal element due to a separate spring

|  | H01H 37/20 |
· · · | by varying the position of the thermal element in relation to switch base or casing

|  | H01H 37/22 |
· · · | by adjustment of a member transmitting motion from the thermal element to contacts or latch

|  | H01H 37/24 |
· · · | by adjustment of position of the movable contact on its driving member

|  | H01H 37/26 |
· · · | by adjustment of abutment for "off" position of the movable contact

|  | H01H 37/28 |
· · · | by adjustment of the position of the fixed contact

|  | H01H 37/30 |
· · · | by varying the position of the contact unit in relation to switch base or casing

|  | H01H 37/32 |
· · | Thermally-sensitive members (temperature-responsive elements in general Fulltext... Hierarchy... Expanded...G01K)

|  | H01H 37/34 |
· · · | Means for transmitting heat thereto, e.g. capsule remote from contact member

|  | H01H 37/36 |
· · · | actuated due to expansion or contraction of a fluid with or without vaporisation (the fluid forming a contact of the switch Fulltext... Hierarchy... Expanded...H01H 29/04, Fulltext... Hierarchy... Expanded...H01H 29/30)

|  | H01H 37/38 |
· · · · | with bellows

|  | H01H 37/40 |
· · · · | with diaphragm

|  | H01H 37/42 |
· · · · | with curled flexible tube, e.g. Bourdon tube

|  | H01H 37/44 |
· · · · | with piston and cylinder

|  | H01H 37/46 |
· · · | actuated due to expansion or contraction of a solid (deflection of a bimetallic element Fulltext... Hierarchy... Expanded...H01H 37/52)

|  | H01H 37/48 |
· · · · | with extensible rigid rods or tubes

|  | H01H 37/50 |
· · · · | with extensible wires under tension

|  | H01H 37/52 |
· · · | actuated due to deflection of bimetallic element

|  | H01H 37/54 |
· · · · | wherein the bimetallic element is inherently snap acting

|  | H01H 37/56 |
· · · · | having spirally wound or helically wound bimetallic element

|  | H01H 37/58 |
· · · | actuated due to thermally controlled change of magnetic permeability

|  | H01H 37/60 |
· · | Means for producing snap action (inherent in bimetallic element Fulltext... Hierarchy... Expanded...H01H 37/54; caused by a magnet Fulltext... Hierarchy... Expanded...H01H 37/66)

|  | H01H 37/62 |
· · | Means other than thermal means for introducing a predetermined time delay

|  | H01H 37/64 |
· · | Contacts

|  | H01H 37/66 |
· · · | Magnetic reinforcement of contact pressure; Magnet causing snap action

|  | H01H 37/68 |
· · · | sealed in evacuated or gas-filled tube

|  | H01H 37/70 |
· · · | Resetting means

|  | H01H 37/72 |
· | Switches in which the opening movement and the closing movement of a contact are effected respectively by heating and cooling or vice versa

|  | H01H 37/74 |
· | Switches in which only the opening movement or only the closing movement of a contact is effected by heating or cooling (for the electrical protection of electric lines or electric apparatus Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 73/00-H01H 83/00)

|  | H01H 37/76 |
· · | Contact member actuated by melting of fusible material, actuated due to burning of combustible material or due to explosion of explosive material (fuses Fulltext... Hierarchy... Expanded...H01H 85/00)

|  | H01H 39/00 |
Switching devices actuated by an explosion produced within the device and initiated by an electric current

|  | H01H 41/00 |
Switches providing a selected number of consecutive operations of the contacts by a single manual actuation of the operating part (for telephone communication Fulltext... Hierarchy... Expanded...H04M 1/26)

|  | H01H 41/04 |
· | Switches without means for setting or mechanically storing a multidigit number

|  | H01H 41/06 |
· · | dial or slide operated

|  | H01H 41/08 |
· · | keyboard operated

|  | H01H 41/10 |
· | Switches with means for setting or mechanically storing a multidigit number

|  | H01H 41/12 |
· · | dial or slide operated

|  | H01H 41/14 |
· · | keyboard operated

|  | H01H 43/00 |
Time or time-programme switches providing a choice of time-intervals for executing one or more switching actions and automatically terminating their operation after the programme is completed (clocks with attached or built-in means operating any device at preselected times or after preselected time intervals Fulltext... Hierarchy... Expanded...G04C 23/00; programme-control systems Fulltext... Hierarchy... Expanded...G05B 19/00)

|  | H01H 43/02 |
· | Details

|  | H01H 43/04 |
· · | Means for time setting

|  | H01H 43/06 |
· · · | comprising separately adjustable parts for each programme step, e.g. with tappets

|  | H01H 43/08 |
· · · | comprising an interchangeable programme part which is common for all programme steps, e.g. with a punched card

|  | H01H 43/10 |
· | with timing of actuation of contacts due to a part rotating at substantially constant speed

|  | H01H 43/12 |
· · | stopping automatically after a single cycle of operation

|  | H01H 43/14 |
· · · | wherein repetition of operation necessitates resetting of time intervals

|  | H01H 43/16 |
· · | stopping automatically after a predetermined plurality of cycles of operation

|  | H01H 43/24 |
· | with timing of actuation of contacts due to a non-rotatably moving part

|  | H01H 43/26 |
· · | the actuation being produced by a substance flowing due to gravity, e.g. sand, water

|  | H01H 43/28 |
· · | the actuation being produced by a part, the speed of which is controlled by fluid-pressure means, e.g. by piston and cylinder

|  | H01H 43/30 |
· | with timing of actuation of contacts due to thermal action

|  | H01H 43/32 |
· | with timing of actuation of contacts due to electrolytic processes; with timing of actuation of contacts due to chemical processes

|  | H01H 45/00 - H01H 61/00 |
Relays

|  | H01H 45/00 |
Details of relays (electric circuit arrangements Fulltext... Hierarchy... Expanded...H01H 47/00; of electromagnetic relays Fulltext... Hierarchy... Expanded...H01H 50/00; details of electrically-operated selector switches Fulltext... Hierarchy... Expanded...H01H 63/00)

|  | H01H 45/02 |
· | Bases; Casings; Covers (frames for mounting two or more relays or for mounting a relay and another electric component Fulltext... Hierarchy... Expanded...H02B 1/01, Fulltext... Hierarchy... Expanded...H04Q 1/08, Fulltext... Hierarchy... Expanded...H05K)

|  | H01H 45/04 |
· · | Mounting complete relay or separate parts of relay on a base or inside a case

|  | H01H 45/06 |
· · | having windows; Transparent cases or covers

|  | H01H 45/08 |
· | Indicators; Distinguishing marks

|  | H01H 45/10 |
· | Electromagnetic or electrostatic shielding (casings Fulltext... Hierarchy... Expanded...H01H 45/02)

|  | H01H 45/12 |
· | Ventilating; Cooling; Heating (for operating electrothermal relays Fulltext... Hierarchy... Expanded...H01H 61/013)

|  | H01H 45/14 |
· | Terminal arrangements

|  | H01H 47/00 |
Circuit arrangements not adapted to a particular application of the relay and designed to obtain desired operating characteristics or to provide energising current (circuit arrangements for electromagnets in general Fulltext... Hierarchy... Expanded...H01F 7/18)

|  | H01H 47/02 |
· | for modifying the operation of the relay

|  | H01H 47/04 |
· · | for holding armature in attracted position, e.g. when initial energising circuit is interrupted; for maintaining armature in attracted position, e.g. with reduced energising current

|  | H01H 47/06 |
· · · | by changing number of serially-connected turns or winding

|  | H01H 47/08 |
· · · | by changing number of parallel-connected turns or windings

|  | H01H 47/10 |
· · · | by switching-in or -out impedance external to the relay winding

|  | H01H 47/12 |
· · | for biasing the electromagnet

|  | H01H 47/14 |
· · | for differential operation of the relay

|  | H01H 47/16 |
· · | for conjoint, e.g. additive, operation of the relay

|  | H01H 47/18 |
· · | for introducing delay in the operation of the relay (short-circuited conducting sleeves, bands, or discs Fulltext... Hierarchy... Expanded...H01H 50/46)

|  | H01H 47/20 |
· · | for producing frequency-selective operation of the relay

|  | H01H 47/22 |
· | for supplying energising current for relay coil

|  | H01H 47/24 |
· · | having light-sensitive input

|  | H01H 47/26 |
· · | having thermo-sensitive input

|  | H01H 47/28 |
· · | Energising current supplied by discharge tube

|  | H01H 47/30 |
· · · | by gas-filled discharge tube

|  | H01H 47/32 |
· · | Energising current supplied by semiconductor device

|  | H01H 47/34 |
· · | Energising current supplied by magnetic amplifier

|  | H01H 47/36 |
· · | Relay coil or coils forming part of a bridge circuit

|  | H01H 49/00 |
Apparatus or processes specially adapted to the manufacture of relays or parts thereof

|  | H01H 50/00 |
Details of electromagnetic relays (electric circuit arrangements Fulltext... Hierarchy... Expanded...H01H 47/00; details of electrically-operated selector switches Fulltext... Hierarchy... Expanded...H01H 63/00)

|  | H01H 50/02 |
· | Bases; Casings; Covers (frames for mounting two or more relays or for mounting a relay and another electric component Fulltext... Hierarchy... Expanded...H02B 1/01, Fulltext... Hierarchy... Expanded...H04Q 1/08, Fulltext... Hierarchy... Expanded...H05K)

|  | H01H 50/04 |
· · | Mounting complete relay or separate parts of relay on a base or inside a case

|  | H01H 50/06 |
· · | having windows; Transparent cases or covers

|  | H01H 50/08 |
· | Indicators; Distinguishing marks

|  | H01H 50/10 |
· | Electromagnetic or electrostatic shielding (casings Fulltext... Hierarchy... Expanded...H01H 50/02)

|  | H01H 50/12 |
· | Ventilating; Cooling; Heating (for operating electrothermal relays Fulltext... Hierarchy... Expanded...H01H 61/013)

|  | H01H 50/14 |
· | Terminal arrangements

|  | H01H 50/16 |
· | Magnetic circuit arrangements (cores, yokes, or armatures in general Fulltext... Hierarchy... Expanded...H01F 3/00; magnets in general Fulltext... Hierarchy... Expanded...H01F 7/00)

|  | H01H 50/18 |
· · | Movable parts of magnetic circuits, e.g. armature

|  | H01H 50/20 |
· · · | movable inside coil and substantially lengthwise with respect to axis thereof; movable coaxially with respect to coil

|  | H01H 50/22 |
· · · · | wherein the magnetic circuit is substantially closed

|  | H01H 50/24 |
· · · | Parts rotatable or rockable outside coil

|  | H01H 50/26 |
· · · · | Parts movable about a knife edge

|  | H01H 50/28 |
· · · · | Parts movable due to bending of a blade spring or reed

|  | H01H 50/30 |
· · · | Mechanical arrangements for preventing or damping vibration or shock, e.g. by balancing of armature

|  | H01H 50/32 |
· · · | Latching movable parts mechanically

|  | H01H 50/34 |
· · · | Means for adjusting limits of movement; Mechanical means for adjusting returning force

|  | H01H 50/36 |
· · | Stationary parts of magnetic circuit, e.g. yoke

|  | H01H 50/38 |
· · · | Part of main magnetic circuit shaped to suppress arcing between the contacts of the relay

|  | H01H 50/40 |
· · · | Branched or mutiple-limb main magnetic circuits

|  | H01H 50/42 |
· · · | Auxiliary magnetic circuits, e.g. for maintaining armature in, or returning armature to, position of rest, for damping or accelerating movement

|  | H01H 50/44 |
· | Magnetic coils or windings (circuit arrangements Fulltext... Hierarchy... Expanded...H01H 47/00; in general Fulltext... Hierarchy... Expanded...H01F 5/00)

|  | H01H 50/46 |
· · | Short-circuited conducting sleeves, bands, or discs

|  | H01H 50/54 |
· | Contact arrangements (contacts for switches in general Fulltext... Hierarchy... Expanded...H01H 1/00)

|  | H01H 50/56 |
· · | Contact spring sets

|  | H01H 50/58 |
· · · | Driving arrangements structurally associated therewith; Mounting of driving arrangement on armature

|  | H01H 50/60 |
· · | moving contact being rigidly combined with movable part of magnetic circuit

|  | H01H 50/62 |
· · | Co-operating movable contacts operated by separate electrical actuating means

|  | H01H 50/64 |
· | Driving arrangements between movable part of magnetic circuit and contact (structurally associated with contact spring sets Fulltext... Hierarchy... Expanded...H01H 50/58)

|  | H01H 50/66 |
· · | with lost motion

|  | H01H 50/68 |
· · | with snap action

|  | H01H 50/70 |
· · | operating contact momentarily during stroke of armature

|  | H01H 50/72 |
· · | for mercury contact

|  | H01H 50/74 |
· · | Mechanical means for producing a desired natural frequency of operation of the contacts, e.g. for self-interrupter

|  | H01H 50/76 |
· · · | using reed or blade spring

|  | H01H 50/78 |
· · · | using diaphragm; using stretched wire or ribbon vibrating sideways

|  | H01H 50/80 |
· · · | using torsionally vibrating member, e.g. wire, strip

|  | H01H 50/82 |
· · · | using spring-loaded pivoted inertia member

|  | H01H 50/84 |
· · · | with means for adjustment of frequency or of make-to-break ratio

|  | H01H 50/86 |
· | Means for introducing a predetermined time delay between the initiation of the switching operation and the opening or closing of the contacts (circuit arrangements for introducing delay Fulltext... Hierarchy... Expanded...H01H 47/18; short-circuited conducting sleeves, bands, or discs Fulltext... Hierarchy... Expanded...H01H 50/46)

|  | H01H 50/88 |
· · | Mechanical means, e.g. dash-pot

|  | H01H 50/90 |
· · · | the delay being effective in both directions of operation

|  | H01H 50/92 |
· · | Thermal means (inherent in electrothermal relays Fulltext... Hierarchy... Expanded...H01H 61/00)

|  | H01H 51/00 |
Electromagnetic relays (relays using the dynamo-electric effect Fulltext... Hierarchy... Expanded...H01H 53/00)

|  | H01H 51/01 |
· | Relays in which the armature is maintained in one position by a permanent magnet and freed by energisation of a coil producing an opposing magnetic field [3]

|  | H01H 51/02 |
· | Non-polarised relays (Fulltext... Hierarchy... Expanded...H01H 51/01 takes precedence) [3]

|  | H01H 51/04 |
· · | with single armature; with single set of ganged armatures

|  | H01H 51/06 |
· · · | Armature is movable between two limit positions of rest and is moved in one direction due to energisation of an electromagnet and after the electromagnet is de-energised is returned by energy stored during the movement in the first direction, e.g. by using a spring, by using a permanent magnet, by gravity

|  | H01H 51/08 |
· · · · | Contacts alternately opened and closed by successive cycles of energisation and de-energisation of the electromagnet, e.g. by use of a ratchet

|  | H01H 51/10 |
· · · · | Contacts retained open or closed by a mechanical latch which is controlled by an electromagnet

|  | H01H 51/12 |
· · · | Armature is movable between two limit positions of rest and is moved in both directions due to the energisation of one or the other of two electromagnets without the storage of energy to effect the return movement

|  | H01H 51/14 |
· · · · | without intermediate neutral position of rest

|  | H01H 51/16 |
· · · · | with intermediate neutral position of rest

|  | H01H 51/18 |
· · · | Armature is rotatable through an unlimited number of revolutions

|  | H01H 51/20 |
· · | with two or more independent armatures

|  | H01H 51/22 |
· | Polarised relays

|  | H01H 51/24 |
· · | without intermediate neutral position of rest

|  | H01H 51/26 |
· · | with intermediate neutral position of rest

|  | H01H 51/27 |
· | Relays with armature having two stable magnetic states and operated by change from one state to the other

|  | H01H 51/28 |
· | Relays having both armature and contacts within a sealed casing outside which the operating coil is located, e.g. contact carried by a magnetic leaf spring or reed (Fulltext... Hierarchy... Expanded...H01H 51/27 takes precedence)

|  | H01H 51/29 |
· | Relays having armature, contacts, and operating coil within a sealed casing (Fulltext... Hierarchy... Expanded...H01H 51/27 takes precedence)

|  | H01H 51/30 |
· | specially adapted for actuation by ac

|  | H01H 51/32 |
· · | Frequency relays; Mechanically-tuned relays

|  | H01H 51/34 |
· | Self-interrupters, i.e. with periodic or other repetitive opening and closing of contacts

|  | H01H 51/36 |
· · | wherein the make-to-break ratio is varied by hand setting or current strength

|  | H01H 53/00 |
Relays using the dynamo-electric effect, i.e. relays in which contacts are opened or closed due to relative movement of current-carrying conductor and magnetic field caused by force of interaction between them

|  | H01H 53/01 |
· | Details

|  | H01H 53/015 |
· · | Moving coils; Contact-driving arrangements associated therewith

|  | H01H 53/02 |
· | Electrodynamic relays, i.e. relays in which the interaction is between two current-carrying conductors

|  | H01H 53/04 |
· · | Ferrodynamic relays, i.e. relays in which the magnetic field is concentrated in ferromagnetic parts

|  | H01H 53/06 |
· | Magnetodynamic relays, i.e. relays in which the magnetic field is produced by a permanent magnet

|  | H01H 53/08 |
· | wherein a mercury contact constitutes the current-carrying conductor

|  | H01H 53/10 |
· | Induction relays, i.e. relays in which the interaction is between a magnetic field and current induced thereby in a conductor

|  | H01H 53/12 |
· · | Ferraris relays

|  | H01H 53/14 |
· | Contacts actuated by an electric motor through fluid-pressure transmission, e.g. using a motor-driven pump

|  | H01H 55/00 |
Magnetostrictive relays

|  | H01H 57/00 |
Electrostrictive relays; Piezo-electric relays

|  | H01H 59/00 |
Electrostatic relays; Electro-adhesion relays (clutches in general using the Johnson-Rahbek effect Fulltext... Hierarchy... Expanded...H02N 13/00)

|  | H01H 61/00 |
Electrothermal relays (thermal switches not operated by electrical input, thermal switches with anticipating electrical input Fulltext... Hierarchy... Expanded...H01H 37/00; thermally-sensitive members Fulltext... Hierarchy... Expanded...H01H 37/32)

|  | H01H 61/01 |
· | Details

|  | H01H 61/013 |
· · | Heating arrangements for operating relays

|  | H01H 61/017 |
· · · | Heating by glow discharge or arc in confined space

|  | H01H 61/02 |
· | wherein the thermally-sensitive member is heated indirectly, e.g. resistively, inductively

|  | H01H 61/04 |
· | wherein the thermally-sensitive member is only heated directly

|  | H01H 61/06 |
· | Self-interrupters, i.e. with periodic or other repetitive opening and closing of contacts

|  | H01H 61/08 |
· · | wherein the make-to-break ratio is varied by hand setting or current strength

|  | H01H 63/00 - H01H 67/00 |
Selectors [3]

|  | H01H 63/00 |
Details of electrically-operated selector switches (details of relays Fulltext... Hierarchy... Expanded...H01H 45/00)

|  | H01H 63/02 |
· | Contacts; Wipers; Connections thereto

|  | H01H 63/04 |
· · | Contact-making or contact-breaking wipers; Position indicators therefor

|  | H01H 63/06 |
· · | Contact banks

|  | H01H 63/08 |
· · · | cylindrical

|  | H01H 63/10 |
· · · | plane

|  | H01H 63/12 |
· · | Multiplying connections to contact banks, e.g. using ribbon cables

|  | H01H 63/14 |
· · · | without soldering

|  | H01H 63/16 |
· | Driving arrangements for multi-position wipers

|  | H01H 63/18 |
· · | with step-by-step motion of wiper to a selector position

|  | H01H 63/20 |
· · · | using stepping magnet and ratchet

|  | H01H 63/22 |
· · · | using step-by-step electromagnetic drive without ratchet, e.g. self-interrupting driving magnet

|  | H01H 63/24 |
· · | with continuous motion of wiper until a selected position is reached

|  | H01H 63/26 |
· · · | with an individual clutch-drive from a shaft common to more than one selector switch

|  | H01H 63/28 |
· · · | with an individual motor for each selector switch

|  | H01H 63/30 |
· · · · | Pneumatic motor for moving wiper to selected position

|  | H01H 63/32 |
· · · · | Spring motor for moving wiper to selected position

|  | H01H 63/33 |
· | Constructional details of co-ordinate-type selector switches not having relays at cross-points

|  | H01H 63/34 |
· | Bases; Cases; Covers; Mountings (racks for mounting selectors with or without other exchange equipment Fulltext... Hierarchy... Expanded...H04Q 1/04); Mounting of fuses on selector switch

|  | H01H 63/36 |
· | Circuit arrangements for ensuring correct or desired operation and not adapted to a particular application of the selector switch

|  | H01H 63/38 |
· · | for multi-position wiper switches

|  | H01H 63/40 |
· · | for multi-position switches without wipers

|  | H01H 63/42 |
· · · | for co-ordinate-type selector switches not having relays at cross-points

|  | H01H 65/00 |
Apparatus or processes specially adapted to the manufacture of selector switches or parts thereof

|  | H01H 67/00 |
Electrically-operated selector switches (details thereof Fulltext... Hierarchy... Expanded...H01H 63/00; selecting in general Fulltext... Hierarchy... Expanded...H04Q)

|  | H01H 67/02 |
· | Multi-position wiper switches

|  | H01H 67/04 |
· · | having wipers movable only in one direction for purpose of selection

|  | H01H 67/06 |
· · · | Rotary switches, i.e. having angularly movable wipers

|  | H01H 67/08 |
· · · · | with wiper selection

|  | H01H 67/10 |
· · · · | with coarse and fine positioning of wipers

|  | H01H 67/12 |
· · · | Linear-motion switches

|  | H01H 67/14 |
· · | having wipers movable in two mutually perpendicular directions for purpose of selection

|  | H01H 67/16 |
· · · | one motion being rotary and the other being parallel to the axis of rotation, e.g. Strowger or "up and around" switches

|  | H01H 67/18 |
· · · | one motion being rotary and the other being perpendicular to the axis of rotation, e.g. "round and in" switches

|  | H01H 67/20 |
· · · | both motions being linear

|  | H01H 67/22 |
· | Switches without multi-position wipers

|  | H01H 67/24 |
· · | Co-ordinate-type relay switches having an individual electromagnet at each cross-point

|  | H01H 67/26 |
· · | Co-ordinate-type selector switches not having relays at cross-points but involving mechanical movement, e.g. cross-bar switch, code-bar switch

|  | H01H 67/30 |
· · | Co-ordinate-type selector switches with field of co-ordinate coil acting directly upon magnetic leaf spring or reed-type contact member

|  | H01H 67/32 |
· · | having a multiplicity of interdependent armatures operated in succession by a single coil and each controlling one contact or set of contacts, e.g. counting relay

|  | H01H 69/00 - H01H 87/00 |
Emergency protective devices

|  | H01H 69/00 |
Apparatus or processes for the manufacture of emergency protective devices (manufacture of switches in general Fulltext... Hierarchy... Expanded...H01H 11/00; manufacture of relays in general Fulltext... Hierarchy... Expanded...H01H 49/00)

|  | H01H 69/01 |
· | for calibrating or setting of devices to function under predetermined conditions (measuring electric values Fulltext... Hierarchy... Expanded...G01R)

|  | H01H 69/02 |
· | Manufacture of fuses

|  | H01H 71/00 |
Details of the protective switches or relays covered by groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 73/00-H01H 83/00

|  | H01H 71/02 |
· | Housings; Casings; Bases; Mountings

|  | H01H 71/04 |
· | Means for indicating condition of the switching device

|  | H01H 71/06 |
· | Distinguishing marks, e.g. colour coding

|  | H01H 71/08 |
· | Terminals; Connections (in general Fulltext... Hierarchy... Expanded...H01R)

|  | H01H 71/10 |
· | Operating or release mechanisms

|  | H01H 71/12 |
· · | Automatic release mechanisms with or without manual release

|  | H01H 71/14 |
· · · | Electrothermal mechanisms

|  | H01H 71/16 |
· · · · | with bimetal element

|  | H01H 71/18 |
· · · · | with expanding rod, strip, or wire

|  | H01H 71/20 |
· · · · | with fusible mass

|  | H01H 71/22 |
· · · · | with compensation for variation of ambient temperature

|  | H01H 71/24 |
· · · | Electromagnetic mechanisms

|  | H01H 71/26 |
· · · · | with windings acting in opposition

|  | H01H 71/28 |
· · · · | with windings acting in conjunction

|  | H01H 71/30 |
· · · · | having additional short-circuited winding

|  | H01H 71/32 |
· · · · | having permanently magnetised part

|  | H01H 71/34 |
· · · · | having two or more armatures controlled by a common winding

|  | H01H 71/36 |
· · · · | frequency selective

|  | H01H 71/38 |
· · · · | wherein the magnet coil also acts as arc blow-out device

|  | H01H 71/40 |
· · · | Combined electrothermal and electromagnetic mechanisms

|  | H01H 71/42 |
· · · | Induction-motor, induced-current, or electrodynamic release mechanisms

|  | H01H 71/43 |
· · · · | Electrodynamic release mechanisms

|  | H01H 71/44 |
· · · | having means for introducing a predetermined time delay (by short-circuited winding Fulltext... Hierarchy... Expanded...H01H 71/30; by additional armature Fulltext... Hierarchy... Expanded...H01H 71/34)

|  | H01H 71/46 |
· · · | having means for operating auxiliary contacts additional to the main contacts

|  | H01H 71/48 |
· · · · | with provision for short-circuiting the electrical input to the release mechanism after release of the switch, e.g. for protection of heating wire

|  | H01H 71/50 |
· · | Manual reset mechanisms

|  | H01H 71/52 |
· · · | actuated by lever

|  | H01H 71/54 |
· · · | actuated by tumbler

|  | H01H 71/56 |
· · · | actuated by rotatable knob or wheel

|  | H01H 71/58 |
· · · | actuated by push-button, pull-knob, or slide

|  | H01H 71/60 |
· · · | actuated by closure of switch casing

|  | H01H 71/62 |
· · · | with means for preventing resetting while abnormal condition persists, e.g. loose handle arrangement

|  | H01H 71/64 |
· · · · | incorporating toggle linkage

|  | H01H 71/66 |
· · | Power reset mechanisms

|  | H01H 71/68 |
· · · | actuated by electromagnet

|  | H01H 71/70 |
· · · | actuated by electric motor

|  | H01H 71/72 |
· · · | actuated automatically a limited number of times

|  | H01H 71/74 |
· | Means for adjusting the conditions under which the device will function to provide protection

|  | H01H 73/00 |
Protective overload circuit-breaking switches in which excess current opens the contacts by automatic release of mechanical energy stored by previous operation of a hand reset mechanism

|  | H01H 73/02 |
· | Details

|  | H01H 73/04 |
· · | Contacts

|  | H01H 73/06 |
· · | Housings; Casings; Bases; Mountings

|  | H01H 73/08 |
· · · | Plug-in housings

|  | H01H 73/10 |
· · · | Cartridge housings, e.g. screw-in housing

|  | H01H 73/12 |
· · | Means for indicating condition of the switch

|  | H01H 73/14 |
· · · | Indicating lamp structurally associated with the switch

|  | H01H 73/16 |
· · | Distinguishing marks, e.g. colour coding

|  | H01H 73/18 |
· · | Means for extinguishing or suppressing arc

|  | H01H 73/20 |
· · | Terminals; Connections (in general Fulltext... Hierarchy... Expanded...H01R)

|  | H01H 73/22 |
· | having electrothermal release and no other automatic release (cartridge type Fulltext... Hierarchy... Expanded...H01H 73/62)

|  | H01H 73/24 |
· · | reset by lever

|  | H01H 73/26 |
· · | reset by tumbler

|  | H01H 73/28 |
· · | reset by rotatable knob or wheel

|  | H01H 73/30 |
· · | reset by push-button, pull-knob, or slide

|  | H01H 73/32 |
· · | reset by closure of switch casing

|  | H01H 73/34 |
· · | reset action requiring replacement or reconditioning of a fusible or explosive part

|  | H01H 73/36 |
· | having electromagnetic release and no other automatic release (cartridge type Fulltext... Hierarchy... Expanded...H01H 73/64)

|  | H01H 73/38 |
· · | reset by lever

|  | H01H 73/40 |
· · | reset by tumbler

|  | H01H 73/42 |
· · | reset by rotatable knob or wheel

|  | H01H 73/44 |
· · | reset by push-button, pull-knob, or slide

|  | H01H 73/46 |
· · | reset by closure of switch casing

|  | H01H 73/48 |
· | having both electrothermal and electromagnetic automatic release (cartridge type Fulltext... Hierarchy... Expanded...H01H 73/66)

|  | H01H 73/50 |
· · | reset by lever

|  | H01H 73/52 |
· · | reset by tumbler

|  | H01H 73/54 |
· · | reset by rotatable knob or wheel

|  | H01H 73/56 |
· · | reset by push-button, pull-knob, or slide

|  | H01H 73/58 |
· · | reset by closure of switch casing

|  | H01H 73/60 |
· | cartridge type, e.g. screw-in cartridge

|  | H01H 73/62 |
· · | having only electrothermal release

|  | H01H 73/64 |
· · | having only electromagnetic release

|  | H01H 73/66 |
· · | having combined electrothermal and electromagnetic release

|  | H01H 75/00 |
Protective overload circuit-breaking switches in which excess current opens the contacts by automatic release of mechanical energy stored by previous operation of power reset mechanism

|  | H01H 75/02 |
· | Details

|  | H01H 75/04 |
· · | Reset mechanisms for automatically reclosing a limited number of times (circuit arrangements Fulltext... Hierarchy... Expanded...H02H 3/06)

|  | H01H 75/06 |
· · · | effecting one reclosing action only

|  | H01H 75/08 |
· | having only electrothermal release

|  | H01H 75/10 |
· | having only electromagnetic release

|  | H01H 75/12 |
· | having combined electrothermal and electromagnetic release

|  | H01H 77/00 |
Protective overload circuit-breaking switches operated by excess current and requiring separate action for resetting (Fulltext... Hierarchy... Expanded...H01H 73/00, Fulltext... Hierarchy... Expanded...H01H 75/00 take precedence)

|  | H01H 77/02 |
· | in which the excess current itself provides the energy for opening the contacts, and having a separate reset mechanism

|  | H01H 77/04 |
· · | with electrothermal opening

|  | H01H 77/06 |
· · | with electromagnetic opening

|  | H01H 77/08 |
· · · | retained closed by permanent or remanent magnetism and opened by windings acting in opposition

|  | H01H 77/10 |
· · | with electrodynamic opening

|  | H01H 79/00 |
Protective switches in which excess current causes the closing of contacts, e.g. for short-circuiting the apparatus to be protected

|  | H01H 81/00 |
Protective switches in which contacts are normally closed but are repeatedly opened and reclosed as long as a condition causing excess current persists, e.g. for current limiting

|  | H01H 81/02 |
· | electrothermally-operated

|  | H01H 81/04 |
· | electromagnetically-operated

|  | H01H 83/00 |
Protective switches, e.g. circuit-breaking switches, or protective relays operated by abnormal electrical conditions otherwise than solely by excess current

|  | H01H 83/02 |
· | operated by earth fault currents (Fulltext... Hierarchy... Expanded...H01H 83/14 takes precedence)

|  | H01H 83/04 |
· · | with testing means for indicating the ability of the switch or relay to function properly

|  | H01H 83/06 |
· | operated by current falling below a predetermined value

|  | H01H 83/08 |
· | operated by reversal of dc

|  | H01H 83/10 |
· | operated by excess voltage, e.g. for lightning protection

|  | H01H 83/12 |
· | operated by voltage falling below a predetermined value, e.g. for no-volt protection

|  | H01H 83/14 |
· | operated by unbalance of two or more currents or voltages, e.g. for differential protection

|  | H01H 83/16 |
· | operated by abnormal ratio of voltage and current, e.g. distance relay

|  | H01H 83/18 |
· | operated by abnormal product of, or abnormal phase angle between, voltage and current, e.g. directional relay

|  | H01H 83/20 |
· | operated by excess current as well as by some other abnormal electrical condition

|  | H01H 83/22 |
· · | the other condition being unbalance of two or more currents or voltages

|  | H01H 85/00 |
Protective devices in which the current flows through a part of fusible material and this current is interrupted by displacement of the fusible material when this current becomes excessive (switches actuated by melting of fusible material Fulltext... Hierarchy... Expanded...H01H 37/76; automatic release of protective switches due to fusion of a mass Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 73/00-H01H 83/00; disposition or arrangement of fuses on boards Fulltext... Hierarchy... Expanded...H02B 1/18)

|  | H01H 85/02 |
· | Details (electrical connections in general Fulltext... Hierarchy... Expanded...H01R)

|  | H01H 85/04 |
· · | Fuses, i.e. expendable parts of the protective device, e.g. cartridges

|  | H01H 85/041 |
· · · | characterised by the type [5]

|  | H01H 85/042 |
· · · · | General constructions or structure of high voltage fuses, i.e. above 1,000 V [5]

|  | H01H 85/044 |
· · · · | General constructions or structure of low voltage fuses, i.e. below 1,000 V, or of fuses where the applicable voltage is not specified (Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 85/046-H01H 85/048 take precedence) [5]

|  | H01H 85/0445 |
· · · · · | fast or slow type (Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...H01H 85/045-H01H 85/048 take precedence) [5]

|  | H01H 85/045 |
· · · · · | cartridge type [5]

|  | H01H 85/046 |
· · · · | Fuses formed as printed circuits [5]

|  | H01H 85/047 |
· · · · | Vacuum fuses [5]

|  | H01H 85/048 |
· · · · | Fuse resistors [5]

|  | H01H 85/05 |
· · · | Component parts thereof [5]

|  | H01H 85/055 |
· · · · | Fusible members [5]

|  | H01H 85/06 |
· · · · · | characterised by the fusible material (Fulltext... Hierarchy... Expanded...H01H 85/11 takes precedence) [5]

|  | H01H 85/08 |
· · · · · | characterised by the shape or form of the fusible member [5]

|  | H01H 85/10 |
· · · · · · | with constriction for localised fusing (Fulltext... Hierarchy... Expanded...H01H 85/11 takes precedence) [5]

|  | H01H 85/11 |
· · · · · · | with applied local area of a metal which, on melting, forms a eutectic with the main material of the fusible member, i.e. M-effect devices [5]

|  | H01H 85/12 |
· · · · · | Two or more separate fusible members in parallel [5]

|  | H01H 85/143 |
· · · · | Electrical contacts; Fastening fusible members to such contacts [5]

|  | H01H 85/147 |
· · · · · | Parallel-side contacts [5]

|  | H01H 85/15 |
· · · · · | Screw-in contacts [5]

|  | H01H 85/153 |
· · · · · | Knife-blade-end contacts [5]

|  | H01H 85/157 |
· · · · · | Ferrule-end contacts [5]

|  | H01H 85/165 |
· · · · | Casings (electrical contacts Fulltext... Hierarchy... Expanded...H01H 85/143; fillings Fulltext... Hierarchy... Expanded...H01H 85/18) [5]

|  | H01H 85/17 |
· · · · · | characterised by the casing material [5]

|  | H01H 85/175 |
· · · · · | characterised by the casing shape or form [5]

|  | H01H 85/18 |
· · · · | Casing fillings, e.g. powder

|  | H01H 85/20 |
· · | Bases for supporting the fuse; Separate parts thereof (bases, casings for connectors, in general Fulltext... Hierarchy... Expanded...H01R)

|  | H01H 85/22 |
· · | Intermediate or auxiliary parts for carrying, holding, or retaining fuse, co-operating with base or fixed holder, and removable therefrom for renewing the fuse

|  | H01H 85/24 |
· · | Means for preventing insertion of incorrect fuse

|  | H01H 85/25 |
· · | Safety arrangements preventing or inhibiting contact with live parts, including operation of isolation on removal of cover (interlocking between casing or protective shutter of a switch and mechanism for operating its contacts Fulltext... Hierarchy... Expanded...H01H 9/22) [5]

|  | H01H 85/26 |
· · | Magazine arrangements

|  | H01H 85/28 |
· · · | effecting automatic replacement

|  | H01H 85/30 |
· · | Means for indicating condition of fuse structurally associated with the fuse

|  | H01H 85/32 |
· · · | Indicating lamp structurally associated with the protective device

|  | H01H 85/34 |
· · | Distinguishing marks, e.g. colour coding

|  | H01H 85/36 |
· · | Means for applying mechanical tension to fusible member

|  | H01H 85/38 |
· · | Means for extinguishing or suppressing arc (by powder filling Fulltext... Hierarchy... Expanded...H01H 85/18; by mechanical tension applied to fusible member Fulltext... Hierarchy... Expanded...H01H 85/36)

|  | H01H 85/40 |
· · · | using an arc-extinguishing liquid (characterised by the composition of the liquid Fulltext... Hierarchy... Expanded...H01H 33/22)

|  | H01H 85/42 |
· · · | using an arc-extinguishing gas (characterised by the composition of the gas Fulltext... Hierarchy... Expanded...H01H 33/22)

|  | H01H 85/43 |
· · | Means for exhausting or absorbing gases liberated by fusing arc, or for ventilating excess pressure generated by heating [5]

|  | H01H 85/44 |
· · | Structural association with spark-gap arrester

|  | H01H 85/46 |
· · | Circuit arrangements not adapted to a particular application of the protective device

|  | H01H 85/47 |
· · | Means for cooling [5]

|  | H01H 85/48 |
· | Protective devices wherein the fuse is carried or held directly by the base

|  | H01H 85/50 |
· · | the fuse having contacts at opposite ends for co-operation with the base

|  | H01H 85/52 |
· · | the fuse being adapted for screwing into the base

|  | H01H 85/54 |
· | Protective devices wherein the fuse is carried, held, or retained by an intermediate or auxiliary part removable from the base, or used as sectionalisers

|  | H01H 85/56 |
· · | the intermediate or auxiliary part having side contacts for plugging into the base, e.g. bridge-carrier type

|  | H01H 85/58 |
· · · | with intermediate auxiliary part and base shaped to interfit and thereby enclose the fuse

|  | H01H 85/60 |
· · | the intermediate or auxiliary part having contacts at opposite ends for co-operation with the base

|  | H01H 85/62 |
· · | the intermediate or auxiliary part being adapted for screwing into the base

|  | H01H 87/00 |
Protective devices in which a current flowing through a liquid or solid is interrupted by the evaporation of the liquid or by the melting and evaporation of the solid when the current becomes excessive, the circuit continuity being reestablished on cooling [3]