|  | C |
SECTION C — CHEMISTRY; METALLURGY

|  | C |
Note(s) In section C, the definitions of groups of chemical elements are as follows: Alkali metals: Li, Na, K, Rb, Cs, Fr Alkaline earth metals: Ca, Sr, Ba, Ra Lanthanides: elements with atomic numbers 57 to 71 inclusive Rare earths: Sc, Y, Lanthanides Actinides: elements with atomic numbers 89 to 103 inclusive Refractory metals: Ti, V, Cr, Zr, Nb, Mo, Hf, Ta, W Halogens: F, Cl, Br, I, At Noble gases: He, Ne, Ar, Kr, Xe, Rn Platinum group: Os, Ir, Pt, Ru, Rh, Pd Noble metals: Ag, Au, Platinum group Light metals: alkali metals, alkaline earth metals, Be, Al, Mg Heavy metals: metals other than light metals Iron group: Fe, Co, Ni Non-metals: H, B, C, Si, N, P, O, S, Se, Te, noble gases, halogens Metals: elements other than non-metals Transition elements: elements with atomic numbers 21 to 30 inclusive, 39 to 48 inclusive, 57 to 80 inclusive, 89 upwards The following notes are meant to assist in the use of this part of the classification scheme. They must not be read as modifying in any way the elaborations. Section C covers: pure chemistry, which covers inorganic compounds, organic compounds, macromolecular compounds, and their methods of preparation; applied chemistry, which covers compositions containing the above compounds, such as: glass, ceramics, fertilisers, plastics compositions, paints, products of the petroleum industry. It also covers certain compositions on account of their having particular properties rendering them suitable for certain purposes, as in the case of explosives, dyestuffs, adhesives, lubricants, and detergents; certain marginal industries, such as the manufacture of coke and of solid or gaseous fuels, the production and refining of oils, fats and waxes, the fermentation industry (e.g., brewing and wine-making), the sugar industry; certain operations or treatments, which are either purely mechanical, e.g., the mechanical treatment of leather and skins, or partly mechanical, e.g., the treatment of water or the prevention of corrosion in general; metallurgy, ferrous or non-ferrous alloys. In the case of operations, treatments, products or articles having both a chemical and a non-chemical part or aspect, the general rule is that the chemical part or aspect is covered by section C. In some of these cases, the chemical part or aspect brings with it a non-chemical one, even though purely mechanical, because this latter aspect either is essential to the operation or treatment or constitutes an important element thereof. It has seemed, in fact, more logical not to dissociate the different parts or aspects of a coherent whole. This is the case for applied chemistry and for the industries, operations and treatments mentioned in Notes (1)(c), (d) and (e). For example, furnaces peculiar to the manufacture of glass are covered by class Fulltext... Hierarchy... Expanded...C03 and not by class Fulltext... Hierarchy... Expanded...F27. There are, however, some exceptions in which the mechanical (or non-chemical) aspect carries with it the chemical aspect, for example: Certain extractive processes, in subclass Fulltext... Hierarchy... Expanded...A61K; The chemical purification of air, in subclass Fulltext... Hierarchy... Expanded...A61L; Chemical methods of fire-fighting, in subclass Fulltext... Hierarchy... Expanded...A62D; Chemical processes and apparatus, in class Fulltext... Hierarchy... Expanded...B01; Impregnation of wood, in subclass Fulltext... Hierarchy... Expanded...B27K; Chemical methods of analysis or testing, in subclass Fulltext... Hierarchy... Expanded...G01N; Photographic materials and processes, in class Fulltext... Hierarchy... Expanded...G03, and, generally, the chemical treatment of textiles and the production of cellulose or paper, in section D. In still other cases, the pure chemical aspect is covered by section C and the applied chemical aspect by another section, such as A, B or F, e.g., the use of a substance or composition for: treatment of plants or animals, covered by subclass Fulltext... Hierarchy... Expanded...A01N; foodstuffs, covered by class Fulltext... Hierarchy... Expanded...A23; ammunition or explosives, covered by class Fulltext... Hierarchy... Expanded...F42. When the chemical and mechanical aspects are so closely interlocked that a neat and simple division is not possible, or when certain mechanical processes follow as a natural or logical continuation of a chemical treatment, section C may cover, in addition to the chemical aspect, a part only of the mechanical aspect, e.g., after-treatment of artificial stone, covered by class Fulltext... Hierarchy... Expanded...C04. In this latter case, a note or a reference is usually given to make the position clear, even if sometimes the division is rather arbitrary.

CHEMISTRY

|  | C06 |
EXPLOSIVES; MATCHES

|  | C06B |
EXPLOSIVE OR THERMIC COMPOSITIONS (blasting Fulltext... Hierarchy... Expanded...F42D); MANUFACTURE THEREOF; USE OF SINGLE SUBSTANCES AS EXPLOSIVES (compounds in general Fulltext... Hierarchy... Expanded...C01, Fulltext... Hierarchy... Expanded...C07 or Fulltext... Hierarchy... Expanded...C08) [2]

|  | C06B |
Note(s) This subclass covers: compositions which are: explosive: compositions included are those containing both a fuel and sufficient oxidiser so that, upon initiation, they are capable of undergoing a chemical change of a relatively high rate of speed, resulting in the production of usable force for blasting, firearms, propelling missiles, or the like; [2] thermic: compositions included have (i) a consumable fuel component which consists of any element which is a metal, B, Si, Se or Te, or mixtures, intercompounds, or hydrides thereof; and (ii) in combination an oxidant component which is either a metal oxide or a salt (organic or inorganic) capable of yielding a metal oxide on decomposition; [2] fuels for rocket engines and intended for reaction with an oxidant, excluding air, in order to provide thrust for motive power purposes; [2] for use in affecting the explosion environment, e.g. for neutralising the poisonous gases of explosives, for cooling the explosion gases, or the like; [2] methods or apparatus for preparing or treating such compositions not otherwise provided for; [2] methods of using single substances as explosives. [2] In this subclass, the following term is used with the meaning indicated: "nitrated" covers compounds having a nitro group or a nitrate ester group. [2] Methods or apparatus for preparing or treating such compositions are classified according to the particular components of the compositions. [2]

|  | C06B |
Subclass index
EXPLOSIVE OR THERMIC COMPOSITIONS |
Containing nitrated derivatives |
inorganic | 31/00
organic | 25/00, 41/00
Containing nitrides or fulminates | 35/00, 37/00
Containing chlorates or perchlorates | 29/00
Containing metal | 27/00, 33/00
Containing phosphorus | 39/00
Other compositions | 23/00, 43/00
Compositions defined by the structure or arrangement of the components | 45/00, 47/00
USE OF A SINGLE SUBSTANCE AS AN EXPLOSIVE | 49/00
MANUFACTURE | 21/00

|  | C06B 21/00 |
Apparatus or methods for working-up explosives, e.g. forming, cutting, drying

|  | C06B 23/00 - C06B 49/00 |
Note(s) In groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...C06B 23/00-C06B 49/00, in the absence of an indication to the contrary, a composition is classified in the last place that provides for an ingredient. [2]

|  | C06B 23/00 |
Compositions characterised by non-explosive or non-thermic constituents [2]

|  | C06B 23/02 |
· | for neutralising poisonous gases from explosives produced during blasting [2]

|  | C06B 23/04 |
· | for cooling the explosion gases [2]

|  | C06B 25/00 |
Compositions containing a nitrated organic compound [2]

|  | C06B 25/02 |
· | the nitrated compound being starch or sugar [2]

|  | C06B 25/04 |
· | the nitrated compound being an aromatic [2]

|  | C06B 25/06 |
· · | with two or more nitrated aromatic compounds present [2]

|  | C06B 25/08 |
· · · | at least one of which is nitrated toluene [2]

|  | C06B 25/10 |
· | the compound being nitroglycerine [2]

|  | C06B 25/12 |
· · | with other nitrated organic compound [2]

|  | C06B 25/14 |
· · · | the other compound being a nitrated aliphatic diol [2]

|  | C06B 25/16 |
· · · | the other compound being a nitrated aromatic [2]

|  | C06B 25/18 |
· | the compound being nitrocellulose present as 10% or more by weight of the total composition [2]

|  | C06B 25/20 |
· · | with a non-explosive or a non-thermic component [2]

|  | C06B 25/22 |
· · | with a nitrated aromatic compound [2]

|  | C06B 25/24 |
· · | with nitroglycerine [2]

|  | C06B 25/26 |
· · · | with an organic non-explosive or an organic non-thermic component [2]

|  | C06B 25/28 |
· | the compound being nitrocellulose present as less than 10% by weight of the total composition [2]

|  | C06B 25/30 |
· · | with nitroglycerine [2]

|  | C06B 25/32 |
· | the compound being nitrated pentaerythritol [2]

|  | C06B 25/34 |
· | the compound being a nitrated acyclic, alicyclic or heterocyclic amine [2]

|  | C06B 25/36 |
· | the compound being a nitroparaffin [2]

|  | C06B 25/38 |
· · | with other nitrated organic compound [2]

|  | C06B 25/40 |
· · | with two or more nitroparaffins present [2]

|  | C06B 27/00 |
Compositions containing a metal, boron, silicon, selenium or tellurium or mixtures, intercompounds or hydrides thereof, and hydrocarbons or halogenated hydrocarbons [2]

|  | C06B 29/00 |
Compositions containing an inorganic oxygen-halogen salt, e.g. chlorate, perchlorate [2]

|  | C06B 29/02 |
· | of an alkali metal [2]

|  | C06B 29/04 |
· · | with an inorganic non-explosive or an inorganic non-thermic component [2]

|  | C06B 29/06 |
· · · | the component being a cyanide; the component being an oxide of iron, chromium or manganese [2]

|  | C06B 29/08 |
· · | with an organic non-explosive or an organic non-thermic component [2]

|  | C06B 29/10 |
· · · | the component being a dye or a colouring agent [2]

|  | C06B 29/12 |
· · | with carbon or sulfur [2]

|  | C06B 29/14 |
· · | with iodine or an iodide [2]

|  | C06B 29/16 |
· · | with a nitrated organic compound [2]

|  | C06B 29/18 |
· · · | the compound being nitrated toluene or a nitrated phenol [2]

|  | C06B 29/20 |
· · · | the compound being nitrocellulose [2]

|  | C06B 29/22 |
· | the salt being ammonium perchlorate [2]

|  | C06B 31/00 |
Compositions containing an inorganic nitrogen-oxygen salt [2]

|  | C06B 31/02 |
· | the salt being an alkali metal or an alkaline earth metal nitrate [2]

|  | C06B 31/04 |
· · | with carbon or sulfur [2]

|  | C06B 31/06 |
· · · | with an organic non-explosive or an organic non-thermic component [2]

|  | C06B 31/08 |
· · | with a metal oxygen-halogen salt, e.g. inorganic chlorate, inorganic perchlorate [2]

|  | C06B 31/10 |
· · · | with carbon or sulfur [2]

|  | C06B 31/12 |
· · | with a nitrated organic compound [2]

|  | C06B 31/14 |
· · · | the compound being an aromatic [2]

|  | C06B 31/16 |
· · · · | the compound being a nitrated toluene [2]

|  | C06B 31/18 |
· · · · | the compound being a nitrated phenol, e.g. picric acid [2]

|  | C06B 31/20 |
· · · | the compound being nitroglycerine [2]

|  | C06B 31/22 |
· · · | the compound being nitrocellulose [2]

|  | C06B 31/24 |
· · · · | with other explosive or thermic component [2]

|  | C06B 31/26 |
· · · · · | the other component being nitroglycerine [2]

|  | C06B 31/28 |
· | the salt being ammonium nitrate [2]

|  | C06B 31/30 |
· · | with vegetable matter; with resin; with rubber [2]

|  | C06B 31/32 |
· · | with a nitrated organic compound [2]

|  | C06B 31/34 |
· · · | the nitrated compound being starch or sugar [2]

|  | C06B 31/36 |
· · · · | with other explosive or thermic component [2]

|  | C06B 31/38 |
· · · | the nitrated compound being an aromatic [2]

|  | C06B 31/40 |
· · · · | with an organic non-explosive or an organic non-thermic component [2]

|  | C06B 31/42 |
· · · · | with other explosive or thermic component [2]

|  | C06B 31/44 |
· · · | the compound being nitroglycerine [2]

|  | C06B 31/46 |
· · · · | with a vegetable matter component, e.g. wood pulp, sawdust [2]

|  | C06B 31/48 |
· · · · | with other explosive or thermic component [2]

|  | C06B 31/50 |
· · · · · | the other component being a nitrated organic compound [2]

|  | C06B 31/52 |
· · · | the compound being nitrocellulose present as 10% or more by weight of the total composition [2]

|  | C06B 31/54 |
· · · · | with other nitrated organic compound [2]

|  | C06B 31/56 |
· · · | the compound being nitrocellulose present as less than 10% by weight of the total composition [2]

|  | C06B 33/00 |
Compositions containing particulate metal, alloy, boron, silicon, selenium or tellurium with at least one oxygen supplying material which is either a metal oxide or a salt, organic or inorganic, capable of yielding a metal oxide [2]

|  | C06B 33/02 |
· | with an organic non-explosive or an organic non-thermic component [2]

|  | C06B 33/04 |
· | the material being an inorganic nitrogen-oxygen salt [2]

|  | C06B 33/06 |
· | the material being an inorganic oxygen-halogen salt [2]

|  | C06B 33/08 |
· | with a nitrated organic compound [2]

|  | C06B 33/10 |
· · | the compound being an aromatic [2]

|  | C06B 33/12 |
· | the material being two or more oxygen-yielding compounds [2]

|  | C06B 33/14 |
· · | at least one being an inorganic nitrogen-oxygen salt [2]

|  | C06B 35/00 |
Compositions containing a metal azide [2]

|  | C06B 37/00 |
Compositions containing a metal fulminate [2]

|  | C06B 37/02 |
· | with a nitrated organic compound or an inorganic oxygen-halogen salt [2]

|  | C06B 39/00 |
Compositions containing free phosphorus or a binary compound of phosphorus, except with oxygen [2]

|  | C06B 39/02 |
· | with an inorganic oxygen-halogen salt [2]

|  | C06B 39/04 |
· · | with a binary compound of phosphorus, except with oxygen [2]

|  | C06B 39/06 |
· | with free metal, alloy, boron, silicon, selenium or tellurium [2]

|  | C06B 41/00 |
Compositions containing a nitrated metallo-organic compound [2]

|  | C06B 41/02 |
· | the compound containing lead [2]

|  | C06B 41/04 |
· · | with an organic explosive or an organic thermic component [2]

|  | C06B 41/06 |
· · · | with an inorganic explosive or an inorganic thermic component [2]

|  | C06B 41/08 |
· · | with a metal azide or a metal fulminate [2]

|  | C06B 41/10 |
· · | with other nitrated metallo-organic compound [2]

|  | C06B 43/00 |
Compositions characterised by explosive or thermic constituents not provided for in groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...C06B 25/00-C06B 41/00 [2]

|  | C06B 45/00 |
Compositions or products which are defined by structure or arrangement of component or product (explosive charges of particular form or shape Fulltext... Hierarchy... Expanded...F42B 1/00, Fulltext... Hierarchy... Expanded...F42B 3/00) [2]

|  | C06B 45/02 |
· | comprising particles of diverse size or shape [2]

|  | C06B 45/04 |
· | comprising solid particles dispersed in solid solution or matrix [2]

|  | C06B 45/06 |
· · | the solid solution or matrix containing an organic component [2]

|  | C06B 45/08 |
· · · | the dispersed solid containing an inorganic explosive or an inorganic thermic component [2]

|  | C06B 45/10 |
· · · | the organic component containing a resin [2]

|  | C06B 45/12 |
· | having contiguous layers or zones [2]

|  | C06B 45/14 |
· · | a layer or zone containing an inorganic explosive or an inorganic thermic component [2]

|  | C06B 45/16 |
· · · | the layer or zone containing at least one inorganic component from the group of azide, fulminate, phosphorus and phosphide [2]

|  | C06B 45/18 |
· | comprising a coated component (particles dispersed in a matrix Fulltext... Hierarchy... Expanded...C06B 45/04; coated explosive charges Fulltext... Hierarchy... Expanded...F42B) [2]

|  | C06B 45/20 |
· · | the component base containing an organic explosive or an organic thermic component [2]

|  | C06B 45/22 |
· · · | the coating containing an organic compound [2]

|  | C06B 45/24 |
· · · · | the compound being an organic explosive or an organic thermic component [2]

|  | C06B 45/26 |
· · · · · | the compound being a nitrated toluene [2]

|  | C06B 45/28 |
· · · | the component base containing nitrocellulose and nitroglycerine [2]

|  | C06B 45/30 |
· · | the component base containing an inorganic explosive or an inorganic thermic component [2]

|  | C06B 45/32 |
· · · | the coating containing an organic compound [2]

|  | C06B 45/34 |
· · · · | the compound being an organic explosive or an organic thermic component [2]

|  | C06B 45/36 |
· · | the component base containing both an organic explosive or thermic component and an inorganic explosive or thermic component [2]

|  | C06B 47/00 |
Compositions in which the components are separately stored until the moment of burning or explosion, e.g. "Sprengel"-type explosives; Suspensions of solid component in a normally non-explosive liquid phase, including a thickened aqueous phase [2]

|  | C06B 47/02 |
· | the components comprising a binary propellant [2]

|  | C06B 47/04 |
· · | a component containing a nitrogen oxide or acid thereof [2]

|  | C06B 47/06 |
· · | a component being a liquefied normally gaseous material supplying oxygen (Fulltext... Hierarchy... Expanded...C06B 47/04 takes precedence) [2]

|  | C06B 47/08 |
· · | a component containing hydrazine or a hydrazine derivative [2]

|  | C06B 47/10 |
· · | a component containing free boron, an organic borane or a binary compound of boron, except with oxygen [2]

|  | C06B 47/12 |
· · | a component being a liquefied normally gaseous fuel [2]

|  | C06B 47/14 |
· | comprising a solid component and an aqueous phase [2]

|  | C06B 49/00 |
Use of single substances as explosives [2]