|  | D |
SECTION D — TEXTILES; PAPER

TEXTILES OR FLEXIBLE MATERIALS NOT OTHERWISE PROVIDED FOR

|  | D02 |
YARNS; MECHANICAL FINISHING OF YARNS OR ROPES; WARPING OR BEAMING

|  | D02 |
Note(s) In this class, the following terms are used with the meanings indicated: "fibre" means a relatively-short, elongated member of natural or artificial material; "filament" means an endless or quasi-endless, elongated member of natural or artificial material; "yarn" means a unitary assembly of fibres, usually produced by spinning; "thread" means an assembly of yarns or filaments, usually produced by twisting.

|  | D02H |
WARPING, BEAMING, OR LEASING

|  | D02H |
Note(s) Attention is drawn to the Note following the title of class Fulltext... Hierarchy... Expanded...D02.

|  | D02H |
Subclass index
CREELS | 1/00
WARPING; BEAMING; WARPING AND BEAMING COMBINED | 3/00; 5/00; 7/00
LEASING | 9/00
OTHER MACHINES AND METHODS | 11/00
DETAILS OF MACHINES | 13/00

|  | D02H 1/00 |
Creels, i.e. apparatus for supplying a multiplicity of individual threads

|  | D02H 3/00 |
Warping machines

|  | D02H 5/00 |
Beaming machines

|  | D02H 5/02 |
· | combined with apparatus for sizing or other treatment of warps (sizing per se Fulltext... Hierarchy... Expanded...D06B)

|  | D02H 7/00 |
Combined warping and beaming machines

|  | D02H 9/00 |
Leasing

|  | D02H 9/02 |
· | Lease rods or bands

|  | D02H 11/00 |
Methods or apparatus not provided for in the preceding groups, e.g. for cleaning the warp

|  | D02H 13/00 |
Details of machines of the preceding groups

|  | D02H 13/02 |
· | Stop motions

|  | D02H 13/04 |
· · | responsive to breakage, slackness, or excessive tension of threads, with detectors for individual threads or small groups of threads

|  | D02H 13/06 |
· · · | mechanical

|  | D02H 13/08 |
· · · | electrical

|  | D02H 13/10 |
· · | responsive to thread-measuring devices, e.g. stopping the machine when required length of warp has been wound

|  | D02H 13/12 |
· | Variable-speed driving mechanisms

|  | D02H 13/14 |
· · | controlled automatically by tension in the warp

|  | D02H 13/16 |
· | Reeds, combs, or other devices for determining the spacing of threads

|  | D02H 13/18 |
· · | with adjustable spacing

|  | D02H 13/20 |
· · | with fixed spacing

|  | D02H 13/22 |
· | Tensioning devices

|  | D02H 13/24 |
· · | for individual threads

|  | D02H 13/26 |
· · | for threads in warp form (controlling the driving of beams, or the like, to keep tension constant Fulltext... Hierarchy... Expanded...D02H 13/14)

|  | D02H 13/28 |
· | Warp beams (cloth beams Fulltext... Hierarchy... Expanded...D03D 49/20)

|  | D02H 13/30 |
· · | with flanges

|  | D02H 13/32 |
· · · | adjustable

|  | D02H 13/34 |
· · | sectional

|  | D02H 13/36 |
· · | Means for attaching warp to beam

|  | D02H 13/38 |
· | Storage racks for beams