|  | F |
SECTION F — MECHANICAL ENGINEERING; LIGHTING; HEATING; WEAPONS; BLASTING

|  | F01 - F04 |
Subsection index
MACHINES |
positive displacement |
rotary or oscillating piston |
liquid and elastic fluid or elastic fluid | F01C
liquid only | F04C
reciprocating piston or other |
liquid and elastic fluid or elastic fluid | F01B
liquid only | F04B
non-positive displacement |
liquid and elastic fluid or elastic fluid | F01D
liquid only | F03B
ENGINES |
positive displacement |
rotary or oscillating piston |
liquid and elastic fluid or elastic fluid | F01C
liquid only | F03C
reciprocating piston or other |
liquid and elastic fluid or elastic fluid | F01B
liquid only | F03C
non-positive displacement |
liquid and elastic fluid or elastic fluid | F01D
liquid only | F03B
PUMPS |
positive displacement |
rotary or oscillating piston | F04C
reciprocating piston or other | F04B
non-positive displacement | F04D

ENGINEERING IN GENERAL

|  | F16 |
ENGINEERING ELEMENTS OR UNITS; GENERAL MEASURES FOR PRODUCING AND MAINTAINING EFFECTIVE FUNCTIONING OF MACHINES OR INSTALLATIONS; THERMAL INSULATION IN GENERAL

|  | F16C |
SHAFTS; FLEXIBLE SHAFTS; ELEMENTS OF CRANKSHAFT MECHANISMS; ROTARY BODIES OTHER THAN GEARING ELEMENTS; BEARINGS [5]

|  | F16C |
2. Note(s) In this subclass, the following expression is used with the meaning indicated: "rotary bodies other than gearing elements" covers any element which rotates so far as its features are affected only by the fact that it rotates. Attention is drawn to the following places:
   Fulltext... Hierarchy... Expanded...A01B 71/04 | Bearings for agricultural machines |
   Fulltext... Hierarchy... Expanded...B21B 31/07 | Adaptation of roll bearings for metal-rolling mills |
   Fulltext... Hierarchy... Expanded...B23Q 1/25 | Bearings for movable or adjustable work or tool supports |
   Fulltext... Hierarchy... Expanded...B61C 17/10 | Connecting-rods, bearings for driving wheels of railway locomotives |
   Fulltext... Hierarchy... Expanded...B61F 15/00 | Axle-boxes for railway vehicles |
   Fulltext... Hierarchy... Expanded...B62K 21/06 | Bearings for steering heads |
   Fulltext... Hierarchy... Expanded...E06B 9/174, Fulltext... Hierarchy... Expanded...E06B 9/50 | Bearings specially adapted for roller shutters or for roller blinds |
   Fulltext... Hierarchy... Expanded...E21B 10/22 | Bearings for drill bits |
   Fulltext... Hierarchy... Expanded...F01C 21/02 | Arrangement of bearings in rotary-piston machines or engines |
   Fulltext... Hierarchy... Expanded...F01D 25/16 | Arrangement of bearings in non-positive displacement machines or engines |
   Fulltext... Hierarchy... Expanded...F02C 7/06 | Arrangement of bearings in gas-turbine plants |
   Fulltext... Hierarchy... Expanded...G01C 19/16 | Bearings for gyroscopes |
   Fulltext... Hierarchy... Expanded...G01D 11/02 | Bearings or suspensions for moving parts of measuring instruments |
   Fulltext... Hierarchy... Expanded...G01G 21/02 | Arrangements of bearings in weighing apparatus |
   Fulltext... Hierarchy... Expanded...G01R 1/10 | Arrangements of bearings in instruments for measuring electric variables |
   Fulltext... Hierarchy... Expanded...G01R 11/12 | Arrangements of bearings for apparatus for measuring time integral of electric power or current |
   Fulltext... Hierarchy... Expanded...G02C 5/22 | Hinges for spectacles |
   Fulltext... Hierarchy... Expanded...G04B 31/00 | Bearings for clockwork |
   Fulltext... Hierarchy... Expanded...H02N 15/00 | Magnetic levitation devices. [5] |

|  | F16C |
Subclass index
FLEXIBLE TRANSMISSIONS, SHAFTS, AXLES, CRANKS, ECCENTRICS | 1/00, 3/00
CROSSHEADS, CONNECTING-RODS | 5/00, 7/00, 9/00
PIVOTS | 11/00
ROLLS, DRUMS, DISCS | 13/00
BEARINGS |
For rotatable parts | 13/00, 17/00 - 27/00
For linearly-movable parts | 29/00
For parts which both rotate and move linearly | 31/00
For crankshafts or connecting- rods | 9/00
Not otherwise provided for | 32/00
Supports; parts or accessories | 27/00, 35/00; 33/00, 41/00
Cooling; relieving load | 37/00; 39/00
MAKING, ASSEMBLING | 33/00, 43/00
CONSTRUCTION OF ROTATABLE BODIES TO RESIST CENTRIFUGAL FORCE | 15/00

P:0 |  | F16C 1/00 |
Flexible shafts (flexible shafts in dental machines for boring or cutting Fulltext... Hierarchy... Expanded...A61C 1/18); Mechanical means for transmitting movement in a flexible sheathing

|  | F16C 1/02 |
· | for conveying rotary movements

|  | F16C 1/04 |
· · | Articulated shafts

|  | F16C 1/06 |
· · | with guiding-sheathing, tube, or box (Fulltext... Hierarchy... Expanded...F16C 1/04 takes precedence; guiding-sheathings Fulltext... Hierarchy... Expanded...F16C 1/26)

|  | F16C 1/08 |
· · | End connections

|  | F16C 1/10 |
· | Means for transmitting linear movement in a flexible sheathing, e.g. "Bowden mechanisms" (guiding-sheathings Fulltext... Hierarchy... Expanded...F16C 1/26)

|  | F16C 1/12 |
· · | Arrangements for transmitting movement to or from the flexible member

|  | F16C 1/14 |
· · · | Construction of the end-piece of the flexible member; Attachment thereof to the flexible member

|  | F16C 1/16 |
· · · | in which the end-piece is guided rectilinearly

|  | F16C 1/18 |
· · · | in which the end portion of the flexible member is laid along a curved surface of a pivoted member

|  | F16C 1/20 |
· · | Construction of flexible members moved to and fro in the sheathing

|  | F16C 1/22 |
· · | Adjusting; Compensating length

|  | F16C 1/24 |
· | Lubrication; Lubricating equipment

|  | F16C 1/26 |
· | Construction of guiding-sheathings or guiding-tubes

|  | F16C 1/28 |
· · | with built-in bearings

P:10 |  | F16C 3/00 |
Shafts (flexible shafts Fulltext... Hierarchy... Expanded...F16C 1/00; marine propeller shafts, paddle wheel shafts Fulltext... Hierarchy... Expanded...B63H 23/34); Axles; Cranks; Eccentrics

|  | F16C 3/02 |
· | Shafts; Axles

|  | F16C 3/03 |
· · | telescopic (axially displaceable couplings Fulltext... Hierarchy... Expanded...F16D 3/06)

|  | F16C 3/035 |
· · · | with built-in bearings

|  | F16C 3/04 |
· | Crankshafts, eccentric-shafts; Cranks, eccentrics

|  | F16C 3/06 |
· · | Crankshafts

|  | F16C 3/08 |
· · · | made in one piece (features relating to lubrication Fulltext... Hierarchy... Expanded...F16C 3/14, to cooling Fulltext... Hierarchy... Expanded...F16C 3/16)

|  | F16C 3/10 |
· · · | assembled of several parts, e.g. by welding

|  | F16C 3/12 |
· · · · | releasably connected

|  | F16C 3/14 |
· · · | Features relating to lubrication

|  | F16C 3/16 |
· · · | Features relating to cooling

|  | F16C 3/18 |
· · | Eccentric-shafts

|  | F16C 3/20 |
· · | Shape of crankshafts or eccentric-shafts having regard to balancing

|  | F16C 3/22 |
· · | Cranks; Eccentrics (constructional features of crank-pins Fulltext... Hierarchy... Expanded...F16C 11/02)

|  | F16C 3/24 |
· · · | with return cranks, i.e. a second crank carried by the crank-pin

|  | F16C 3/26 |
· · · | Elastic crank-webs; Resiliently-mounted crank-pins (elastic connecting-rods Fulltext... Hierarchy... Expanded...F16C 7/04)

|  | F16C 3/28 |
· · · | Adjustable cranks or eccentrics (adjustable crank mechanisms Fulltext... Hierarchy... Expanded...F16H 21/20)

|  | F16C 3/30 |
· · · | with arrangements for overcoming dead-centres

P:20 |  | F16C 5/00 |
Crossheads; Constructions of connecting-rod heads or piston-rod connections rigid with crossheads (piston-rods, i.e. rods rigidly connected to the piston, Fulltext... Hierarchy... Expanded...F16J 7/00)

P:30 |  | F16C 7/00 |
Connecting-rods or like links pivoted at both ends (coupling-rods for locomotive driving-wheels Fulltext... Hierarchy... Expanded...B61C; inhibiting shift in gearing during unfavourable conditions Fulltext... Hierarchy... Expanded...F16H 61/16); Construction of connecting-rod heads (heads rigid with crossheads Fulltext... Hierarchy... Expanded...F16C 5/00)

|  | F16C 7/02 |
· | Constructions of connecting-rods with constant length

|  | F16C 7/04 |
· | with elastic intermediate part or fluid cushion

|  | F16C 7/06 |
· | Adjustable connecting-rods

|  | F16C 7/08 |
· | made from sheet metal

P:40 |  | F16C 9/00 |
Bearings for crankshafts or connecting-rods; Attachment of connecting-rods (lubrication of connecting-rods in connection with crankshafts Fulltext... Hierarchy... Expanded...F16C 3/14; connections to crossheads Fulltext... Hierarchy... Expanded...F16C 5/00, to pistons Fulltext... Hierarchy... Expanded...F16J 1/14)

|  | F16C 9/02 |
· | Crankshaft bearings

|  | F16C 9/03 |
· · | Arrangements for adjusting play

|  | F16C 9/04 |
· | Connecting-rod bearings; Attachment thereof

|  | F16C 9/06 |
· · | Arrangements for adjusting play in bearings, operating either automatically or not (bearings adjustable for play in general Fulltext... Hierarchy... Expanded...F16C 25/00)

P:50 |  | F16C 11/00 |
Pivots; Pivotal connections (arrangements of steering linkage connections Fulltext... Hierarchy... Expanded...B62D 7/16)

|  | F16C 11/02 |
· | Trunnions; Crank-pins (fastening crank-pins to webs, crank-pins integral with cranks Fulltext... Hierarchy... Expanded...F16C 3/06, Fulltext... Hierarchy... Expanded...F16C 3/22)

|  | F16C 11/04 |
· | Pivotal connections (hinges for doors, windows or wings Fulltext... Hierarchy... Expanded...E05D; rubber springs with stiff outer sleeve and inner sleeve or pin Fulltext... Hierarchy... Expanded...F16F 1/38)

|  | F16C 11/06 |
· · | Ball-joints; Other joints having more than one degree of angular freedom, i.e. universal joints (for transmitting rotary motion Fulltext... Hierarchy... Expanded...F16D 3/00; supports for apparatus with ball-joint heads Fulltext... Hierarchy... Expanded...F16M 11/14)

|  | F16C 11/08 |
· · · | with resilient bearings

|  | F16C 11/10 |
· · | Arrangements for locking

|  | F16C 11/12 |
· · | incorporating flexible connections, e.g. leaf springs

P:70 |  | F16C 13/00 |
Rolls, drums, discs, or the like (guide rollers in feeding webs Fulltext... Hierarchy... Expanded...B65H 27/00; calender rolls, bearings therefor Fulltext... Hierarchy... Expanded...D21G 1/02; pulleys Fulltext... Hierarchy... Expanded...F16H 55/00; rotary drums or rollers for heat-exchange or heat-transfer apparatus Fulltext... Hierarchy... Expanded...F28F 5/02; special adaptations, see the relevant classes); Bearings or mountings therefor

|  | F16C 13/02 |
· | Bearings

|  | F16C 13/04 |
· · | Bearings with only partial enclosure of the member to be borne; Bearings with local support at two or more points

|  | F16C 13/06 |
· · | self-adjusting

P:60 |  | F16C 15/00 |
Construction of rotary bodies to resist centrifugal force (flywheels, correction weights Fulltext... Hierarchy... Expanded...F16F 15/30, Fulltext... Hierarchy... Expanded...F16F 15/32)

|  | F16C 17/00 - F16C 27/00 |
Bearings for rotary parts (Fulltext... Hierarchy... Expanded...F16C 9/00, Fulltext... Hierarchy... Expanded...F16C 13/02 take precedence; allowing for linear movement also Fulltext... Hierarchy... Expanded...F16C 31/00)

P:130 |  | F16C 17/00 |
Sliding-contact bearings (Fulltext... Hierarchy... Expanded...F16C 32/06 takes precedence; adjustable bearings Fulltext... Hierarchy... Expanded...F16C 23/00, Fulltext... Hierarchy... Expanded...F16C 25/00) [2]

|  | F16C 17/02 |
· | for radial load only

|  | F16C 17/03 |
· · | with tiltably-supported segments, e.g. Michell bearings

|  | F16C 17/04 |
· | for axial load only

|  | F16C 17/06 |
· · | with tiltably-supported segments, e.g. Michell bearings

|  | F16C 17/08 |
· · | for supporting the end face of a shaft or other member, e.g. footstep bearings

|  | F16C 17/10 |
· | for both radial and axial load

|  | F16C 17/12 |
· | characterised by features not related to the direction of the load

|  | F16C 17/14 |
· · | specially adapted for operating in water

|  | F16C 17/18 |
· · | with floating brasses or bushes, rotatable at a reduced speed

|  | F16C 17/20 |
· · | with emergency supports or bearings

|  | F16C 17/22 |
· · | with arrangements compensating for thermal expansion

|  | F16C 17/24 |
· · | with devices affected by abnormal or undesired conditions, e.g. for preventing overheating, for safety

|  | F16C 17/26 |
· | Systems consisting of a plurality of sliding-contact bearings

P:120 |  | F16C 19/00 |
Bearings with rolling contact (adjustable bearings Fulltext... Hierarchy... Expanded...F16C 23/00, Fulltext... Hierarchy... Expanded...F16C 25/00)

|  | F16C 19/02 |
· | with bearing balls essentially of the same size in one or more circular rows

|  | F16C 19/04 |
· · | for radial load mainly

|  | F16C 19/06 |
· · · | with a single row of balls

|  | F16C 19/08 |
· · · | with two or more rows of balls

|  | F16C 19/10 |
· · | for axial load mainly

|  | F16C 19/12 |
· · · | for supporting the end face of a shaft or other member, e.g. footstep bearings

|  | F16C 19/14 |
· · | for both radial and axial load

|  | F16C 19/16 |
· · · | with a single row of balls

|  | F16C 19/18 |
· · · | with two or more rows of balls

|  | F16C 19/20 |
· · | with loose spacing bodies, e.g. balls, between the bearing balls

|  | F16C 19/22 |
· | with bearing rollers essentially of the same size in one or more circular rows, e.g. needle bearings

|  | F16C 19/24 |
· · | for radial load mainly

|  | F16C 19/26 |
· · · | with a single row of rollers

|  | F16C 19/28 |
· · · | with two or more rows of rollers

|  | F16C 19/30 |
· · | for axial load mainly

|  | F16C 19/32 |
· · · | for supporting the end face of a shaft or other member, e.g. footstep bearings

|  | F16C 19/34 |
· · | for both radial and axial load

|  | F16C 19/36 |
· · · | with a single row of rollers

|  | F16C 19/38 |
· · · | with two or more rows of rollers

|  | F16C 19/40 |
· · | with loose spacing bodies between the rollers

|  | F16C 19/44 |
· · | Needle bearings

|  | F16C 19/46 |
· · · | with one row of needles

|  | F16C 19/48 |
· · · | with two or more rows of needles

|  | F16C 19/49 |
· | Bearings with both balls and rollers

|  | F16C 19/50 |
· | Other types of ball or roller bearings

|  | F16C 19/52 |
· | with devices affected by abnormal or undesired conditions

|  | F16C 19/54 |
· | Systems consisting of a plurality of bearings with rolling friction (spindle bearings Fulltext... Hierarchy... Expanded...F16C 35/08)

|  | F16C 19/55 |
· · | with intermediate floating rings rotating at reduced speed

|  | F16C 19/56 |
· · | in which the rolling bodies of one bearing differ in diameter from those of another

P:110 |  | F16C 21/00 |
Combinations of sliding-contact bearings with ball or roller bearings (Fulltext... Hierarchy... Expanded...F16C 17/24, Fulltext... Hierarchy... Expanded...F16C 19/52 take precedence) [2]

P:100 |  | F16C 23/00 |
Bearings adjustable for aligning or positioning (Fulltext... Hierarchy... Expanded...F16C 27/00 takes precedence)

|  | F16C 23/02 |
· | Sliding-contact bearings

|  | F16C 23/04 |
· · | self-adjusting

|  | F16C 23/06 |
· | Ball or roller bearings

|  | F16C 23/08 |
· · | self-adjusting

|  | F16C 23/10 |
· | Bearings, parts of which are eccentrically adjustable with respect to each other

P:90 |  | F16C 25/00 |
Bearings adjustable for wear or play (Fulltext... Hierarchy... Expanded...F16C 27/00 takes precedence)

|  | F16C 25/02 |
· | Sliding-contact bearings

|  | F16C 25/04 |
· · | self-adjusting

|  | F16C 25/06 |
· | Ball or roller bearings

|  | F16C 25/08 |
· · | self-adjusting

P:80 |  | F16C 27/00 |
Elastic or yielding bearings or bearing supports (shock-damping bearings for watches or clocks Fulltext... Hierarchy... Expanded...G04B 31/02)

|  | F16C 27/02 |
· | Sliding-contact bearings

|  | F16C 27/04 |
· | Ball or roller bearings, e.g. with resilient rolling bodies

|  | F16C 27/06 |
· | by means of parts of rubber or like materials (Fulltext... Hierarchy... Expanded...F16C 27/08 takes precedence; with sliding surfaces of rubber or synthetic rubber Fulltext... Hierarchy... Expanded...F16C 33/22; construction of units comprising rigid inner and outer members with rubber or the like between them Fulltext... Hierarchy... Expanded...F16F 1/38)

|  | F16C 27/08 |
· | primarily for axial load, e.g. for vertically-arranged shafts

|  | F16C 29/00 - F16C 32/00 |
Other bearings

P:150 |  | F16C 29/00 |
Bearings for parts moving only linearly (Fulltext... Hierarchy... Expanded...F16C 32/06 takes precedence; incorporated in flexible shafts Fulltext... Hierarchy... Expanded...F16C 1/28) [2]

|  | F16C 29/02 |
· | Sliding-contact bearings

|  | F16C 29/04 |
· | Ball or roller bearings

|  | F16C 29/06 |
· · | in which the rolling bodies circulate partly without carrying load

|  | F16C 29/08 |
· | Arrangements for covering or protecting the ways

|  | F16C 29/10 |
· | Arrangements for locking the bearings (preventing relative movement between machine parts in general Fulltext... Hierarchy... Expanded...F16B, e.g. Fulltext... Hierarchy... Expanded...F16B 1/00)

|  | F16C 29/12 |
· | Arrangements for adjusting play

P:140 |  | F16C 31/00 |
Bearings for parts which both rotate and move linearly

|  | F16C 31/02 |
· | Sliding-contact bearings

|  | F16C 31/04 |
· | Ball or roller bearings

|  | F16C 31/06 |
· · | in which the rolling bodies circulate partly without carrying load

P:160 |  | F16C 32/00 |
Bearings not otherwise provided for

|  | F16C 32/02 |
· | Knife-edge bearings

|  | F16C 32/04 |
· | using magnetic or electric supporting means [2]

|  | F16C 32/06 |
· | with moving member supported by a fluid cushion formed, at least to a large extent, otherwise than by movement of the shaft, e.g. hydrostatic air-cushion bearings [2]

|  | F16C 33/00 - F16C 43/00 |
Details or accessories of bearings

P:210 |  | F16C 33/00 |
Parts of bearings; Special methods for making bearings or parts thereof (metal-working or like operations, see the relevant classes)

|  | F16C 33/02 |
· | Parts of sliding-contact bearings

|  | F16C 33/04 |
· · | Brasses; Bushes; Linings

|  | F16C 33/06 |
· · · | Sliding surface mainly made of metal (Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...F16C 33/24-F16C 33/28 take precedence)

|  | F16C 33/08 |
· · · · | Attachment of brasses, bushes, or linings to the bearing housing

|  | F16C 33/10 |
· · · · | Construction relative to lubrication

|  | F16C 33/12 |
· · · · | Structural composition; Use of special materials or surface treatments, e.g. for rust-proofing (the materials or treatments themselves, see the relevant places, e.g. Fulltext... Hierarchy... Expanded...C22C)

|  | F16C 33/14 |
· · · · | Special methods of manufacture; Running-in

|  | F16C 33/16 |
· · · | Sliding surface consisting mainly of graphite

|  | F16C 33/18 |
· · · | Sliding surface consisting mainly of wood or fibrous material

|  | F16C 33/20 |
· · · | Sliding surface consisting mainly of plastics (Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...F16C 33/22-F16C 33/28 take precedence)

|  | F16C 33/22 |
· · · | Sliding surface consisting mainly of rubber or synthetic rubber (Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...F16C 33/24-F16C 33/28 take precedence; of interest apart from the surface itself Fulltext... Hierarchy... Expanded...F16C 27/06)

|  | F16C 33/24 |
· · · | with different areas of the sliding surface consisting of different materials

|  | F16C 33/26 |
· · · | made from wire coils; made from a number of discs, rings, rods, or other members

|  | F16C 33/28 |
· · · | with embedded reinforcements shaped as frames or meshed materials

|  | F16C 33/30 |
· | Parts of ball or roller bearings

|  | F16C 33/32 |
· · | Balls

|  | F16C 33/34 |
· · | Rollers; Needles

|  | F16C 33/36 |
· · · | with bearing-surfaces other than cylindrical, e.g. tapered; with grooves in the bearing surfaces

|  | F16C 33/37 |
· · | Loose spacing bodies

|  | F16C 33/372 |
· · · | rigid

|  | F16C 33/374 |
· · · | resilient

|  | F16C 33/38 |
· · | Ball cages

|  | F16C 33/40 |
· · · | for multiple rows of balls

|  | F16C 33/41 |
· · · | comb-shaped

|  | F16C 33/42 |
· · · | made from wire or sheet-metal strips (Fulltext... Hierarchy... Expanded...F16C 33/40, Fulltext... Hierarchy... Expanded...F16C 33/41 take precedence)

|  | F16C 33/44 |
· · · | Selection of substances (Fulltext... Hierarchy... Expanded...F16C 33/40, Fulltext... Hierarchy... Expanded...F16C 33/41 take precedence)

|  | F16C 33/46 |
· · | Cages for rollers or needles

|  | F16C 33/48 |
· · · | for multiple rows of rollers or needles

|  | F16C 33/49 |
· · · | comb-shaped

|  | F16C 33/50 |
· · · | formed of interconnected members, e.g. chains

|  | F16C 33/51 |
· · · | formed of unconnected members

|  | F16C 33/52 |
· · · | with no part entering between, or touching, the bearing surfaces of the rollers (Fulltext... Hierarchy... Expanded...F16C 33/50 takes precedence)

|  | F16C 33/54 |
· · · | made from wire, strips, or sheet metal (Fulltext... Hierarchy... Expanded...F16C 33/48, Fulltext... Hierarchy... Expanded...F16C 33/49 take precedence)

|  | F16C 33/56 |
· · · | Selection of substances (Fulltext... Hierarchy... Expanded...F16C 33/48, Fulltext... Hierarchy... Expanded...F16C 33/49 take precedence)

|  | F16C 33/58 |
· · | Raceways; Race rings

|  | F16C 33/60 |
· · · | divided

|  | F16C 33/61 |
· · · · | formed by wires

|  | F16C 33/62 |
· · · | Selection of substances

|  | F16C 33/64 |
· · · | Special methods of manufacture

|  | F16C 33/66 |
· · | Special parts or details in view of lubrication

|  | F16C 33/72 |
· | Sealings (sealings in general Fulltext... Hierarchy... Expanded...F16J)

|  | F16C 33/74 |
· · | of sliding-contact bearings

|  | F16C 33/76 |
· · | of ball or roller bearings

|  | F16C 33/78 |
· · · | with a diaphragm, disc, or ring, with or without resilient members

|  | F16C 33/80 |
· · · | Labyrinth sealings

|  | F16C 33/82 |
· · · | Arrangements for electrostatic or magnetic action against dust or other particles

P:200 |  | F16C 35/00 |
Rigid support of bearing units; Housings, e.g. caps, covers (Fulltext... Hierarchy... Expanded...F16C 23/00 takes precedence; elastic or yielding supports Fulltext... Hierarchy... Expanded...F16C 27/00)

|  | F16C 35/02 |
· | in the case of sliding-contact bearings

|  | F16C 35/04 |
· | in the case of ball or roller bearings

|  | F16C 35/06 |
· · | Mounting of ball or roller bearings; Fixing them onto shaft or in housing (hand-tools for inserting or withdrawing sleeves or ball races Fulltext... Hierarchy... Expanded...B25B 27/06)

|  | F16C 35/063 |
· · · | Fixing them on the shaft (with interposition of an element Fulltext... Hierarchy... Expanded...F16C 35/07) [3]

|  | F16C 35/067 |
· · · | Fixing them in a housing (with interposition of an element Fulltext... Hierarchy... Expanded...F16C 35/07) [3]

|  | F16C 35/07 |
· · · | Fixing them on the shaft or housing with interposition of an element [3]

|  | F16C 35/073 |
· · · · | between shaft and inner race ring [3]

|  | F16C 35/077 |
· · · · | between housing and outer race ring [3]

|  | F16C 35/078 |
· · · | using pressure fluid as mounting aid [3]

|  | F16C 35/08 |
· | for spindles

|  | F16C 35/10 |
· · | with sliding-contact bearings

|  | F16C 35/12 |
· · | with ball or roller bearings

P:180 |  | F16C 37/00 |
Cooling of bearings

P:170 |  | F16C 39/00 |
Relieving load on bearings

|  | F16C 39/02 |
· | using mechanical means

|  | F16C 39/04 |
· | using hydraulic or pneumatic means

|  | F16C 39/06 |
· | using magnetic means

P:220 |  | F16C 41/00 |
Other accessories

|  | F16C 41/02 |
· | Arrangements for equalising the load on a plurality of bearings or their elements

|  | F16C 41/04 |
· | Preventing damage to bearings during storage or transport thereof or when otherwise out of use

P:190 |  | F16C 43/00 |
Assembling bearings

|  | F16C 43/02 |
· | Assembling sliding-contact bearings

|  | F16C 43/04 |
· | Assembling rolling contact bearings

|  | F16C 43/06 |
· · | Placing rolling bodies in cages or bearings

|  | F16C 43/08 |
· · · | by deforming the cages or the races