|  | E |
SECTION E — FIXED CONSTRUCTIONS

BUILDING

|  | E05 |
LOCKS; KEYS; WINDOW OR DOOR FITTINGS; SAFES

|  | E05 |
Note(s) In this class, the following terms are used with the meanings indicated: "wing" is a general term for swingable, slidable, or otherwise movable doors or windows. This term also includes other movable structures such as drawers, lids of chests, car boots, or car bonnets, to which the operating, mounting, latching, or locking means covered by this class may be applied; "frame" means any member to which a wing may be held by a fastening device. It does not include a framework forming part of the wing, but it may be another wing; "lock" means primarily a device for releasing or securing any member, which requires a key or a permutation mechanism for release. In groups Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...E05B 1/00-E05B 9/00, Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...E05B 13/00-E05B 17/00, Fulltext... Hierarchy... Expanded...Fulltext... Hierarchy... Expanded...E05B 39/00-E05B 47/00, Fulltext... Hierarchy... Expanded...E05B 51/00, Fulltext... Hierarchy... Expanded...E05B 53/00, Fulltext... Hierarchy... Expanded...E05B 63/00 and Fulltext... Hierarchy... Expanded...E05B 65/00 however, the term "lock" may include other fastening devices; "bolt" means a sliding, pivoted, or otherwise movable member such as is normally carried by a door to hold it shut by engagement with a keeper on the frame. It may be operated by hand directly or through mechanism or by a key; it may be a latch (see below); "latch" means a bolt arranged to be moved to the releasing position against the force of a spring, or some other returning force, when a wing meets the frame on closing, so that it does not have to be operated by hand to secure the wing, but only to open it; "hasp" means a member hinged to the frame or wing so that it can be moved towards the face of the wing or frame and secured thereto, e.g. by a turn-button, by a padlock and staple.

|  | E05D |
HINGES OR OTHER SUSPENSION DEVICES FOR DOORS, WINDOWS, OR WINGS (pivotal connections in general Fulltext... Hierarchy... Expanded...F16C 11/00)

|  | E05D |
Subclass index
HINGES |
General structure | 1/00, 3/00
Special structure | 7/00
Details; accessories | 5/00, 9/00; 11/00
OTHER SUSPENSION DEVICES FOR WINGS | 13/00, 15/00

P:50 |  | E05D 1/00 |
Pinless hinges; Substitutes for hinges

|  | E05D 1/02 |
· | made of one piece

|  | E05D 1/04 |
· | with guide members shaped as circular arcs

|  | E05D 1/06 |
· | consisting of two easily-separable parts

P:40 |  | E05D 3/00 |
Hinges with pins

|  | E05D 3/02 |
· | with one pin

|  | E05D 3/04 |
· · | engaging three or more parts, e.g. sleeves, movable relatively to one another for connecting two or more wings to another member

|  | E05D 3/06 |
· | with two or more pins (Fulltext... Hierarchy... Expanded...E05D 7/08 takes precedence) [2]

|  | E05D 3/08 |
· · | for swing-doors, i.e. openable by pushing from either side

|  | E05D 3/10 |
· · | with non-parallel pins

|  | E05D 3/12 |
· · | with two parallel pins and one arm (Fulltext... Hierarchy... Expanded...E05D 3/08 takes precedence) [7]

|  | E05D 3/14 |
· · | with four parallel pins and two arms (Fulltext... Hierarchy... Expanded...E05D 3/08 takes precedence) [7]

|  | E05D 3/16 |
· · | with seven parallel pins and four arms (Fulltext... Hierarchy... Expanded...E05D 3/08 takes precedence) [7]

|  | E05D 3/18 |
· · | with sliding pins or guides (Fulltext... Hierarchy... Expanded...E05D 3/08 takes precedence) [7]

P:70 |  | E05D 5/00 |
Construction of single parts, e.g. the parts for attachment

|  | E05D 5/02 |
· | Parts for attachment, e.g. flaps

|  | E05D 5/04 |
· · | Flat flaps

|  | E05D 5/06 |
· · | Bent flaps

|  | E05D 5/08 |
· · | of cylindrical shape

|  | E05D 5/10 |
· | Pins, sockets or sleeves; Removable pins (Fulltext... Hierarchy... Expanded...E05D 15/522 takes precedence) [2]

|  | E05D 5/12 |
· · | Securing pins in sockets, movably or not

|  | E05D 5/14 |
· · | Construction of sockets or sleeves

|  | E05D 5/16 |
· · · | to be secured without special attachment parts on the socket or sleeve

P:20 |  | E05D 7/00 |
Hinges or pivots of special construction (used for special suspension arrangements Fulltext... Hierarchy... Expanded...E05D 15/00; so as to be self-closing Fulltext... Hierarchy... Expanded...E05F 1/06, Fulltext... Hierarchy... Expanded...E05F 1/12; with means for raising wings before being turned Fulltext... Hierarchy... Expanded...E05F 7/02)

|  | E05D 7/02 |
· | for use on the right-hand as well as on the left-hand side; Convertible right-hand or left-hand hinges

|  | E05D 7/04 |
· | Hinges adjustable relative to the wing or the frame

|  | E05D 7/06 |
· | to allow tilting of the members

|  | E05D 7/08 |
· | for use in suspensions comprising two spigots placed at opposite edges of the wing, especially at the top and the bottom, e.g. trunnions

|  | E05D 7/081 |
· · | the pivot axis of the wing being situated near one edge of the wing (braking devices therefor Fulltext... Hierarchy... Expanded...E05D 11/08) [2]

|  | E05D 7/082 |
· · | the pivot axis of the wing being situated at a considerable distance from the edges of the wing [2]

|  | E05D 7/083 |
· · · | with a fixed pivot axis [2]

|  | E05D 7/084 |
· · · | with a movable pivot axis [2]

|  | E05D 7/085 |
· · · · | with two or more pivot axes, e.g. used at the same time [2]

|  | E05D 7/086 |
· · · | Braking devices structurally combined with hinges (braking devices for windows per se Fulltext... Hierarchy... Expanded...E05F 5/00) [2]

|  | E05D 7/10 |
· | to allow easy separation of the parts at the hinge axis (substitutes for hinges Fulltext... Hierarchy... Expanded...E05D 1/06)

|  | E05D 7/12 |
· | to allow easy detachment of the hinge from the wing or the frame

|  | E05D 7/14 |
· | Hinges for safes

P:60 |  | E05D 9/00 |
Flaps or sleeves specially designed for making from particular material, e.g. hoop-iron, sheet metal, plastics

P:30 |  | E05D 11/00 |
Additional features or accessories of hinges

|  | E05D 11/02 |
· | Lubricating arrangements

|  | E05D 11/04 |
· | relating to the use of free balls as bearing-surfaces (Fulltext... Hierarchy... Expanded...E05D 7/06 takes precedence)

|  | E05D 11/06 |
· | Devices for limiting the opening movement of hinges

|  | E05D 11/08 |
· | Friction devices between relatively-movable hinge parts (Fulltext... Hierarchy... Expanded...E05D 7/086 takes precedence) [2]

|  | E05D 11/10 |
· | Devices for preventing movement between relatively-movable hinge parts

P:10 |  | E05D 13/00 |
Accessories for sliding or lifting wings, e.g. pulleys, safety catches (counterbalance devices Fulltext... Hierarchy... Expanded...E05F 1/00, Fulltext... Hierarchy... Expanded...E05F 3/00) [4]

P:0 |  | E05D 15/00 |
Suspension arrangements for wings (arrangements of wings not characterised by the construction of the supporting means Fulltext... Hierarchy... Expanded...E06B 3/32)

|  | E05D 15/02 |
· | for revolving wings

|  | E05D 15/04 |
· | with arms fixed on the wing pivoting about an axis outside of the wing

|  | E05D 15/06 |
· | for wings sliding horizontally more or less in their own plane

|  | E05D 15/08 |
· · | consisting of two or more independent parts movable each in its own guides

|  | E05D 15/10 |
· · | movable out of one plane into a second parallel plane

|  | E05D 15/12 |
· · | consisting of parts connected at their edges

|  | E05D 15/14 |
· · | with movable arms situated in the plane of the wing

|  | E05D 15/16 |
· | for wings sliding vertically more or less in their own plane

|  | E05D 15/18 |
· · | consisting of two or more independent parts movable each in its own guides

|  | E05D 15/20 |
· · | movable out of one plane into a second parallel plane

|  | E05D 15/22 |
· · | allowing an additional movement

|  | E05D 15/24 |
· · | consisting of parts connected at their edges

|  | E05D 15/26 |
· | for folding wings

|  | E05D 15/28 |
· | supported on arms movable in horizontal plane

|  | E05D 15/30 |
· · | with pivoted arms and sliding guides

|  | E05D 15/32 |
· · | with two pairs of pivoted arms

|  | E05D 15/34 |
· · · | with wings opening parallel to themselves

|  | E05D 15/36 |
· | moving along slide-ways so arranged that one guide member of the wing moves in a direction substantially perpendicular to the movement of another guide member

|  | E05D 15/38 |
· · | for upwardly-moving wings, e.g. up-and-over doors

|  | E05D 15/40 |
· | supported on arms movable in vertical planes

|  | E05D 15/42 |
· · | with pivoted arms and horizontally-sliding guides

|  | E05D 15/44 |
· · | with pivoted arms and vertically-sliding guides

|  | E05D 15/46 |
· · | with two pairs of pivoted arms

|  | E05D 15/48 |
· | allowing alternative movements (for vertically-sliding wings Fulltext... Hierarchy... Expanded...E05D 15/22)

|  | E05D 15/50 |
· · | for opening at either of two opposite edges

|  | E05D 15/52 |
· · | for opening about a vertical as well as a horizontal axis

|  | E05D 15/522 |
· · · | with disconnecting means for the appropriate pivoting parts [2]

|  | E05D 15/523 |
· · · · | using movable rods [2]

|  | E05D 15/524 |
· · · · · | Actuating mechanisms [2]

|  | E05D 15/526 |
· · · | Safety devices [2]

|  | E05D 15/54 |
· · | for opening both inwards and outwards

|  | E05D 15/56 |
· | with successive different movements

|  | E05D 15/58 |
· · | with both swinging and sliding movements