|  | E |
SECTION E — FIXED CONSTRUCTIONS

BUILDING

|  | E03 |
WATER SUPPLY; SEWERAGE

|  | E03C |
DOMESTIC PLUMBING INSTALLATIONS FOR FRESH WATER OR WASTE WATER (not connected to either water-supply main or to waste pipe Fulltext... Hierarchy... Expanded...A47K; devices of the kind used in the ground Fulltext... Hierarchy... Expanded...E03B, Fulltext... Hierarchy... Expanded...E03F); SINKS

|  | E03C 1/00 |
Domestic plumbing installations for fresh water or waste water; Sinks

|  | E03C 1/01 |
· | for combinations of baths, douches, sinks, wash-basins, closets, urinals, or the like

|  | E03C 1/02 |
· | Plumbing installations for fresh water

|  | E03C 1/04 |
· · | Water-basin installations specially adapted to wash-basins or baths (valves, faucets, mixing valves, taps Fulltext... Hierarchy... Expanded...F16K)

|  | E03C 1/042 |
· · · | Arrangements on taps for wash-basins or baths for connecting to the wall

|  | E03C 1/044 |
· · · | having a heating or cooling apparatus in the supply line (water heaters, e.g. with continuous flow, Fulltext... Hierarchy... Expanded...F24H)

|  | E03C 1/046 |
· · · | Adding soap, disinfectant, or the like, in the supply line (preventing contamination of drinking-water pipes Fulltext... Hierarchy... Expanded...E03C 1/10)

|  | E03C 1/048 |
· · · | supplying water through two or more openings around or along one side of the water-basin

|  | E03C 1/05 |
· · | Arrangements of devices on wash-basins, baths, sinks, or the like for remote control of taps (remote control of taps or the like per se Fulltext... Hierarchy... Expanded...F16K)

|  | E03C 1/06 |
· · | Devices for suspending or supporting the supply pipe or supply hose of a shower-bath

|  | E03C 1/08 |
· · | Jet regulators, e.g. anti-splash devices

|  | E03C 1/084 |
· · · | Jet regulators with aerating means

|  | E03C 1/086 |
· · · | Jet regulators or jet guides, easily mountable on the outlet of taps

|  | E03C 1/10 |
· · | Devices for preventing contamination of drinking-water pipes, e.g. means for aerating self-closing flushing valves (vacuum-breakers in general Fulltext... Hierarchy... Expanded...F16K, Fulltext... Hierarchy... Expanded...F16L)

|  | E03C 1/12 |
· | Plumbing installations for waste water; Basins or fountains connected thereto (drainage devices in floors Fulltext... Hierarchy... Expanded...E03F 5/04); Sinks

|  | E03C 1/122 |
· · | Pipe-line systems for waste water in buildings (pipe-line systems in general Fulltext... Hierarchy... Expanded...F17D)

|  | E03C 1/126 |
· · | Installations for disinfecting or deodorising waste-water plumbing installations

|  | E03C 1/14 |
· · | Wash-basins connected to the waste pipe

|  | E03C 1/16 |
· · | Wash-fountains connected to the waste-pipe

|  | E03C 1/18 |
· · | Sinks, whether or not connected to the waste-pipe

|  | E03C 1/181 |
· · · | Anti-splash devices in sinks (jet regulators Fulltext... Hierarchy... Expanded...E03C 1/08)

|  | E03C 1/182 |
· · · | connected to the waste-pipe

|  | E03C 1/184 |
· · · · | adapted for attachment of washing machines or heating or cooling devices (washing machines for attachment Fulltext... Hierarchy... Expanded...D06F 7/00)

|  | E03C 1/186 |
· · · | Separate partition walls, lids, protecting borders, or the like, for sinks

|  | E03C 1/20 |
· · | Connecting baths or bidets to the waste-pipe

|  | E03C 1/22 |
· · | Outlet devices mounted in basins, baths, or sinks (stoppers Fulltext... Hierarchy... Expanded...A47K 1/14)

|  | E03C 1/23 |
· · · | with mechanical closure mechanisms

|  | E03C 1/232 |
· · · · | combined with overflow devices (overflow devices for basins or baths per se Fulltext... Hierarchy... Expanded...E03C 1/24)

|  | E03C 1/24 |
· · | Overflow devices for basins or baths (Fulltext... Hierarchy... Expanded...E03C 1/232 takes precedence)

|  | E03C 1/242 |
· · · | automatically actuating supply or draining valves

|  | E03C 1/244 |
· · · | Separate devices to be placed on the outlet opening

|  | E03C 1/26 |
· · | Object-catching inserts or similar devices for outlets (Fulltext... Hierarchy... Expanded...E03C 1/28 takes precedence)

|  | E03C 1/262 |
· · · | combined with outlet stoppers

|  | E03C 1/264 |
· · · | Separate sieves or similar object-catching inserts

|  | E03C 1/266 |
· · · | Arrangements or adaptations of disintegrating apparatus in waste pipes, outlets to waste pipes, or the like (disintegrating apparatus per se Fulltext... Hierarchy... Expanded...B02C)

|  | E03C 1/28 |
· · | Odour seals

|  | E03C 1/282 |
· · · | combined with additional object-catching devices

|  | E03C 1/284 |
· · · | having U-shaped trap

|  | E03C 1/286 |
· · · · | having hand-operated valves against return of waste water

|  | E03C 1/288 |
· · · · | having non-return valves against return of waste water (Fulltext... Hierarchy... Expanded...E03C 1/286 takes precedence)

|  | E03C 1/29 |
· · · | having housing containing dividing wall, e.g. tubular

|  | E03C 1/292 |
· · · · | having elastic housing

|  | E03C 1/294 |
· · · | with provisions against loss of water lock

|  | E03C 1/295 |
· · · · | using air-supply valves

|  | E03C 1/296 |
· · · · | using water-supply valves

|  | E03C 1/298 |
· · · | consisting only of non-return valve

|  | E03C 1/30 |
· · | Devices to facilitate removing of obstructions in waste pipes or sinks

|  | E03C 1/302 |
· · · | using devices moved through the pipes

|  | E03C 1/304 |
· · · | using fluid under pressure

|  | E03C 1/306 |
· · · · | by means of a tube connected to the water mains

|  | E03C 1/308 |
· · · · | by means of a pumping device

|  | E03C 1/32 |
· · | Holders or supports for basins

|  | E03C 1/322 |
· · · | connected to the wall only

|  | E03C 1/324 |
· · · · | adjustable

|  | E03C 1/326 |
· · · | resting on the floor

|  | E03C 1/328 |
· · · · | adjustable

|  | E03C 1/33 |
· · · | Fastening sinks or basins in an apertured support