|  | E |
SECTION E — FIXED CONSTRUCTIONS

BUILDING

|  | E02 |
HYDRAULIC ENGINEERING; FOUNDATIONS; SOIL-SHIFTING

|  | E02C |
SHIP-LIFTING DEVICES OR MECHANISMS

|  | E02C 1/00 |
Locks; Shaft locks, i.e. locks of which one front side is formed by a solid wall with an opening in the lower part through which the ships pass (lock gates Fulltext... Hierarchy... Expanded...E02B 7/20)

|  | E02C 1/02 |
· | with auxiliary basins

|  | E02C 1/04 |
· | with floating troughs

|  | E02C 1/06 |
· | Devices for filling or emptying locks (in lock gates Fulltext... Hierarchy... Expanded...E02B 7/20)

|  | E02C 1/08 |
· | Arrangements for dissipating the energy of the water (carried by lock gates Fulltext... Hierarchy... Expanded...E02B 8/06)

|  | E02C 1/10 |
· | Equipment for use in connection with the navigation of ships in locks; Mooring equipment (in general Fulltext... Hierarchy... Expanded...E02B 3/22)

|  | E02C 3/00 |
Inclined-plane ship-lifting mechanisms

|  | E02C 5/00 |
Mechanisms for lifting ships vertically (salvaging sunken vessels Fulltext... Hierarchy... Expanded...B63C 7/00)

|  | E02C 5/02 |
· | with floating chambers